(kicad_pcb
	(version 20240108)
	(generator "pcbnew")
	(generator_version "8.0")
	(general
		(thickness 1.6)
		(legacy_teardrops no)
	)
	(paper "A4")
	(layers
		(0 "F.Cu" signal)
		(31 "B.Cu" signal)
		(32 "B.Adhes" user "B.Adhesive")
		(33 "F.Adhes" user "F.Adhesive")
		(34 "B.Paste" user)
		(35 "F.Paste" user)
		(36 "B.SilkS" user "B.Silkscreen")
		(37 "F.SilkS" user "F.Silkscreen")
		(38 "B.Mask" user)
		(39 "F.Mask" user)
		(40 "Dwgs.User" user "User.Drawings")
		(41 "Cmts.User" user "User.Comments")
		(42 "Eco1.User" user "User.Eco1")
		(43 "Eco2.User" user "User.Eco2")
		(44 "Edge.Cuts" user)
		(45 "Margin" user)
		(46 "B.CrtYd" user "B.Courtyard")
		(47 "F.CrtYd" user "F.Courtyard")
		(48 "B.Fab" user)
		(49 "F.Fab" user)
		(50 "User.1" user)
		(51 "User.2" user)
		(52 "User.3" user)
		(53 "User.4" user)
		(54 "User.5" user)
		(55 "User.6" user)
		(56 "User.7" user)
		(57 "User.8" user)
		(58 "User.9" user)
	)
	(setup
		(stackup
			(layer "F.SilkS"
				(type "Top Silk Screen")
			)
			(layer "F.Paste"
				(type "Top Solder Paste")
			)
			(layer "F.Mask"
				(type "Top Solder Mask")
				(thickness 0.01)
			)
			(layer "F.Cu"
				(type "copper")
				(thickness 0.035)
			)
			(layer "dielectric 1"
				(type "core")
				(thickness 1.51)
				(material "FR4")
				(epsilon_r 4.5)
				(loss_tangent 0.02)
			)
			(layer "B.Cu"
				(type "copper")
				(thickness 0.035)
			)
			(layer "B.Mask"
				(type "Bottom Solder Mask")
				(thickness 0.01)
			)
			(layer "B.Paste"
				(type "Bottom Solder Paste")
			)
			(layer "B.SilkS"
				(type "Bottom Silk Screen")
			)
			(copper_finish "None")
			(dielectric_constraints no)
		)
		(pad_to_mask_clearance 0)
		(allow_soldermask_bridges_in_footprints no)
		(pcbplotparams
			(layerselection 0x0001000_ffffffff)
			(plot_on_all_layers_selection 0x0000000_00000000)
			(disableapertmacros yes)
			(usegerberextensions yes)
			(usegerberattributes yes)
			(usegerberadvancedattributes yes)
			(creategerberjobfile yes)
			(dashed_line_dash_ratio 12.000000)
			(dashed_line_gap_ratio 3.000000)
			(svgprecision 4)
			(plotframeref no)
			(viasonmask no)
			(mode 1)
			(useauxorigin no)
			(hpglpennumber 1)
			(hpglpenspeed 20)
			(hpglpendiameter 15.000000)
			(pdf_front_fp_property_popups yes)
			(pdf_back_fp_property_popups yes)
			(dxfpolygonmode yes)
			(dxfimperialunits yes)
			(dxfusepcbnewfont yes)
			(psnegative no)
			(psa4output no)
			(plotreference no)
			(plotvalue no)
			(plotfptext no)
			(plotinvisibletext no)
			(sketchpadsonfab no)
			(subtractmaskfromsilk no)
			(outputformat 1)
			(mirror no)
			(drillshape 0)
			(scaleselection 1)
			(outputdirectory "gerber/")
		)
	)
	(net 0 "")
	(net 1 "5V")
	(net 2 "GND")
	(net 3 "SWIO")
	(net 4 "SCL")
	(net 5 "SDA")
	(net 6 "PWM2")
	(net 7 "/PC7")
	(net 8 "/PC5")
	(net 9 "RC_IN")
	(net 10 "PWM1")
	(net 11 "/PD7")
	(net 12 "/PD6")
	(net 13 "/PA1")
	(net 14 "/PD5")
	(net 15 "/PA2")
	(net 16 "/PD4")
	(net 17 "Net-(J20-Pin_5)")
	(footprint "Stripe-ch32:Servo_pads"
		(layer "F.Cu")
		(uuid "0fa2c90e-46eb-4d6f-8477-4fc2d336d207")
		(at 1.017034 42.60044 180)
		(descr "Through hole straight pin header, 1x03, 2.54mm pitch, single row")
		(tags "Through hole pin header THT 1x03 2.54mm single row")
		(property "Reference" "Srv10"
			(at 0 -2.33 0)
			(layer "F.SilkS")
			(hide yes)
			(uuid "7124dda4-ba15-484c-9321-6034d2b3ff26")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "~"
			(at 0 7.41 0)
			(layer "F.Fab")
			(uuid "60140176-9e46-48b7-ac31-195bc00fcd48")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Footprint" "Stripe-ch32:Servo_pads"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "4183c153-a3d9-4c6a-8a91-18af6b23f9f7")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "60207b7d-0f7b-454e-878b-24d24b5eac6e")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "6d5ddd43-82b2-4453-ba86-c0d349eb2edb")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(path "/118f3d0b-dcbb-4571-b440-5e71eb82f561")
		(sheetname "Root")
		(sheetfile "stripe_board.kicad_sch")
		(attr through_hole)
		(fp_line
			(start 1.33 6.41)
			(end 1.3208 -1.27)
			(stroke
				(width 0.1)
				(type default)
			)
			(layer "F.SilkS")
			(uuid "1d4d6f8c-13ed-4b21-9184-528b0a588de2")
		)
		(fp_line
			(start -1.3208 -1.27)
			(end 1.3208 -1.27)
			(stroke
				(width 0.1)
				(type default)
			)
			(layer "F.SilkS")
			(uuid "05d080a5-c0d9-46cf-9a3a-79e75212258f")
		)
		(fp_line
			(start -1.33 6.41)
			(end 1.33 6.41)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "ec5592ee-3cf1-4014-a143-d486009ef02b")
		)
		(fp_line
			(start -1.33 6.41)
			(end -1.3208 -1.27)
			(stroke
				(width 0.1)
				(type default)
			)
			(layer "F.SilkS")
			(uuid "55b37539-cb42-438f-8c10-f41b04b4b889")
		)
		(fp_line
			(start 1.8 6.85)
			(end 1.8 -1.8)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "0f0b201d-989b-424f-8d72-daf78fd7a048")
		)
		(fp_line
			(start 1.8 -1.8)
			(end -1.8 -1.8)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "c558cc45-47fa-463d-b03a-0bb401dec520")
		)
		(fp_line
			(start -1.8 6.85)
			(end 1.8 6.85)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "e99a3e53-8942-4087-a624-ad809aadd2a9")
		)
		(fp_line
			(start -1.8 -1.8)
			(end -1.8 6.85)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "e0551c9e-1a65-4d00-9a9b-bfdac140930f")
		)
		(fp_line
			(start 1.27 6.35)
			(end -1.27 6.35)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "80a1b799-cb44-49a2-84f3-6c35ed02a034")
		)
		(fp_line
			(start 1.27 -1.27)
			(end 1.27 6.35)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "7c6f8e46-c508-4ed0-b2a7-18b787d64044")
		)
		(fp_line
			(start -0.635 -1.27)
			(end 1.27 -1.27)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "bc6437eb-cef3-4c02-b506-233adf1e103e")
		)
		(fp_line
			(start -1.27 6.35)
			(end -1.27 -0.635)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "30da405a-72c9-4965-aac7-e64f8f46f9ef")
		)
		(fp_line
			(start -1.27 -0.635)
			(end -0.635 -1.27)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "bb455745-b0fa-46ed-9525-8434c8777493")
		)
		(fp_text user "GND"
			(at -1.3208 -1.27 180)
			(unlocked yes)
			(layer "F.SilkS")
			(uuid "724cb496-44f7-48c6-812e-f41db21c8d88")
			(effects
				(font
					(size 0.7 0.7)
					(thickness 0.1)
				)
				(justify left bottom)
			)
		)
		(fp_text user "5V"
			(at 1.3716 3.048 180)
			(unlocked yes)
			(layer "F.SilkS")
			(uuid "a148ec15-e7d0-4992-b156-cb7f26e8684d")
			(effects
				(font
					(size 0.7 0.7)
					(thickness 0.1)
				)
				(justify left bottom)
			)
		)
		(fp_text user "${REFERENCE}"
			(at 0 2.54 90)
			(layer "F.Fab")
			(uuid "6e00ce45-1cc9-498f-8168-f83b81c7cefc")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(pad "1" thru_hole rect
			(at 0 0 180)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers yes)
			(keep_end_layers yes)
			(zone_layer_connections)
			(net 2 "GND")
			(pinfunction "GND")
			(pintype "passive")
			(uuid "0b86565f-3cec-4174-b60e-61443bddf1d6")
		)
		(pad "2" thru_hole oval
			(at 0 2.54 180)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers yes)
			(keep_end_layers yes)
			(zone_layer_connections)
			(net 1 "5V")
			(pinfunction "5v")
			(pintype "passive")
			(uuid "6daaf3fb-3368-407e-a373-8d43e7f184bb")
		)
		(pad "3" thru_hole oval
			(at 0 5.08 180)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers yes)
			(keep_end_layers yes)
			(zone_layer_connections)
			(net 10 "PWM1")
			(pinfunction "PWM")
			(pintype "passive")
			(uuid "219a1cd3-a0db-490a-b236-9284f8b67059")
		)
		(model "${KICAD8_3DMODEL_DIR}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x03_P2.54mm_Vertical.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Connector_PinHeader_2.54mm:PinHeader_2x04_P2.54mm_Vertical"
		(layer "F.Cu")
		(uuid "110cb9be-9bf3-4545-9669-d04e15f93b45")
		(at 10.199015 7.92533 -90)
		(descr "Through hole straight pin header, 2x04, 2.54mm pitch, double rows")
		(tags "Through hole pin header THT 2x04 2.54mm double row")
		(property "Reference" "J20"
			(at 1.27 -2.33 90)
			(layer "F.SilkS")
			(uuid "9e3b8fe9-671e-4e0a-b43d-357382e1bbc3")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "Conn_02x04_Odd_Even"
			(at 1.27 9.95 90)
			(layer "F.Fab")
			(uuid "84a54534-4454-4cdb-b8b7-a6790896a296")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Footprint" "Connector_PinHeader_2.54mm:PinHeader_2x04_P2.54mm_Vertical"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "b148fd1c-bccb-42ec-8e59-656e25f77cf0")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "0943a174-8013-4786-afca-b0f1edb0c6de")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "Generic connector, double row, 02x04, odd/even pin numbering scheme (row 1 odd numbers, row 2 even numbers), script generated (kicad-library-utils/schlib/autogen/connector/)"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "0861c235-f1b7-486d-95d3-6ab6c71979bd")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "Connector*:*_2x??_*")
		(path "/4eddbb30-df47-448f-9189-404123a0a8c4")
		(sheetname "Root")
		(sheetfile "stripe_board.kicad_sch")
		(attr through_hole)
		(fp_line
			(start -1.33 8.95)
			(end 3.87 8.95)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "a921077b-41eb-4774-857e-78df4fa3f5f2")
		)
		(fp_line
			(start -1.33 1.27)
			(end -1.33 8.95)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "b66c6eea-804c-44e4-b457-21c64fa87e2a")
		)
		(fp_line
			(start -1.33 1.27)
			(end 1.27 1.27)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "c8185e85-1b5c-41b1-8f16-579992305703")
		)
		(fp_line
			(start 1.27 1.27)
			(end 1.27 -1.33)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "5811bbc6-ad9a-4ac2-9e7d-b94cee12ec0c")
		)
		(fp_line
			(start -1.33 0)
			(end -1.33 -1.33)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "c3876f33-7446-48c3-8358-f1cee23f10c0")
		)
		(fp_line
			(start -1.33 -1.33)
			(end 0 -1.33)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "aaf68a32-7122-4776-8de0-2cfa92074864")
		)
		(fp_line
			(start 1.27 -1.33)
			(end 3.87 -1.33)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "575b5ae3-d422-4522-9061-6c60ee5046a6")
		)
		(fp_line
			(start 3.87 -1.33)
			(end 3.87 8.95)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "8ed8853f-8e86-4b5e-9d0e-419f1c890882")
		)
		(fp_line
			(start -1.8 9.4)
			(end 4.35 9.4)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "b2bfc176-46ef-4b3f-b5de-730480ecbf34")
		)
		(fp_line
			(start 4.35 9.4)
			(end 4.35 -1.8)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "5f1614e3-a40d-4bea-89d8-ab87795205ba")
		)
		(fp_line
			(start -1.8 -1.8)
			(end -1.8 9.4)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "0aab6770-a7d4-448a-9455-79f0e9f82f4c")
		)
		(fp_line
			(start 4.35 -1.8)
			(end -1.8 -1.8)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "5b56e2d5-77c2-4977-a9db-7e22840ecad6")
		)
		(fp_line
			(start -1.27 8.89)
			(end -1.27 0)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "912629b2-b239-41ba-a24a-3c152b2c8cd7")
		)
		(fp_line
			(start 3.81 8.89)
			(end -1.27 8.89)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "b2192388-d9a3-4a37-ae9c-4312c85ac22d")
		)
		(fp_line
			(start -1.27 0)
			(end 0 -1.27)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "48370432-73da-4bec-bd30-d77b9e24d4a8")
		)
		(fp_line
			(start 0 -1.27)
			(end 3.81 -1.27)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "e5024b59-a58e-4605-80f6-e83446a90d6e")
		)
		(fp_line
			(start 3.81 -1.27)
			(end 3.81 8.89)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "a3ad4013-2e4f-4094-8237-c6b2ffe23348")
		)
		(fp_text user "${REFERENCE}"
			(at 1.27 3.81 360)
			(layer "F.Fab")
			(uuid "4c3e3fe3-ebfc-45ea-a514-202d304d03bc")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(pad "1" thru_hole rect
			(at 0 0 270)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers yes)
			(keep_end_layers yes)
			(zone_layer_connections)
			(net 10 "PWM1")
			(pinfunction "Pin_1")
			(pintype "passive")
			(uuid "2c39a476-20aa-465f-aabe-2ade6340df77")
		)
		(pad "2" thru_hole oval
			(at 2.54 0 270)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers yes)
			(keep_end_layers yes)
			(zone_layer_connections)
			(net 6 "PWM2")
			(pinfunction "Pin_2")
			(pintype "passive")
			(uuid "5458002f-77ea-490f-9bcf-7c6333d84344")
		)
		(pad "3" thru_hole oval
			(at 0 2.54 270)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers yes)
			(keep_end_layers yes)
			(zone_layer_connections)
			(net 1 "5V")
			(pinfunction "Pin_3")
			(pintype "passive")
			(uuid "64f1f005-1909-4224-9566-3d68e178657c")
		)
		(pad "4" thru_hole oval
			(at 2.54 2.54 270)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers yes)
			(keep_end_layers yes)
			(zone_layer_connections)
			(net 1 "5V")
			(pinfunction "Pin_4")
			(pintype "passive")
			(uuid "f27140de-5ef6-4343-a482-2a596e9165a7")
		)
		(pad "5" thru_hole oval
			(at 0 5.08 270)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers yes)
			(keep_end_layers yes)
			(zone_layer_connections)
			(net 17 "Net-(J20-Pin_5)")
			(pinfunction "Pin_5")
			(pintype "passive")
			(uuid "79173b7e-d93e-470d-aebf-e61d70b77443")
		)
		(pad "6" thru_hole oval
			(at 2.54 5.08 270)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers yes)
			(keep_end_layers yes)
			(zone_layer_connections)
			(net 17 "Net-(J20-Pin_5)")
			(pinfunction "Pin_6")
			(pintype "passive")
			(uuid "5af04a60-a98c-44b0-ae41-6473ca550d64")
		)
		(pad "7" thru_hole oval
			(at 0 7.62 270)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers yes)
			(keep_end_layers yes)
			(zone_layer_connections)
			(net 1 "5V")
			(pinfunction "Pin_7")
			(pintype "passive")
			(uuid "d8de7974-2075-4e26-b456-6603393473aa")
		)
		(pad "8" thru_hole oval
			(at 2.54 7.62 270)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers yes)
			(keep_end_layers yes)
			(zone_layer_connections)
			(net 2 "GND")
			(pinfunction "Pin_8")
			(pintype "passive")
			(uuid "fa974dc7-1418-47cc-9e3d-c57f82794ea6")
		)
		(model "${KICAD8_3DMODEL_DIR}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_2x04_P2.54mm_Vertical.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Package_SO:SOP-16_3.9x9.9mm_P1.27mm"
		(layer "F.Cu")
		(uuid "139e0f84-ec00-46b4-a285-6ec3ca936ac8")
		(at 27.804015 11.07533)
		(descr "SOP, 16 Pin (https://www.diodes.com/assets/Datasheets/PAM8403.pdf), generated with kicad-footprint-generator ipc_gullwing_generator.py")
		(tags "SOP SO")
		(property "Reference" "U1"
			(at 0 -5.9 0)
			(layer "F.SilkS")
			(uuid "7885cc02-f3fc-4f18-b571-16ee525dde61")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "CH32V003AxMx"
			(at 0 5.9 0)
			(layer "F.Fab")
			(uuid "4e12c4ab-74eb-414e-9b27-ed7db43749b8")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Footprint" "Package_SO:SOP-16_3.9x9.9mm_P1.27mm"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "3a4d269b-626e-49e8-befd-d6c5d83313b2")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" "https://www.wch-ic.com/products/CH32V003.html"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "5e2526a9-c480-4875-889e-3d9d985bd3cd")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "CH32V003 series are industrial-grade general-purpose microcontrollers designed based on 32-bit RISC-V instruction set and architecture. It adopts QingKe V2A core, RV32EC instruction set, and supports 2 levels of interrupt nesting. The series are mounted with rich peripheral interfaces and function modules. Its internal organizational structure meets the low-cost and low-power embedded application scenarios."
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "fc1d2e14-6ccb-4408-8143-b324e3357709")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "SOP*3.9x9.9mm*P1.27mm*")
		(path "/01a8fdf8-05d2-4248-8af8-3ae7adc6396e")
		(sheetname "Root")
		(sheetfile "stripe_board.kicad_sch")
		(attr smd)
		(fp_line
			(start 0 -5.06)
			(end -1.95 -5.06)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "b6a439d4-469f-4f4e-a661-89acea1005bf")
		)
		(fp_line
			(start 0 -5.06)
			(end 1.95 -5.06)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "365a5426-6424-41f8-a1a9-8ae3747303e4")
		)
		(fp_line
			(start 0 5.06)
			(end -1.95 5.06)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "0ef4d057-5da1-4bda-af4e-791ce03902e6")
		)
		(fp_line
			(start 0 5.06)
			(end 1.95 5.06)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "308bb1ee-743d-426a-9cd1-c31fc7b4547a")
		)
		(fp_poly
			(pts
				(xy -2.725 -5.005) (xy -2.965 -5.335) (xy -2.485 -5.335) (xy -2.725 -5.005)
			)
			(stroke
				(width 0.12)
				(type solid)
			)
			(fill solid)
			(layer "F.SilkS")
			(uuid "e633cfba-628c-4ac2-860b-73a7a93d55d8")
		)
		(fp_line
			(start -3.75 -5.2)
			(end -3.75 5.2)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "bea0f519-738d-4fa5-ba37-ddde973f706c")
		)
		(fp_line
			(start -3.75 5.2)
			(end 3.75 5.2)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "6395c8c6-b040-44ce-bd6f-db4b51cf02a9")
		)
		(fp_line
			(start 3.75 -5.2)
			(end -3.75 -5.2)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "241004d6-64b2-4057-836d-9100da6a2c5b")
		)
		(fp_line
			(start 3.75 5.2)
			(end 3.75 -5.2)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "48d402f6-26b9-4a78-82c7-956799eb76a0")
		)
		(fp_line
			(start -1.95 -3.975)
			(end -0.975 -4.95)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "24e62f75-dd60-4922-854a-ea61eba77be8")
		)
		(fp_line
			(start -1.95 4.95)
			(end -1.95 -3.975)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "a7f8bb79-fcdb-41c6-b5cd-ba2c0f95cea2")
		)
		(fp_line
			(start -0.975 -4.95)
			(end 1.95 -4.95)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "6e2cef91-1467-445b-9167-d94ecaff3229")
		)
		(fp_line
			(start 1.95 -4.95)
			(end 1.95 4.95)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "f9ae12a4-e864-451b-ac21-8c32a7ad3a7b")
		)
		(fp_line
			(start 1.95 4.95)
			(end -1.95 4.95)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "871d9a05-94c4-4746-91c5-b23313b53cc6")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
			(uuid "bcd5a0f7-bdca-48c3-ae1a-120c30623347")
			(effects
				(font
					(size 0.98 0.98)
					(thickness 0.15)
				)
			)
		)
		(pad "1" smd roundrect
			(at -2.5 -4.445)
			(size 2 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 5 "SDA")
			(pinfunction "PC1")
			(pintype "bidirectional")
			(uuid "49834ca5-d8da-4c31-bc76-e55ec2cc12fc")
		)
		(pad "2" smd roundrect
			(at -2.5 -3.175)
			(size 2 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 4 "SCL")
			(pinfunction "PC2")
			(pintype "bidirectional")
			(uuid "392b9a37-cf5f-489a-91c5-cbb2748af997")
		)
		(pad "3" smd roundrect
			(at -2.5 -1.905)
			(size 2 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 10 "PWM1")
			(pinfunction "PC3")
			(pintype "bidirectional")
			(uuid "f838e997-2515-438e-965c-ddbd93d76604")
		)
		(pad "4" smd roundrect
			(at -2.5 -0.635)
			(size 2 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 6 "PWM2")
			(pinfunction "PC4")
			(pintype "bidirectional")
			(uuid "b3ade773-b90a-4141-8642-2aefe59283df")
		)
		(pad "5" smd roundrect
			(at -2.5 0.635)
			(size 2 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 8 "/PC5")
			(pinfunction "PC6")
			(pintype "bidirectional")
			(uuid "891f6513-bf07-45cc-91a9-38a72ec8b18c")
		)
		(pad "6" smd roundrect
			(at -2.5 1.905)
			(size 2 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 7 "/PC7")
			(pinfunction "PC7")
			(pintype "bidirectional")
			(uuid "1f3dfd57-cddd-4b07-853e-bc4525bcc113")
		)
		(pad "7" smd roundrect
			(at -2.5 3.175)
			(size 2 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 3 "SWIO")
			(pinfunction "PD1")
			(pintype "bidirectional")
			(uuid "8c7db55b-dcde-49fe-8634-30e910b7fa85")
		)
		(pad "8" smd roundrect
			(at -2.5 4.445)
			(size 2 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 16 "/PD4")
			(pinfunction "PD4")
			(pintype "bidirectional")
			(uuid "337a9c80-b780-419e-a316-59c604cf7da0")
		)
		(pad "9" smd roundrect
			(at 2.5 4.445)
			(size 2 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 14 "/PD5")
			(pinfunction "PD5")
			(pintype "bidirectional")
			(uuid "0a406ef0-2ced-435c-b681-817cd00f9ae4")
		)
		(pad "10" smd roundrect
			(at 2.5 3.175)
			(size 2 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 12 "/PD6")
			(pinfunction "PD6")
			(pintype "bidirectional")
			(uuid "ae7a77e9-05e0-488c-b126-c179a2cb97aa")
		)
		(pad "11" smd roundrect
			(at 2.5 1.905)
			(size 2 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 11 "/PD7")
			(pinfunction "PD7")
			(pintype "bidirectional")
			(uuid "d2614770-4d35-41b9-bf60-31a815582df4")
		)
		(pad "12" smd roundrect
			(at 2.5 0.635)
			(size 2 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 13 "/PA1")
			(pinfunction "PA1")
			(pintype "bidirectional")
			(uuid "a015f4b8-b659-4cd8-bbbf-52a7eacfb448")
		)
		(pad "13" smd roundrect
			(at 2.5 -0.635)
			(size 2 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 15 "/PA2")
			(pinfunction "PA2")
			(pintype "bidirectional")
			(uuid "a3845420-8f18-4f0e-a9c1-6ca388e7b603")
		)
		(pad "14" smd roundrect
			(at 2.5 -1.905)
			(size 2 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 2 "GND")
			(pinfunction "VSS")
			(pintype "power_in")
			(uuid "e1cc74ca-992e-43bb-aa1a-e1134ef6156f")
		)
		(pad "15" smd roundrect
			(at 2.5 -3.175)
			(size 2 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 1 "5V")
			(pinfunction "VDD")
			(pintype "power_in")
			(uuid "6f0a239f-90d3-44b7-b561-ecc34a9fa0b8")
		)
		(pad "16" smd roundrect
			(at 2.5 -4.445)
			(size 2 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 9 "RC_IN")
			(pinfunction "PC0")
			(pintype "bidirectional")
			(uuid "d41c8072-88b1-43ef-a6b1-e83458ce7818")
		)
		(model "${KICAD8_3DMODEL_DIR}/Package_SO.3dshapes/SOP-16_3.9x9.9mm_P1.27mm.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Stripe-ch32:stripe"
		(layer "F.Cu")
		(uuid "1fc05b22-4ed7-4937-8fb2-fe229ebba179")
		(at 32.209015 27.54033 90)
		(descr "Through hole straight socket strip, 1x06, 2.54mm pitch, single row (from Kicad 4.0.7), script generated")
		(tags "Through hole socket strip THT 1x06 2.54mm single row")
		(property "Reference" "J6"
			(at -9.12 0 0)
			(layer "F.SilkS")
			(uuid "feeac2e2-f4c6-4f37-ba94-3af93d318bed")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "Conn_01x01_Pin"
			(at 0 2.794 90)
			(layer "F.Fab")
			(uuid "979dba6b-eac9-4056-b8c2-118a83230ae6")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Footprint" "Stripe-ch32:stripe"
			(at -6.35 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "0ee247d7-3632-413a-9db1-4d4c7b1079b8")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" ""
			(at -6.35 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "c61f7a33-536a-484c-9262-d6344d2de7b5")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "Generic connector, single row, 01x01, script generated"
			(at -6.35 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "1d2242aa-ab1d-4065-83e0-d4191ac1509e")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "Connector*:*_1x??_*")
		(path "/693946dd-5b0b-4eb4-9173-0fa5180ea10e")
		(sheetname "Root")
		(sheetfile "stripe_board.kicad_sch")
		(attr through_hole)
		(net_tie_pad_groups "stripe-net")
		(fp_line
			(start -5.85 0)
			(end 5.85 0)
			(stroke
				(width 0.5)
				(type default)
			)
			(layer "F.Cu")
			(uuid "4f15c993-fdd8-4f49-915f-7b940d8b46c7")
		)
		(fp_line
			(start -7.62 -1.33)
			(end 7.68 -1.33)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "beb8d5f7-a2ee-448a-8a4f-aa70c2e121d0")
		)
		(fp_line
			(start 7.68 1.33)
			(end 7.68 -1.33)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "26b7b99d-db07-41ad-b2b1-14fd5d8742b4")
		)
		(fp_line
			(start -7.62 1.33)
			(end -7.62 -1.33)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "7cefb558-6822-40fb-8f35-7bc9132b9282")
		)
		(fp_line
			(start -7.62 1.33)
			(end 7.68 1.33)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "34a91caf-e75b-4dce-a677-54ad1b87cae3")
		)
		(fp_line
			(start 8.1 -1.75)
			(end 8.1 1.8)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "8d06c6c6-e1eb-438e-a6f1-ef01f04874a1")
		)
		(fp_line
			(start -8.15 -1.75)
			(end 8.1 -1.75)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "483b5b63-4c23-403a-a074-0b483b824a2d")
		)
		(fp_line
			(start 8.1 1.8)
			(end -8.15 1.8)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "68396a44-e0cb-4792-a9a6-fff1a39f8f58")
		)
		(fp_line
			(start -8.15 1.8)
			(end -8.15 -1.75)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "91677d81-609d-4277-ad47-3f95920cbb20")
		)
		(fp_line
			(start 7.62 -1.27)
			(end 7.62 1.27)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "80beda5d-8466-4c1e-85af-fb3f1dea2f8e")
		)
		(fp_line
			(start -6.985 -1.27)
			(end 7.62 -1.27)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "58482b65-7e4f-422d-8583-98699f5e241b")
		)
		(fp_line
			(start -7.62 -0.635)
			(end -6.985 -1.27)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "e1def95b-2cce-4f67-94a3-4726942142b2")
		)
		(fp_line
			(start 7.62 1.27)
			(end -7.62 1.27)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "f997a128-3e40-48b2-8db6-4ae8e0c29072")
		)
		(fp_line
			(start -7.62 1.27)
			(end -7.62 -0.635)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "826f7587-f7ae-4626-9908-52a5f69a22b6")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
			(uuid "b4e029fa-cf14-4c36-8df8-df714d22bdb4")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(pad "1" thru_hole circle
			(at -6.35 0 180)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers yes)
			(keep_end_layers yes)
			(zone_layer_connections)
			(net 11 "/PD7")
			(pinfunction "Pin_1")
			(pintype "passive")
			(uuid "6ea2af69-1502-4730-b531-a1d1625604a7")
		)
		(pad "1" thru_hole oval
			(at -3.81 0 180)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers yes)
			(keep_end_layers yes)
			(zone_layer_connections)
			(net 11 "/PD7")
			(pinfunction "Pin_1")
			(pintype "passive")
			(uuid "7330e6b5-ebe5-4445-9375-167ac6f1e8ca")
		)
		(pad "1" thru_hole oval
			(at -1.27 0 180)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers yes)
			(keep_end_layers yes)
			(zone_layer_connections)
			(net 11 "/PD7")
			(pinfunction "Pin_1")
			(pintype "passive")
			(uuid "7efb07ed-9d18-419e-9e5d-1375d4762127")
		)
		(pad "1" thru_hole oval
			(at 1.27 0 180)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers yes)
			(keep_end_layers yes)
			(zone_layer_connections)
			(net 11 "/PD7")
			(pinfunction "Pin_1")
			(pintype "passive")
			(uuid "fd7dc789-221c-46a0-a550-409a083a0af6")
		)
		(pad "1" thru_hole oval
			(at 3.81 0 180)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers yes)
			(keep_end_layers yes)
			(zone_layer_connections)
			(net 11 "/PD7")
			(pinfunction "Pin_1")
			(pintype "passive")
			(uuid "5e5c64ad-2ead-42ed-88be-e2d5128f4ec3")
		)
		(pad "1" thru_hole oval
			(at 6.35 0 180)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers yes)
			(keep_end_layers yes)
			(zone_layer_connections)
			(net 11 "/PD7")
			(pinfunction "Pin_1")
			(pintype "passive")
			(uuid "80c9e53b-8a0a-4bd7-aab0-f6b65552a7cf")
		)
		(model "${KICAD8_3DMODEL_DIR}/Connector_PinSocket_2.54mm.3dshapes/PinSocket_1x06_P2.54mm_Vertical.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Connector_JST:JST_XH_B4B-XH-A_1x04_P2.50mm_Vertical"
		(layer "F.Cu")
		(uuid "3859ccae-0e44-4cf4-b403-3ef74b76bea8")
		(at 8.399015 -1.04967)
		(descr "JST XH series connector, B4B-XH-A (http://www.jst-mfg.com/product/pdf/eng/eXH.pdf), generated with kicad-footprint-generator")
		(tags "connector JST XH vertical")
		(property "Reference" "J17"
			(at 3.75 -3.55 0)
			(layer "F.SilkS")
			(uuid "f046a691-ce89-4c62-9507-552eb9396ab6")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "Conn_01x04_Pin"
			(at 3.75 4.6 0)
			(layer "F.Fab")
			(uuid "da7e758a-8f6f-4a78-a047-0d0cb5db7d30")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Footprint" "Connector_JST:JST_XH_B4B-XH-A_1x04_P2.50mm_Vertical"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "95ddc06c-7ab1-494f-b8f3-b0d11d867c24")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "cf832826-a902-4b31-9bda-b60913be95f9")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "Generic connector, single row, 01x04, script generated"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "7c57008e-2345-4b51-9894-4791ac9a78ca")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "Connector*:*_1x??_*")
		(path "/501488e2-8892-417a-9245-21b024be178d")
		(sheetname "Root")
		(sheetfile "stripe_board.kicad_sch")
		(attr through_hole)
		(fp_line
			(start -2.85 -2.75)
			(end -2.85 -1.5)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "a91394c7-5e04-4612-9ab6-8a24fd2f9218")
		)
		(fp_line
			(start -2.56 -2.46)
			(end -2.56 3.51)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "15804726-89fc-4503-b003-d6f54b65d4bc")
		)
		(fp_line
			(start -2.56 3.51)
			(end 10.06 3.51)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "28d0e48a-b32c-474f-9d71-40581713c8f9")
		)
		(fp_line
			(start -2.55 -2.45)
			(end -2.55 -1.7)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "06dd7f07-4ee0-470a-a891-d147311e8dbd")
		)
		(fp_line
			(start -2.55 -1.7)
			(end -0.75 -1.7)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "25f32080-2234-4a93-87de-d6bd0a4b9a57")
		)
		(fp_line
			(start -2.55 -0.2)
			(end -1.8 -0.2)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "54a6bdf3-dc78-49f3-a95d-52c7413c1e7d")
		)
		(fp_line
			(start -1.8 -0.2)
			(end -1.8 2.75)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "c9dedb58-b2da-40de-a22f-2a99e6de0d12")
		)
		(fp_line
			(start -1.8 2.75)
			(end 3.75 2.75)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "101035f8-9f3c-41ed-8536-6b8941bdffda")
		)
		(fp_line
			(start -1.6 -2.75)
			(end -2.85 -2.75)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "687a3be1-340c-4e52-b86d-01d268867dff")
		)
		(fp_line
			(start -0.75 -2.45)
			(end -2.55 -2.45)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "fa4747a2-4f29-41e7-ab93-22f62d61dadf")
		)
		(fp_line
			(start -0.75 -1.7)
			(end -0.75 -2.45)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "242390dc-0763-469e-8609-b193c4409134")
		)
		(fp_line
			(start 0.75 -2.45)
			(end 0.75 -1.7)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "32668b36-f3ec-49a9-b919-c3c5944cb802")
		)
		(fp_line
			(start 0.75 -1.7)
			(end 6.75 -1.7)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "5aa293a4-7259-418f-ba0b-c61d23e298f4")
		)
		(fp_line
			(start 6.75 -2.45)
			(end 0.75 -2.45)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "45b7dabd-bb2d-46aa-9ec8-724f91354ad1")
		)
		(fp_line
			(start 6.75 -1.7)
			(end 6.75 -2.45)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "af0e2bb5-5dfc-4382-aefa-17ce49c2d693")
		)
		(fp_line
			(start 8.25 -2.45)
			(end 8.25 -1.7)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "70381c36-9999-4c58-b254-8ba97ec3e161")
		)
		(fp_line
			(start 8.25 -1.7)
			(end 10.05 -1.7)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "461f5793-d80f-47a0-9075-95ab2293ed71")
		)
		(fp_line
			(start 9.3 -0.2)
			(end 9.3 2.75)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "eeff4213-a846-4d7e-94a0-768a7323ae3f")
		)
		(fp_line
			(start 9.3 2.75)
			(end 3.75 2.75)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "db482b7b-5647-489f-affa-0ff13ffa8e94")
		)
		(fp_line
			(start 10.05 -2.45)
			(end 8.25 -2.45)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "612eebe3-4f06-4bd4-bc13-19b424d9dd92")
		)
		(fp_line
			(start 10.05 -1.7)
			(end 10.05 -2.45)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "715a5b31-602e-429e-b120-ad779c81b1dd")
		)
		(fp_line
			(start 10.05 -0.2)
			(end 9.3 -0.2)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "4c4e2137-34ff-4aa3-882e-f277d1f9562b")
		)
		(fp_line
			(start 10.06 -2.46)
			(end -2.56 -2.46)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "eb23b880-7e86-4c1b-9b99-7f031542e258")
		)
		(fp_line
			(start 10.06 3.51)
			(end 10.06 -2.46)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "f9deac46-ebc3-4603-8631-04f632ab59e1")
		)
		(fp_line
			(start -2.95 -2.85)
			(end -2.95 3.9)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "958a188f-75fd-48e1-b15a-9b4a56eb35b0")
		)
		(fp_line
			(start -2.95 3.9)
			(end 10.45 3.9)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "da739282-5281-4c55-b6db-6e1d4aea64b0")
		)
		(fp_line
			(start 10.45 -2.85)
			(end -2.95 -2.85)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "ddc0ef88-74d1-432c-b76a-89f164136ed0")
		)
		(fp_line
			(start 10.45 3.9)
			(end 10.45 -2.85)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "06dbbc83-3311-47d6-91f4-90abb373f60b")
		)
		(fp_line
			(start -2.45 -2.35)
			(end -2.45 3.4)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "c27c6731-4f00-4970-a868-985d26825939")
		)
		(fp_line
			(start -2.45 3.4)
			(end 9.95 3.4)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "4c0100b3-8dcc-4c23-96ad-b08308fbf95b")
		)
		(fp_line
			(start -0.625 -2.35)
			(end 0 -1.35)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "446d8477-803f-4a0a-8311-0dc72e0f2d58")
		)
		(fp_line
			(start 0 -1.35)
			(end 0.625 -2.35)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "da0c1a90-feb8-4db2-8a9f-47d552f8a073")
		)
		(fp_line
			(start 9.95 -2.35)
			(end -2.45 -2.35)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "b4e3ad9e-102a-4903-b4c8-aaacbf471b3a")
		)
		(fp_line
			(start 9.95 3.4)
			(end 9.95 -2.35)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "35b1a106-e9ec-428e-bdef-0c3b696a15c1")
		)
		(fp_text user "${REFERENCE}"
			(at 3.75 2.7 0)
			(layer "F.Fab")
			(uuid "cae4eb04-2f5b-41b8-a4ec-acc9fd4adcc6")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(pad "1" thru_hole roundrect
			(at 0 0)
			(size 1.7 1.95)
			(drill 0.95)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(roundrect_rratio 0.147059)
			(net 2 "GND")
			(pinfunction "Pin_1")
			(pintype "passive")
			(uuid "ea4fc6fa-ca1f-40f6-9aa1-6708ccc258af")
		)
		(pad "2" thru_hole oval
			(at 2.5 0)
			(size 1.7 1.95)
			(drill 0.95)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 4 "SCL")
			(pinfunction "Pin_2")
			(pintype "passive")
			(uuid "7733f1d9-6fe9-449f-8ec2-4a3e878703ca")
		)
		(pad "3" thru_hole oval
			(at 5 0)
			(size 1.7 1.95)
			(drill 0.95)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 5 "SDA")
			(pinfunction "Pin_3")
			(pintype "passive")
			(uuid "5bc8b393-6ebb-46fb-a504-6f7376f48040")
		)
		(pad "4" thru_hole oval
			(at 7.5 0)
			(size 1.7 1.95)
			(drill 0.95)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "5V")
			(pinfunction "Pin_4")
			(pintype "passive")
			(uuid "b6ac9011-716a-48d7-bd5f-e4c85477e21d")
		)
		(model "${KICAD8_3DMODEL_DIR}/Connector_JST.3dshapes/JST_XH_B4B-XH-A_1x04_P2.50mm_Vertical.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Stripe-ch32:Servo_pads"
		(layer "F.Cu")
		(uuid "3e38b468-ad46-4ad2-8e7f-58214fde18e7")
		(at 36.019015 42.78033 180)
		(descr "Through hole straight pin header, 1x03, 2.54mm pitch, single row")
		(tags "Through hole pin header THT 1x03 2.54mm single row")
		(property "Reference" "Srv7"
			(at 0 -2.33 0)
			(layer "F.SilkS")
			(hide yes)
			(uuid "2fbc0bae-6a99-46d1-8a36-d577b6e0d428")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "~"
			(at 0 7.41 0)
			(layer "F.Fab")
			(uuid "b59ae760-843f-4661-a5c3-b7be65d2c2aa")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Footprint" "Stripe-ch32:Servo_pads"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "ccc64842-4b0e-4982-a3f4-68246f181fd8")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "f8de513c-c518-40a0-91f5-646e1d2cd55b")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "0249ea2b-9b76-417a-aaf5-3bdd6fa3e227")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(path "/9335fceb-9808-4e22-8c2b-92f8aa2ed449")
		(sheetname "Root")
		(sheetfile "stripe_board.kicad_sch")
		(attr through_hole)
		(fp_line
			(start 1.33 6.41)
			(end 1.3208 -1.27)
			(stroke
				(width 0.1)
				(type default)
			)
			(layer "F.SilkS")
			(uuid "ee0b5353-4f53-4ebe-bbbb-dd05c58a64c4")
		)
		(fp_line
			(start -1.3208 -1.27)
			(end 1.3208 -1.27)
			(stroke
				(width 0.1)
				(type default)
			)
			(layer "F.SilkS")
			(uuid "cbc43e2b-bdfc-4011-84a1-fb17151dce4e")
		)
		(fp_line
			(start -1.33 6.41)
			(end 1.33 6.41)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "412ab8f2-1138-4676-a7e1-563c9c208fdd")
		)
		(fp_line
			(start -1.33 6.41)
			(end -1.3208 -1.27)
			(stroke
				(width 0.1)
				(type default)
			)
			(layer "F.SilkS")
			(uuid "9a5defb2-b865-483b-b5e2-a194c38bb84f")
		)
		(fp_line
			(start 1.8 6.85)
			(end 1.8 -1.8)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "106ba59e-fdd4-476c-9312-87dfdeeb90bb")
		)
		(fp_line
			(start 1.8 -1.8)
			(end -1.8 -1.8)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "a09b9018-1849-4fb5-b14a-f92144684ecb")
		)
		(fp_line
			(start -1.8 6.85)
			(end 1.8 6.85)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "a5f2f544-8704-4ffe-88b3-999fc762bbf5")
		)
		(fp_line
			(start -1.8 -1.8)
			(end -1.8 6.85)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "ae429945-2a67-41b3-84e2-2e7b70850b1b")
		)
		(fp_line
			(start 1.27 6.35)
			(end -1.27 6.35)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "9a410441-94fc-489a-9cc8-b0138cdaa695")
		)
		(fp_line
			(start 1.27 -1.27)
			(end 1.27 6.35)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "a412b28f-c33d-432c-a821-a6deedc84cd2")
		)
		(fp_line
			(start -0.635 -1.27)
			(end 1.27 -1.27)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "f1383055-448c-4b8d-9546-f9f358b3e421")
		)
		(fp_line
			(start -1.27 6.35)
			(end -1.27 -0.635)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "09502209-149e-4fea-92fb-6caab2b51a34")
		)
		(fp_line
			(start -1.27 -0.635)
			(end -0.635 -1.27)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "ca7b0604-a09b-49de-8809-fe6617fc28bc")
		)
		(fp_text user "5V"
			(at 1.3716 3.048 180)
			(unlocked yes)
			(layer "F.SilkS")
			(uuid "1fcaf5ee-cabc-48d9-b310-35d199a566ae")
			(effects
				(font
					(size 0.7 0.7)
					(thickness 0.1)
				)
				(justify left bottom)
			)
		)
		(fp_text user "GND"
			(at -1.3208 -1.27 180)
			(unlocked yes)
			(layer "F.SilkS")
			(uuid "c806b8c4-30cb-48f3-b00a-7973a5e82b42")
			(effects
				(font
					(size 0.7 0.7)
					(thickness 0.1)
				)
				(justify left bottom)
			)
		)
		(fp_text user "${REFERENCE}"
			(at 0 2.54 90)
			(layer "F.Fab")
			(uuid "38f1946c-1973-4ec7-96b0-1e6acde4ea20")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(pad "1" thru_hole rect
			(at 0 0 180)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers yes)
			(keep_end_layers yes)
			(zone_layer_connections)
			(net 2 "GND")
			(pinfunction "GND")
			(pintype "passive")
			(uuid "d6e3122e-92df-49eb-b1e0-e3c98099408b")
		)
		(pad "2" thru_hole oval
			(at 0 2.54 180)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers yes)
			(keep_end_layers yes)
			(zone_layer_connections)
			(net 1 "5V")
			(pinfunction "5v")
			(pintype "passive")
			(uuid "d5ac2302-184d-42a2-b2d2-f634c134721f")
		)
		(pad "3" thru_hole oval
			(at 0 5.08 180)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers yes)
			(keep_end_layers yes)
			(zone_layer_connections)
			(net 13 "/PA1")
			(pinfunction "PWM")
			(pintype "passive")
			(uuid "a8ec4498-3b99-4990-9f61-8b8ba5c4c7b1")
		)
		(model "${KICAD8_3DMODEL_DIR}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x03_P2.54mm_Vertical.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Stripe-ch32:Servo_pads"
		(layer "F.Cu")
		(uuid "4adba61e-ecd5-4d7e-a4f7-d711af8a4977")
		(at 5.329015 42.80033 180)
		(descr "Through hole straight pin header, 1x03, 2.54mm pitch, single row")
		(tags "Through hole pin header THT 1x03 2.54mm single row")
		(property "Reference" "Srv9"
			(at 0 -2.33 0)
			(layer "F.SilkS")
			(hide yes)
			(uuid "57633c30-f765-419a-98f4-aa9c46645c91")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "~"
			(at 0 7.41 0)
			(layer "F.Fab")
			(uuid "cc1229b7-d567-4c2e-85c9-73b99871ff6b")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Footprint" "Stripe-ch32:Servo_pads"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "e0f296db-9004-4c54-8069-2d147e14fbee")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "ced85a21-c026-4d47-9e3b-39d326873e40")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "cc2467a4-0363-47ad-bee4-84c2c396f15f")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(path "/4b5b2b0d-0ef8-445e-abe0-9f63a123096c")
		(sheetname "Root")
		(sheetfile "stripe_board.kicad_sch")
		(attr through_hole)
		(fp_line
			(start 1.33 6.41)
			(end 1.3208 -1.27)
			(stroke
				(width 0.1)
				(type default)
			)
			(layer "F.SilkS")
			(uuid "a8aefecf-b655-4d90-9480-8d98ea92835d")
		)
		(fp_line
			(start -1.3208 -1.27)
			(end 1.3208 -1.27)
			(stroke
				(width 0.1)
				(type default)
			)
			(layer "F.SilkS")
			(uuid "8c9d1d2c-cbeb-4648-aacf-db3d8083425b")
		)
		(fp_line
			(start -1.33 6.41)
			(end 1.33 6.41)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "a5c99428-6f9e-4b9d-9741-8b16312d0344")
		)
		(fp_line
			(start -1.33 6.41)
			(end -1.3208 -1.27)
			(stroke
				(width 0.1)
				(type default)
			)
			(layer "F.SilkS")
			(uuid "f8d0dc6f-f896-4208-904a-dba0a6df0e8b")
		)
		(fp_line
			(start 1.8 6.85)
			(end 1.8 -1.8)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "9eb8ad04-6288-462a-8cf5-0ef9c26d3d36")
		)
		(fp_line
			(start 1.8 -1.8)
			(end -1.8 -1.8)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "b0373dcb-382e-42c1-82de-c1503bfd7f03")
		)
		(fp_line
			(start -1.8 6.85)
			(end 1.8 6.85)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "f7a00aab-15e1-4467-9e64-005e7cca9164")
		)
		(fp_line
			(start -1.8 -1.8)
			(end -1.8 6.85)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "a62c8f89-f35e-4dcd-880f-a3c07f97476a")
		)
		(fp_line
			(start 1.27 6.35)
			(end -1.27 6.35)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "9509f6b6-e11a-4abb-9210-17d1d1b7fda4")
		)
		(fp_line
			(start 1.27 -1.27)
			(end 1.27 6.35)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "4c7d2329-b3c8-4362-80a8-6a801f9f94b2")
		)
		(fp_line
			(start -0.635 -1.27)
			(end 1.27 -1.27)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "c28e3efa-f58e-4e16-b145-00996d9f8ac8")
		)
		(fp_line
			(start -1.27 6.35)
			(end -1.27 -0.635)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "7a7ad0b7-dbb3-4168-a583-52410faf4137")
		)
		(fp_line
			(start -1.27 -0.635)
			(end -0.635 -1.27)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "d864175a-346e-441c-8dec-563f3d48f751")
		)
		(fp_text user "5V"
			(at 1.3716 3.048 180)
			(unlocked yes)
			(layer "F.SilkS")
			(uuid "b33c3620-aad4-449c-ba29-6fc847b733e3")
			(effects
				(font
					(size 0.7 0.7)
					(thickness 0.1)
				)
				(justify left bottom)
			)
		)
		(fp_text user "GND"
			(at -1.3208 -1.27 180)
			(unlocked yes)
			(layer "F.SilkS")
			(uuid "c26bde3a-fafe-4dd0-b2c4-d3d09cfc09c0")
			(effects
				(font
					(size 0.7 0.7)
					(thickness 0.1)
				)
				(justify left bottom)
			)
		)
		(fp_text user "${REFERENCE}"
			(at 0 2.54 90)
			(layer "F.Fab")
			(uuid "e4e697c5-7e3f-49d2-8184-3dc5e03dfdc8")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(pad "1" thru_hole rect
			(at 0 0 180)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers yes)
			(keep_end_layers yes)
			(zone_layer_connections)
			(net 2 "GND")
			(pinfunction "GND")
			(pintype "passive")
			(uuid "3bd4a8fd-dd27-4723-b7b3-2a3e4f2eee0d")
		)
		(pad "2" thru_hole oval
			(at 0 2.54 180)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers yes)
			(keep_end_layers yes)
			(zone_layer_connections)
			(net 1 "5V")
			(pinfunction "5v")
			(pintype "passive")
			(uuid "9dcbc65f-9ba5-4080-ad82-e4fcf3d88b49")
		)
		(pad "3" thru_hole oval
			(at 0 5.08 180)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers yes)
			(keep_end_layers yes)
			(zone_layer_connections)
			(net 6 "PWM2")
			(pinfunction "PWM")
			(pintype "passive")
			(uuid "ba7a0d73-d538-48ba-979c-7f2456e9660b")
		)
		(model "${KICAD8_3DMODEL_DIR}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x03_P2.54mm_Vertical.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Stripe-ch32:stripe"
		(layer "F.Cu")
		(uuid "5968e0d7-93a4-44ae-a1bd-e7bdb1989d25")
		(at 16.759015 27.56033 90)
		(descr "Through hole straight socket strip, 1x06, 2.54mm pitch, single row (from Kicad 4.0.7), script generated")
		(tags "Through hole socket strip THT 1x06 2.54mm single row")
		(property "Reference" "J3"
			(at -9.12 0 0)
			(layer "F.SilkS")
			(uuid "c2249125-39f5-43cb-892b-4801396db381")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "Conn_01x01_Pin"
			(at 0 2.794 90)
			(layer "F.Fab")
			(uuid "8ca90d93-ce87-48ac-9f2e-ff0a84f2e193")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Footprint" "Stripe-ch32:stripe"
			(at -6.35 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "1c2446dc-3b0e-4262-beca-df22f68a578e")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" ""
			(at -6.35 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "12d14033-cb70-4679-a2e5-264b1193b5f7")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "Generic connector, single row, 01x01, script generated"
			(at -6.35 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "c399dbb7-bc31-41a4-a385-d5bdd9f828d2")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "Connector*:*_1x??_*")
		(path "/84422458-73ac-4523-a766-9d2e39686ac7")
		(sheetname "Root")
		(sheetfile "stripe_board.kicad_sch")
		(attr through_hole)
		(net_tie_pad_groups "stripe-net")
		(fp_line
			(start -5.85 0)
			(end 5.85 0)
			(stroke
				(width 0.5)
				(type default)
			)
			(layer "F.Cu")
			(uuid "ff182bfb-128e-4b81-a49f-a683b91b40c2")
		)
		(fp_line
			(start -7.62 -1.33)
			(end 7.68 -1.33)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "b30f26fc-b11f-47ed-9bb2-5315efb21328")
		)
		(fp_line
			(start 7.68 1.33)
			(end 7.68 -1.33)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "a7f38087-40d6-4331-a58e-5b2757aa43df")
		)
		(fp_line
			(start -7.62 1.33)
			(end -7.62 -1.33)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "ec6dc23a-f9b9-4394-ac7e-cf91c731b189")
		)
		(fp_line
			(start -7.62 1.33)
			(end 7.68 1.33)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "5491ee8f-fbcc-46e4-8e41-62be0f7f95f1")
		)
		(fp_line
			(start 8.1 -1.75)
			(end 8.1 1.8)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "6016c593-919d-453f-8018-d94b44d45097")
		)
		(fp_line
			(start -8.15 -1.75)
			(end 8.1 -1.75)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "f7a178fd-9a19-4629-b8cd-863736c4b2a4")
		)
		(fp_line
			(start 8.1 1.8)
			(end -8.15 1.8)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "ac54d106-c963-4226-922c-5b9e08313cdb")
		)
		(fp_line
			(start -8.15 1.8)
			(end -8.15 -1.75)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "9636d4d4-79d5-44bd-96f2-96df1d394008")
		)
		(fp_line
			(start 7.62 -1.27)
			(end 7.62 1.27)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "cbca1c1d-662a-4cca-9eba-48e0473d2cf8")
		)
		(fp_line
			(start -6.985 -1.27)
			(end 7.62 -1.27)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "7cb9bdd9-8dbb-4846-a983-91779ff6df44")
		)
		(fp_line
			(start -7.62 -0.635)
			(end -6.985 -1.27)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "c40bdfdb-5735-4966-a8fd-8fd922c3090f")
		)
		(fp_line
			(start 7.62 1.27)
			(end -7.62 1.27)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "7ad7d61d-aded-40f2-9667-6c77c031acd4")
		)
		(fp_line
			(start -7.62 1.27)
			(end -7.62 -0.635)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "ae26947f-b158-4d1f-8732-e0305cd3d33c")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
			(uuid "4405e36d-6fe4-4d0f-8fc1-52cbba0e5cf5")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(pad "1" thru_hole circle
			(at -6.35 0 180)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers yes)
			(keep_end_layers yes)
			(zone_layer_connections)
			(net 16 "/PD4")
			(pinfunction "Pin_1")
			(pintype "passive")
			(uuid "72d5a59c-cf04-45c5-8ad8-705ffe57674c")
		)
		(pad "1" thru_hole oval
			(at -3.81 0 180)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers yes)
			(keep_end_layers yes)
			(zone_layer_connections)
			(net 16 "/PD4")
			(pinfunction "Pin_1")
			(pintype "passive")
			(uuid "4a3e4f7a-8208-4033-9760-e3fe405af9a9")
		)
		(pad "1" thru_hole oval
			(at -1.27 0 180)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers yes)
			(keep_end_layers yes)
			(zone_layer_connections)
			(net 16 "/PD4")
			(pinfunction "Pin_1")
			(pintype "passive")
			(uuid "011bcf52-9111-4498-b765-feab776ec50f")
		)
		(pad "1" thru_hole oval
			(at 1.27 0 180)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers yes)
			(keep_end_layers yes)
			(zone_layer_connections)
			(net 16 "/PD4")
			(pinfunction "Pin_1")
			(pintype "passive")
			(uuid "09e32ef3-f3e3-47ef-80c3-411e86ce9845")
		)
		(pad "1" thru_hole oval
			(at 3.81 0 180)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers yes)
			(keep_end_layers yes)
			(zone_layer_connections)
			(net 16 "/PD4")
			(pinfunction "Pin_1")
			(pintype "passive")
			(uuid "42db0d3b-bad6-4f39-a060-b790fc3ec344")
		)
		(pad "1" thru_hole oval
			(at 6.35 0 180)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers yes)
			(keep_end_layers yes)
			(zone_layer_connections)
			(net 16 "/PD4")
			(pinfunction "Pin_1")
			(pintype "passive")
			(uuid "6f0955bb-bc68-479f-b5df-2d13efe97910")
		)
		(model "${KICAD8_3DMODEL_DIR}/Connector_PinSocket_2.54mm.3dshapes/PinSocket_1x06_P2.54mm_Vertical.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "MountingHole:MountingHole_3.2mm_M3"
		(layer "F.Cu")
		(uuid "7bdb2b98-3234-4199-824e-e706d040b8fb")
		(at 40 0)
		(descr "Mounting Hole 3.2mm, no annular, M3")
		(tags "mounting hole 3.2mm no annular m3")
		(property "Reference" "REF**"
			(at 0 -4.2 0)
			(layer "F.SilkS")
			(uuid "bf8bcadf-d530-4776-9521-c560231e2e83")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "MountingHole_3.2mm_M3"
			(at 0 4.2 0)
			(layer "F.Fab")
			(uuid "d41414f1-e908-4836-9061-14e3ff6f4371")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Footprint" "MountingHole:MountingHole_3.2mm_M3"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "ebe68f78-2d6e-452a-b23d-54844273dd89")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "fae0d058-d208-41c3-9e34-d0cd8dd14f05")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "9c754a98-7f19-4694-b517-dd4394d37e73")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(attr exclude_from_pos_files exclude_from_bom)
		(fp_circle
			(center 0 0)
			(end 3.2 0)
			(stroke
				(width 0.15)
				(type solid)
			)
			(fill none)
			(layer "Cmts.User")
			(uuid "d75147e2-c8ef-4d71-9435-d5526b084f6c")
		)
		(fp_circle
			(center 0 0)
			(end 3.45 0)
			(stroke
				(width 0.05)
				(type solid)
			)
			(fill none)
			(layer "F.CrtYd")
			(uuid "7d208eeb-5314-466e-99cf-d615e321b1fd")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
			(uuid "709136ae-a76a-48ad-8ee7-9569491af5ac")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(pad "" np_thru_hole circle
			(at 0 0)
			(size 3.2 3.2)
			(drill 3.2)
			(layers "*.Cu" "*.Mask")
			(uuid "af0eafe7-be3f-4e2c-b360-3a45635871e8")
		)
	)
	(footprint "Stripe-ch32:stripe"
		(layer "F.Cu")
		(uuid "7ea60f4a-81b7-47a7-ae9f-e3986336433e")
		(at 36.019015 27.54033 90)
		(descr "Through hole straight socket strip, 1x06, 2.54mm pitch, single row (from Kicad 4.0.7), script generated")
		(tags "Through hole socket strip THT 1x06 2.54mm single row")
		(property "Reference" "J2"
			(at -9.12 0 0)
			(layer "F.SilkS")
			(uuid "e3842b2d-309b-40db-9947-5ee1d3565503")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "Conn_01x01_Pin"
			(at 0 2.794 90)
			(layer "F.Fab")
			(uuid "1ac781d1-537f-4233-9f83-3abb2185ea3f")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Footprint" "Stripe-ch32:stripe"
			(at -6.35 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "e1343449-6de8-4191-b46e-43fc7f3ce01b")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" ""
			(at -6.35 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "37164fe2-7e9d-473d-93fc-962670472c68")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "Generic connector, single row, 01x01, script generated"
			(at -6.35 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "a3826876-e88c-483e-af53-c57cb16ff580")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "Connector*:*_1x??_*")
		(path "/49329885-2322-4c2c-b8b7-df3f376acb44")
		(sheetname "Root")
		(sheetfile "stripe_board.kicad_sch")
		(attr through_hole)
		(net_tie_pad_groups "stripe-net")
		(fp_line
			(start -5.85 0)
			(end 5.85 0)
			(stroke
				(width 0.5)
				(type default)
			)
			(layer "F.Cu")
			(uuid "12f25b14-7de2-417b-9ba1-01dfcf872756")
		)
		(fp_line
			(start -7.62 -1.33)
			(end 7.68 -1.33)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "75d78a63-7e77-4a2a-8dd7-92835f2384b0")
		)
		(fp_line
			(start 7.68 1.33)
			(end 7.68 -1.33)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "447d46d5-b9c1-47cf-bdc3-e7b07c1c25dd")
		)
		(fp_line
			(start -7.62 1.33)
			(end -7.62 -1.33)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "0a5a8d5c-24f5-4103-8af2-3b50f91deae3")
		)
		(fp_line
			(start -7.62 1.33)
			(end 7.68 1.33)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "2300ac31-b7ea-4995-8630-8cc877181a98")
		)
		(fp_line
			(start 8.1 -1.75)
			(end 8.1 1.8)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "99568351-6607-4934-bd81-76fd0cfbb0cd")
		)
		(fp_line
			(start -8.15 -1.75)
			(end 8.1 -1.75)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "915cb61c-301f-4ec2-a491-ddb0ac69ced7")
		)
		(fp_line
			(start 8.1 1.8)
			(end -8.15 1.8)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "f08ccb48-ef39-4d73-b370-5a9a31f347e0")
		)
		(fp_line
			(start -8.15 1.8)
			(end -8.15 -1.75)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "cbbfefdf-f84a-4e65-aa98-6c269329cbf3")
		)
		(fp_line
			(start 7.62 -1.27)
			(end 7.62 1.27)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "d2692c3c-59fc-48a5-bb7d-b670a09512af")
		)
		(fp_line
			(start -6.985 -1.27)
			(end 7.62 -1.27)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "1601168c-6422-4a84-a79d-e7a1d68fc282")
		)
		(fp_line
			(start -7.62 -0.635)
			(end -6.985 -1.27)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "b11ea039-d483-4f55-8598-6a111ed407f1")
		)
		(fp_line
			(start 7.62 1.27)
			(end -7.62 1.27)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "98669285-28e7-42ee-b380-ed91368e23f0")
		)
		(fp_line
			(start -7.62 1.27)
			(end -7.62 -0.635)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "a7b6563e-520a-4aab-82f4-9cb98d810045")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
			(uuid "24ec251c-287e-4bb2-a229-033702ef257b")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(pad "1" thru_hole circle
			(at -6.35 0 180)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers yes)
			(keep_end_layers yes)
			(zone_layer_connections)
			(net 13 "/PA1")
			(pinfunction "Pin_1")
			(pintype "passive")
			(uuid "8dd073b0-851c-4490-9995-df5e4f3a60a0")
		)
		(pad "1" thru_hole oval
			(at -3.81 0 180)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers yes)
			(keep_end_layers yes)
			(zone_layer_connections)
			(net 13 "/PA1")
			(pinfunction "Pin_1")
			(pintype "passive")
			(uuid "fc2162ad-df5b-40a4-bfc7-b310caed4c3c")
		)
		(pad "1" thru_hole oval
			(at -1.27 0 180)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers yes)
			(keep_end_layers yes)
			(zone_layer_connections)
			(net 13 "/PA1")
			(pinfunction "Pin_1")
			(pintype "passive")
			(uuid "168ac18f-cc40-4dd8-85c2-54ebc8377059")
		)
		(pad "1" thru_hole oval
			(at 1.27 0 180)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers yes)
			(keep_end_layers yes)
			(zone_layer_connections)
			(net 13 "/PA1")
			(pinfunction "Pin_1")
			(pintype "passive")
			(uuid "2ade1b20-0973-460c-8fa5-376a07a9ff9c")
		)
		(pad "1" thru_hole oval
			(at 3.81 0 180)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers yes)
			(keep_end_layers yes)
			(zone_layer_connections)
			(net 13 "/PA1")
			(pinfunction "Pin_1")
			(pintype "passive")
			(uuid "7d4c13e1-c06e-4446-acd2-bb8972b0559a")
		)
		(pad "1" thru_hole oval
			(at 6.35 0 180)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers yes)
			(keep_end_layers yes)
			(zone_layer_connections)
			(net 13 "/PA1")
			(pinfunction "Pin_1")
			(pintype "passive")
			(uuid "2cd44912-12b5-413f-b505-95bcfdfc0f06")
		)
		(model "${KICAD8_3DMODEL_DIR}/Connector_PinSocket_2.54mm.3dshapes/PinSocket_1x06_P2.54mm_Vertical.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Stripe-ch32:stripe"
		(layer "F.Cu")
		(uuid "7f428ec5-eca3-4328-9b76-e3f3d91675de")
		(at 39.829015 27.54033 90)
		(descr "Through hole straight socket strip, 1x06, 2.54mm pitch, single row (from Kicad 4.0.7), script generated")
		(tags "Through hole socket strip THT 1x06 2.54mm single row")
		(property "Reference" "J8"
			(at -9.12 0 0)
			(layer "F.SilkS")
			(uuid "c4f7718e-c309-4c5f-acbe-b9c5e0e58345")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "Conn_01x01_Pin"
			(at 0 2.794 90)
			(layer "F.Fab")
			(uuid "c87bb7ea-754b-4232-9d43-09936b543e23")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Footprint" "Stripe-ch32:stripe"
			(at -6.35 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "4c2c0e35-1193-4c38-8205-1aa3b788560b")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" ""
			(at -6.35 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "38017027-5e6d-438c-9321-dec95507936e")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "Generic connector, single row, 01x01, script generated"
			(at -6.35 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "d85386dd-537c-4ac4-b410-342f164350fa")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "Connector*:*_1x??_*")
		(path "/2c176999-e1e1-46ca-92be-59b16b284fb2")
		(sheetname "Root")
		(sheetfile "stripe_board.kicad_sch")
		(attr through_hole)
		(net_tie_pad_groups "stripe-net")
		(fp_line
			(start -5.85 0)
			(end 5.85 0)
			(stroke
				(width 0.5)
				(type default)
			)
			(layer "F.Cu")
			(uuid "4ff53775-7aac-4ecf-806b-9e11b6deb7c1")
		)
		(fp_line
			(start -7.62 -1.33)
			(end 7.68 -1.33)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "85697274-3fa0-40a3-be36-bc329fa22cf9")
		)
		(fp_line
			(start 7.68 1.33)
			(end 7.68 -1.33)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "a6628fb3-df9a-4b5f-ba2d-75071c77e672")
		)
		(fp_line
			(start -7.62 1.33)
			(end -7.62 -1.33)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "13255a2b-b69e-4098-8e1a-c2540ca8adea")
		)
		(fp_line
			(start -7.62 1.33)
			(end 7.68 1.33)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "acb1afcd-02cd-41ca-b855-82942a266357")
		)
		(fp_line
			(start 8.1 -1.75)
			(end 8.1 1.8)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "51d47a56-7afc-4364-a8fc-f9569235b580")
		)
		(fp_line
			(start -8.15 -1.75)
			(end 8.1 -1.75)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "617a0236-a5ed-40ea-8f0c-937f5d7b2581")
		)
		(fp_line
			(start 8.1 1.8)
			(end -8.15 1.8)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "79afa015-2df8-48f4-b301-4cd021be3c6f")
		)
		(fp_line
			(start -8.15 1.8)
			(end -8.15 -1.75)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "d700a494-7737-44f6-92a2-865baab1ce70")
		)
		(fp_line
			(start 7.62 -1.27)
			(end 7.62 1.27)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "6fb4d05a-8acb-4c0f-81cf-39b10daa38c6")
		)
		(fp_line
			(start -6.985 -1.27)
			(end 7.62 -1.27)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "9f3302fe-ab1d-47eb-ac9e-ccb19dc56d8b")
		)
		(fp_line
			(start -7.62 -0.635)
			(end -6.985 -1.27)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "6288ef78-0ca0-4ca5-a1b0-b7753371b3b3")
		)
		(fp_line
			(start 7.62 1.27)
			(end -7.62 1.27)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "18763877-87db-4026-8f97-cce81fb664b9")
		)
		(fp_line
			(start -7.62 1.27)
			(end -7.62 -0.635)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "c45ba92d-6c23-4e69-8645-7a7cf506b860")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
			(uuid "c8c957e2-8d1c-4a3d-a5eb-1fb31adac2f8")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(pad "1" thru_hole circle
			(at -6.35 0 180)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers yes)
			(keep_end_layers yes)
			(zone_layer_connections)
			(net 15 "/PA2")
			(pinfunction "Pin_1")
			(pintype "passive")
			(uuid "eb727082-e186-4ecc-af90-e8a92d621680")
		)
		(pad "1" thru_hole oval
			(at -3.81 0 180)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers yes)
			(keep_end_layers yes)
			(zone_layer_connections)
			(net 15 "/PA2")
			(pinfunction "Pin_1")
			(pintype "passive")
			(uuid "31d8fb25-362f-43e1-8640-7b6f971b3047")
		)
		(pad "1" thru_hole oval
			(at -1.27 0 180)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers yes)
			(keep_end_layers yes)
			(zone_layer_connections)
			(net 15 "/PA2")
			(pinfunction "Pin_1")
			(pintype "passive")
			(uuid "7e096639-b16f-4e5c-ade0-af385517342a")
		)
		(pad "1" thru_hole oval
			(at 1.27 0 180)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers yes)
			(keep_end_layers yes)
			(zone_layer_connections)
			(net 15 "/PA2")
			(pinfunction "Pin_1")
			(pintype "passive")
			(uuid "e4f28d35-23b4-46fe-9cd5-b017f8af54ac")
		)
		(pad "1" thru_hole oval
			(at 3.81 0 180)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers yes)
			(keep_end_layers yes)
			(zone_layer_connections)
			(net 15 "/PA2")
			(pinfunction "Pin_1")
			(pintype "passive")
			(uuid "c1d743aa-cf75-42cd-ab68-3587c79a4466")
		)
		(pad "1" thru_hole oval
			(at 6.35 0 180)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers yes)
			(keep_end_layers yes)
			(zone_layer_connections)
			(net 15 "/PA2")
			(pinfunction "Pin_1")
			(pintype "passive")
			(uuid "218735b3-724c-40b6-87c2-79c1d8637550")
		)
		(model "${KICAD8_3DMODEL_DIR}/Connector_PinSocket_2.54mm.3dshapes/PinSocket_1x06_P2.54mm_Vertical.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Stripe-ch32:stripe"
		(layer "F.Cu")
		(uuid "8961659e-159b-492f-acaa-9f54416c1dec")
		(at 9.139015 27.56033 90)
		(descr "Through hole straight socket strip, 1x06, 2.54mm pitch, single row (from Kicad 4.0.7), script generated")
		(tags "Through hole socket strip THT 1x06 2.54mm single row")
		(property "Reference" "J10"
			(at -9.12 0 0)
			(layer "F.SilkS")
			(uuid "94379806-4e1b-4085-b89e-2fa8f2841484")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "Conn_01x01_Pin"
			(at 0 2.794 90)
			(layer "F.Fab")
			(uuid "ddd4efff-e05f-45c6-8c46-39bdacb71403")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Footprint" "Stripe-ch32:stripe"
			(at -6.35 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "d9ed81b4-9fa3-4642-9dda-4744763ee233")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" ""
			(at -6.35 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "2f367367-136a-4586-bd38-448be91860e0")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "Generic connector, single row, 01x01, script generated"
			(at -6.35 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "80070bdf-b04b-4074-94a6-fb76875545ff")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "Connector*:*_1x??_*")
		(path "/148af821-747d-4ea2-895a-f95ffb147224")
		(sheetname "Root")
		(sheetfile "stripe_board.kicad_sch")
		(attr through_hole)
		(net_tie_pad_groups "stripe-net")
		(fp_line
			(start -5.85 0)
			(end 5.85 0)
			(stroke
				(width 0.5)
				(type default)
			)
			(layer "F.Cu")
			(uuid "a02022da-8323-4f7b-8c48-3a9e5e489445")
		)
		(fp_line
			(start -7.62 -1.33)
			(end 7.68 -1.33)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "9e4a8474-13c3-4bc8-ae7f-ebee97874ba4")
		)
		(fp_line
			(start 7.68 1.33)
			(end 7.68 -1.33)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "f8958f5c-78be-41a3-b86d-b1eb63333f8a")
		)
		(fp_line
			(start -7.62 1.33)
			(end -7.62 -1.33)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "91d3e1b0-0e6d-4ab9-9990-3b8c6af1c98c")
		)
		(fp_line
			(start -7.62 1.33)
			(end 7.68 1.33)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "e7864106-3047-4958-b743-fb368d1d0a3c")
		)
		(fp_line
			(start 8.1 -1.75)
			(end 8.1 1.8)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "74b1e8b8-c1d5-4b2f-a807-0f236de70175")
		)
		(fp_line
			(start -8.15 -1.75)
			(end 8.1 -1.75)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "4cb31956-fa87-434a-acd6-dce1d84b243c")
		)
		(fp_line
			(start 8.1 1.8)
			(end -8.15 1.8)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "1726c956-7367-412a-b65f-660871da57a7")
		)
		(fp_line
			(start -8.15 1.8)
			(end -8.15 -1.75)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "12f4f916-72da-48e6-aac1-4fa790381f7c")
		)
		(fp_line
			(start 7.62 -1.27)
			(end 7.62 1.27)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "f2b5fa1f-3fac-4cac-abf2-4235321f31a6")
		)
		(fp_line
			(start -6.985 -1.27)
			(end 7.62 -1.27)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "759eef15-d445-478a-8c09-bffcfafdb457")
		)
		(fp_line
			(start -7.62 -0.635)
			(end -6.985 -1.27)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "8afa27f2-5da7-4ca3-91a7-980106c770e9")
		)
		(fp_line
			(start 7.62 1.27)
			(end -7.62 1.27)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "89ce58e8-1c6e-44cd-a8d0-e358b6b0e48f")
		)
		(fp_line
			(start -7.62 1.27)
			(end -7.62 -0.635)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "98719235-fc9d-4474-8c41-bfa58b07e40d")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
			(uuid "4f8fe50f-d65f-4dbf-9345-6b3c43a1a013")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(pad "1" thru_hole circle
			(at -6.35 0 180)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers yes)
			(keep_end_layers yes)
			(zone_layer_connections)
			(net 8 "/PC5")
			(pinfunction "Pin_1")
			(pintype "passive")
			(uuid "58d1b650-7d0a-49da-8337-61258fdae013")
		)
		(pad "1" thru_hole oval
			(at -3.81 0 180)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers yes)
			(keep_end_layers yes)
			(zone_layer_connections)
			(net 8 "/PC5")
			(pinfunction "Pin_1")
			(pintype "passive")
			(uuid "fc374f62-5b62-4ffd-85fe-16a01164361f")
		)
		(pad "1" thru_hole oval
			(at -1.27 0 180)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers yes)
			(keep_end_layers yes)
			(zone_layer_connections)
			(net 8 "/PC5")
			(pinfunction "Pin_1")
			(pintype "passive")
			(uuid "fcae5e46-bf3a-43a1-9471-11fc8f262041")
		)
		(pad "1" thru_hole oval
			(at 1.27 0 180)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers yes)
			(keep_end_layers yes)
			(zone_layer_connections)
			(net 8 "/PC5")
			(pinfunction "Pin_1")
			(pintype "passive")
			(uuid "b0a23b9d-5a6e-4c0d-944d-664c78452c13")
		)
		(pad "1" thru_hole oval
			(at 3.81 0 180)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers yes)
			(keep_end_layers yes)
			(zone_layer_connections)
			(net 8 "/PC5")
			(pinfunction "Pin_1")
			(pintype "passive")
			(uuid "0cc15e2b-7954-4016-b0f7-4406c6ed1c56")
		)
		(pad "1" thru_hole oval
			(at 6.35 0 180)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers yes)
			(keep_end_layers yes)
			(zone_layer_connections)
			(net 8 "/PC5")
			(pinfunction "Pin_1")
			(pintype "passive")
			(uuid "91c5c708-90bd-4e72-876e-576bcc18159d")
		)
		(model "${KICAD8_3DMODEL_DIR}/Connector_PinSocket_2.54mm.3dshapes/PinSocket_1x06_P2.54mm_Vertical.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Stripe-ch32:Servo_pads"
		(layer "F.Cu")
		(uuid "8d28bff8-363a-435e-a521-9a7511393fa0")
		(at 23.819015 1.20033 90)
		(descr "Through hole straight pin header, 1x03, 2.54mm pitch, single row")
		(tags "Through hole pin header THT 1x03 2.54mm single row")
		(property "Reference" "J16"
			(at 0 -2.33 90)
			(layer "F.SilkS")
			(hide yes)
			(uuid "b9ebbc5d-3758-494e-a6a5-502536f9b582")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "PROG"
			(at 0 7.41 90)
			(layer "F.Fab")
			(uuid "384ed856-0168-4ceb-b6d5-1fa2f95c8ee9")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Footprint" "Stripe-ch32:Servo_pads"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "9c571b02-2bd3-4286-83cd-75cf3134312a")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "fa22ccbe-31af-4871-8369-9a17b1eeec81")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "Generic connector, single row, 01x03, script generated"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "ca2355af-c2bc-4cd5-acf9-f7684bd6144a")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "Connector*:*_1x??_*")
		(path "/30ee1f63-4968-49ae-9ba6-990b0579d8d8")
		(sheetname "Root")
		(sheetfile "stripe_board.kicad_sch")
		(attr through_hole)
		(fp_line
			(start -1.3208 -1.27)
			(end 1.3208 -1.27)
			(stroke
				(width 0.1)
				(type default)
			)
			(layer "F.SilkS")
			(uuid "4de933c7-c57b-4c8b-b263-1d92e42aa35d")
		)
		(fp_line
			(start 1.33 6.41)
			(end 1.3208 -1.27)
			(stroke
				(width 0.1)
				(type default)
			)
			(layer "F.SilkS")
			(uuid "59a906a1-9ad2-4488-91bf-0334aacfd635")
		)
		(fp_line
			(start -1.33 6.41)
			(end -1.3208 -1.27)
			(stroke
				(width 0.1)
				(type default)
			)
			(layer "F.SilkS")
			(uuid "6f8780ce-8ed8-4221-813c-1e9b7da3eb26")
		)
		(fp_line
			(start -1.33 6.41)
			(end 1.33 6.41)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "ee8e0dfd-e272-411a-bb19-38af8935a98a")
		)
		(fp_line
			(start 1.8 -1.8)
			(end -1.8 -1.8)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "c34c5ee4-c5a4-4310-baca-35f86085a6ec")
		)
		(fp_line
			(start -1.8 -1.8)
			(end -1.8 6.85)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "22c10550-1b88-4a7b-bfb2-1783f051fcfb")
		)
		(fp_line
			(start 1.8 6.85)
			(end 1.8 -1.8)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "5d19d19c-2a84-4605-ba85-4ffc7a5d7393")
		)
		(fp_line
			(start -1.8 6.85)
			(end 1.8 6.85)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "76435192-b8cd-488f-ab0b-210767e36eaa")
		)
		(fp_line
			(start 1.27 -1.27)
			(end 1.27 6.35)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "a89efcf8-6374-44d5-8e61-321eada7239d")
		)
		(fp_line
			(start -0.635 -1.27)
			(end 1.27 -1.27)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "369c633c-e434-42af-8fd5-6c6a445ffb87")
		)
		(fp_line
			(start -1.27 -0.635)
			(end -0.635 -1.27)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "e14324d8-218e-43bc-8b7b-37983ee9a6a0")
		)
		(fp_line
			(start 1.27 6.35)
			(end -1.27 6.35)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "f0a052ce-61e8-4a22-b7cd-6071ca6f0887")
		)
		(fp_line
			(start -1.27 6.35)
			(end -1.27 -0.635)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "0127fa02-b99a-4afe-86da-cd7eeff27732")
		)
		(fp_text user "GND"
			(at -1.3208 -1.27 90)
			(unlocked yes)
			(layer "F.SilkS")
			(uuid "1fccebe4-17cd-4cb2-a11f-19b7dc684467")
			(effects
				(font
					(size 0.7 0.7)
					(thickness 0.1)
				)
				(justify left bottom)
			)
		)
		(fp_text user "5V"
			(at 1.3716 3.048 90)
			(unlocked yes)
			(layer "F.SilkS")
			(uuid "c69e60fa-6192-48d4-82f3-7efe26d480d7")
			(effects
				(font
					(size 0.7 0.7)
					(thickness 0.1)
				)
				(justify left bottom)
			)
		)
		(fp_text user "${REFERENCE}"
			(at 0 2.54 180)
			(layer "F.Fab")
			(uuid "ca390ef9-dc53-406e-a3c8-b3b8b87dbe5e")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(pad "1" thru_hole rect
			(at 0 0 90)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 3 "SWIO")
			(pinfunction "Pin_1")
			(pintype "passive")
			(uuid "df90b9bd-d10c-4aa1-9890-38c60cea81fb")
		)
		(pad "2" thru_hole oval
			(at 0 2.54 90)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "5V")
			(pinfunction "Pin_2")
			(pintype "passive")
			(uuid "f198eb4f-38aa-4114-87be-65cfd9e6163b")
		)
		(pad "3" thru_hole oval
			(at 0 5.08 90)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 2 "GND")
			(pinfunction "Pin_3")
			(pintype "passive")
			(uuid "dfb8273e-7b1b-4a9d-a2c3-ea2720e97412")
		)
		(model "${KICAD8_3DMODEL_DIR}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x03_P2.54mm_Vertical.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Stripe-ch32:stripe"
		(layer "F.Cu")
		(uuid "8f59e2c1-04a3-44a1-9300-caf918d88378")
		(at -2.600985 27.44033 90)
		(descr "Through hole straight socket strip, 1x06, 2.54mm pitch, single row (from Kicad 4.0.7), script generated")
		(tags "Through hole socket strip THT 1x06 2.54mm single row")
		(property "Reference" "J1"
			(at -9.12 0 360)
			(layer "F.SilkS")
			(uuid "23ab58d8-8992-498b-a451-9f2ef7960f83")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "Conn_01x01_Pin"
			(at 0 2.794 90)
			(layer "F.Fab")
			(uuid "584705ba-d1c1-4aa9-bc38-d1d67b124b54")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Footprint" "Stripe-ch32:stripe"
			(at -6.35 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "2bf13f33-726c-4113-8788-65eac40eff23")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" ""
			(at -6.35 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "91445245-1af7-4411-b353-c1e8696bf245")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "Generic connector, single row, 01x01, script generated"
			(at -6.35 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "5fbb06e5-e9be-4599-85e0-ba002c0ba61b")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "Connector*:*_1x??_*")
		(path "/09769d3b-bd64-4cff-b4ec-413d0e4b04fa")
		(sheetname "Root")
		(sheetfile "stripe_board.kicad_sch")
		(attr through_hole)
		(net_tie_pad_groups "stripe-net")
		(fp_line
			(start -5.85 0)
			(end 5.85 0)
			(stroke
				(width 0.5)
				(type default)
			)
			(layer "F.Cu")
			(uuid "219e3070-5b2f-4b76-a7c5-88e958e93ec2")
		)
		(fp_line
			(start -7.62 -1.33)
			(end 7.68 -1.33)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "561c0399-1095-4d97-b9c1-dd32312b314f")
		)
		(fp_line
			(start 7.68 1.33)
			(end 7.68 -1.33)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "71792429-9610-4f53-8b07-a6c412edd482")
		)
		(fp_line
			(start -7.62 1.33)
			(end -7.62 -1.33)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "056cd777-d08e-4836-8bc0-74ffb7925419")
		)
		(fp_line
			(start -7.62 1.33)
			(end 7.68 1.33)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "4c8e9319-0e49-4974-81e7-3c0a6da6c8d3")
		)
		(fp_line
			(start 8.1 -1.75)
			(end 8.1 1.8)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "83d8bd0d-22b3-40e9-88df-b6bb0f6829d2")
		)
		(fp_line
			(start -8.15 -1.75)
			(end 8.1 -1.75)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "cbb2c818-7999-4ec8-ac0c-81ae7721f486")
		)
		(fp_line
			(start 8.1 1.8)
			(end -8.15 1.8)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "801a2116-541e-4964-816f-82ccfbee86da")
		)
		(fp_line
			(start -8.15 1.8)
			(end -8.15 -1.75)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "d48e10a3-5bf9-411a-bdbe-e8d6d7b5c171")
		)
		(fp_line
			(start 7.62 -1.27)
			(end 7.62 1.27)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "29b8f5a9-624c-4054-9830-d9ac2f910082")
		)
		(fp_line
			(start -6.985 -1.27)
			(end 7.62 -1.27)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "cf1ce8a3-b82d-46d5-bf5c-08a82fc7dbe5")
		)
		(fp_line
			(start -7.62 -0.635)
			(end -6.985 -1.27)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "ac9032fd-992b-49b8-92cf-ba713aa04b9b")
		)
		(fp_line
			(start 7.62 1.27)
			(end -7.62 1.27)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "28449a35-6f52-4020-88ec-a913ddfc022a")
		)
		(fp_line
			(start -7.62 1.27)
			(end -7.62 -0.635)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "15a2c364-1017-4688-a0e9-2b72666b0dd8")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
			(uuid "72efff43-5e63-49d7-a4e2-246abbbf03d9")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(pad "1" thru_hole circle
			(at -6.35 0 180)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 2 "GND")
			(pinfunction "Pin_1")
			(pintype "passive")
			(uuid "96076d0a-6e14-4c43-85e1-20224b75c87c")
		)
		(pad "1" thru_hole oval
			(at -3.81 0 180)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 2 "GND")
			(pinfunction "Pin_1")
			(pintype "passive")
			(uuid "d477e8d7-2f6d-4cdf-bf03-458ffeeae837")
		)
		(pad "1" thru_hole oval
			(at -1.27 0 180)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 2 "GND")
			(pinfunction "Pin_1")
			(pintype "passive")
			(uuid "cb64085c-e86f-406c-a21d-7d2237442f9c")
		)
		(pad "1" thru_hole oval
			(at 1.27 0 180)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 2 "GND")
			(pinfunction "Pin_1")
			(pintype "passive")
			(uuid "675c8faa-dd73-4c36-a569-fb74e0b3d930")
		)
		(pad "1" thru_hole oval
			(at 3.81 0 180)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 2 "GND")
			(pinfunction "Pin_1")
			(pintype "passive")
			(uuid "255ae85f-8c46-4ce5-8d77-f3b0fa9ba657")
		)
		(pad "1" thru_hole oval
			(at 6.35 0 180)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 2 "GND")
			(pinfunction "Pin_1")
			(pintype "passive")
			(uuid "0265f69e-af30-41f6-866d-506641650259")
		)
		(model "${KICAD8_3DMODEL_DIR}/Connector_PinSocket_2.54mm.3dshapes/PinSocket_1x06_P2.54mm_Vertical.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Stripe-ch32:stripe"
		(layer "F.Cu")
		(uuid "975d3b9b-55cf-42b0-a4e2-f8707991610d")
		(at 12.949015 27.56033 90)
		(descr "Through hole straight socket strip, 1x06, 2.54mm pitch, single row (from Kicad 4.0.7), script generated")
		(tags "Through hole socket strip THT 1x06 2.54mm single row")
		(property "Reference" "J9"
			(at -9.12 0 0)
			(layer "F.SilkS")
			(uuid "e0814818-064d-461a-bbd0-bdd713032f83")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "Conn_01x01_Pin"
			(at 0 2.794 90)
			(layer "F.Fab")
			(uuid "9d0f4bc4-6a01-4c92-9bd4-1d62f8774837")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Footprint" "Stripe-ch32:stripe"
			(at -6.35 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "bf95dada-6ec2-4fec-afb5-f5c71f49f20e")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" ""
			(at -6.35 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "cf79f51d-91f8-4e5a-9a36-44a8abe6435f")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "Generic connector, single row, 01x01, script generated"
			(at -6.35 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "7a397176-0d23-48bb-a94a-e8fd972b94b3")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "Connector*:*_1x??_*")
		(path "/d57dfca4-f1a9-45ae-9660-e8b423601df2")
		(sheetname "Root")
		(sheetfile "stripe_board.kicad_sch")
		(attr through_hole)
		(net_tie_pad_groups "stripe-net")
		(fp_line
			(start -5.85 0)
			(end 5.85 0)
			(stroke
				(width 0.5)
				(type default)
			)
			(layer "F.Cu")
			(uuid "e5dcba7b-dd80-4c31-9fe1-ad2a4d974647")
		)
		(fp_line
			(start -7.62 -1.33)
			(end 7.68 -1.33)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "d5a8bf25-ba06-4a45-be15-abb407068b01")
		)
		(fp_line
			(start 7.68 1.33)
			(end 7.68 -1.33)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "aede698f-4665-442c-a638-78e971872cb2")
		)
		(fp_line
			(start -7.62 1.33)
			(end -7.62 -1.33)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "b3dad363-2737-49ec-9435-12e553fc5edb")
		)
		(fp_line
			(start -7.62 1.33)
			(end 7.68 1.33)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "a30e42aa-1ec1-4998-b882-54b9ffdeaeb5")
		)
		(fp_line
			(start 8.1 -1.75)
			(end 8.1 1.8)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "8697aa67-a9ce-41e8-ab97-f4c87b5d5711")
		)
		(fp_line
			(start -8.15 -1.75)
			(end 8.1 -1.75)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "0433a305-e8fe-4c1d-84fd-2f68e17d29ba")
		)
		(fp_line
			(start 8.1 1.8)
			(end -8.15 1.8)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "ee0c82e3-c48d-4820-9170-92331a4e7bfa")
		)
		(fp_line
			(start -8.15 1.8)
			(end -8.15 -1.75)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "cc7c73a8-5624-4287-8d53-8ef741bcc6ff")
		)
		(fp_line
			(start 7.62 -1.27)
			(end 7.62 1.27)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "5298cb72-38e8-4549-b25a-ac3b55ac3821")
		)
		(fp_line
			(start -6.985 -1.27)
			(end 7.62 -1.27)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "f739af00-4a8d-47cf-b389-510508b44f87")
		)
		(fp_line
			(start -7.62 -0.635)
			(end -6.985 -1.27)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "7a68e690-c51d-4959-88de-7355897734b7")
		)
		(fp_line
			(start 7.62 1.27)
			(end -7.62 1.27)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "1b3d2ba7-780b-4bfa-af59-62398c7a73a7")
		)
		(fp_line
			(start -7.62 1.27)
			(end -7.62 -0.635)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "eb48aa29-be13-42c0-bb06-fe1ec885d18a")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
			(uuid "7387c25e-af94-49dd-b174-09a09f2533e0")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(pad "1" thru_hole circle
			(at -6.35 0 180)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers yes)
			(keep_end_layers yes)
			(zone_layer_connections)
			(net 7 "/PC7")
			(pinfunction "Pin_1")
			(pintype "passive")
			(uuid "709466c5-f0ac-42ec-9a09-5178ce2f87cd")
		)
		(pad "1" thru_hole oval
			(at -3.81 0 180)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers yes)
			(keep_end_layers yes)
			(zone_layer_connections)
			(net 7 "/PC7")
			(pinfunction "Pin_1")
			(pintype "passive")
			(uuid "e659d4a0-38b4-4ec5-be97-290e7fe85c46")
		)
		(pad "1" thru_hole oval
			(at -1.27 0 180)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers yes)
			(keep_end_layers yes)
			(zone_layer_connections)
			(net 7 "/PC7")
			(pinfunction "Pin_1")
			(pintype "passive")
			(uuid "b3f22ef6-bad8-470e-87b4-0b92dac4296b")
		)
		(pad "1" thru_hole oval
			(at 1.27 0 180)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers yes)
			(keep_end_layers yes)
			(zone_layer_connections)
			(net 7 "/PC7")
			(pinfunction "Pin_1")
			(pintype "passive")
			(uuid "71751bd1-ed9e-49d6-bfe4-1b5a381a0bfd")
		)
		(pad "1" thru_hole oval
			(at 3.81 0 180)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers yes)
			(keep_end_layers yes)
			(zone_layer_connections)
			(net 7 "/PC7")
			(pinfunction "Pin_1")
			(pintype "passive")
			(uuid "438b2ea0-dadf-4e18-81ea-f43c0e29d1ea")
		)
		(pad "1" thru_hole oval
			(at 6.35 0 180)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers yes)
			(keep_end_layers yes)
			(zone_layer_connections)
			(net 7 "/PC7")
			(pinfunction "Pin_1")
			(pintype "passive")
			(uuid "c6d0b295-97d7-4092-95ec-89b305a6579e")
		)
		(model "${KICAD8_3DMODEL_DIR}/Connector_PinSocket_2.54mm.3dshapes/PinSocket_1x06_P2.54mm_Vertical.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Stripe-ch32:Servo_pads"
		(layer "F.Cu")
		(uuid "99c7a693-6077-4c19-bf19-6de414b0314c")
		(at 32.209015 42.78033 180)
		(descr "Through hole straight pin header, 1x03, 2.54mm pitch, single row")
		(tags "Through hole pin header THT 1x03 2.54mm single row")
		(property "Reference" "Srv1"
			(at 0 -2.33 0)
			(layer "F.SilkS")
			(hide yes)
			(uuid "886a4a7e-5df4-4421-ad0e-d33b7a243a80")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "~"
			(at 0 7.41 0)
			(layer "F.Fab")
			(uuid "bc21c39b-ca74-4926-9e72-5bbecba86bb3")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Footprint" "Stripe-ch32:Servo_pads"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "ccf5858f-3ec9-4984-8e37-bde018a64b7c")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "e3842133-171b-4683-b8dc-6e17f3fb0a3a")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "2cc4c437-9540-4d7d-a736-77a1df864a9f")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(path "/3faba6f6-0d84-4506-93d6-f4ff72c8062a")
		(sheetname "Root")
		(sheetfile "stripe_board.kicad_sch")
		(attr through_hole)
		(fp_line
			(start 1.33 6.41)
			(end 1.3208 -1.27)
			(stroke
				(width 0.1)
				(type default)
			)
			(layer "F.SilkS")
			(uuid "74db846f-04b7-49fe-812b-d72e28f4201f")
		)
		(fp_line
			(start -1.3208 -1.27)
			(end 1.3208 -1.27)
			(stroke
				(width 0.1)
				(type default)
			)
			(layer "F.SilkS")
			(uuid "bc61306f-d3ca-408b-85b8-32f1506df2f5")
		)
		(fp_line
			(start -1.33 6.41)
			(end 1.33 6.41)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "b839cf1f-5ab1-4e81-bcb6-90fec4261beb")
		)
		(fp_line
			(start -1.33 6.41)
			(end -1.3208 -1.27)
			(stroke
				(width 0.1)
				(type default)
			)
			(layer "F.SilkS")
			(uuid "c40c2dbe-e60a-4da7-98f4-066ee4bb0332")
		)
		(fp_line
			(start 1.8 6.85)
			(end 1.8 -1.8)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "c6513914-04d1-4516-97ca-f2a3e40a3d76")
		)
		(fp_line
			(start 1.8 -1.8)
			(end -1.8 -1.8)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "f56f6c23-5e7a-4e9e-9ee1-ae4d70750e63")
		)
		(fp_line
			(start -1.8 6.85)
			(end 1.8 6.85)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "9d418ed1-2251-454f-ae29-0d8ebf964eaf")
		)
		(fp_line
			(start -1.8 -1.8)
			(end -1.8 6.85)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "cefe145f-7d3b-4989-be26-4605284f9213")
		)
		(fp_line
			(start 1.27 6.35)
			(end -1.27 6.35)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "2937af05-c08b-47a8-a669-e72aa3882c48")
		)
		(fp_line
			(start 1.27 -1.27)
			(end 1.27 6.35)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "1711f2b7-6b9b-4f2f-ae69-5f3a209c3125")
		)
		(fp_line
			(start -0.635 -1.27)
			(end 1.27 -1.27)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "8d146b46-f4eb-4924-803f-ac206cdd73b5")
		)
		(fp_line
			(start -1.27 6.35)
			(end -1.27 -0.635)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "947d9789-bff1-48b4-8635-fe17665af28b")
		)
		(fp_line
			(start -1.27 -0.635)
			(end -0.635 -1.27)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "74d4c348-69cd-4305-9f83-b3095ebf7a23")
		)
		(fp_text user "5V"
			(at 1.3716 3.048 180)
			(unlocked yes)
			(layer "F.SilkS")
			(uuid "111c250a-ae01-4fa7-8ec2-eaf6c0b27afe")
			(effects
				(font
					(size 0.7 0.7)
					(thickness 0.1)
				)
				(justify left bottom)
			)
		)
		(fp_text user "GND"
			(at -1.3208 -1.27 180)
			(unlocked yes)
			(layer "F.SilkS")
			(uuid "f0f33b1b-8e33-4b60-a214-5c10c4f4a7e8")
			(effects
				(font
					(size 0.7 0.7)
					(thickness 0.1)
				)
				(justify left bottom)
			)
		)
		(fp_text user "${REFERENCE}"
			(at 0 2.54 90)
			(layer "F.Fab")
			(uuid "f4a45f8e-ce51-4b3a-bb30-07ff1275652b")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(pad "1" thru_hole rect
			(at 0 0 180)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers yes)
			(keep_end_layers yes)
			(zone_layer_connections)
			(net 2 "GND")
			(pinfunction "GND")
			(pintype "passive")
			(uuid "5572a226-40da-4acc-958e-8316c1451511")
		)
		(pad "2" thru_hole oval
			(at 0 2.54 180)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers yes)
			(keep_end_layers yes)
			(zone_layer_connections)
			(net 1 "5V")
			(pinfunction "5v")
			(pintype "passive")
			(uuid "a8366b47-e7eb-4cf5-a324-6a1144955ffa")
		)
		(pad "3" thru_hole oval
			(at 0 5.08 180)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers yes)
			(keep_end_layers yes)
			(zone_layer_connections)
			(net 11 "/PD7")
			(pinfunction "PWM")
			(pintype "passive")
			(uuid "c18de194-bf6f-4e35-84ce-a34af7c8b36a")
		)
		(model "${KICAD8_3DMODEL_DIR}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x03_P2.54mm_Vertical.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "MountingHole:MountingHole_3.2mm_M3"
		(layer "F.Cu")
		(uuid "9a8307b8-1928-4b58-b21d-52e244dd75a4")
		(at 0 0)
		(descr "Mounting Hole 3.2mm, no annular, M3")
		(tags "mounting hole 3.2mm no annular m3")
		(property "Reference" "REF**"
			(at 0 -4.2 0)
			(layer "F.SilkS")
			(uuid "2e7f4579-5d8b-439a-9b0b-1fe98f500d6b")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "MountingHole_3.2mm_M3"
			(at 0 4.2 0)
			(layer "F.Fab")
			(uuid "6a71ebe2-7d71-4770-8b32-9721544049a1")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Footprint" "MountingHole:MountingHole_3.2mm_M3"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "92e469d0-d7c4-47a6-8f00-785e203d74e7")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "ae2f551d-0f73-4e66-901c-bba3a733f1d4")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "3bd095ff-50bc-4ed6-a345-bed9c84ec8c0")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(attr exclude_from_pos_files exclude_from_bom)
		(fp_circle
			(center 0 0)
			(end 3.2 0)
			(stroke
				(width 0.15)
				(type solid)
			)
			(fill none)
			(layer "Cmts.User")
			(uuid "76537439-6f11-4746-887f-49bf580ac4c3")
		)
		(fp_circle
			(center 0 0)
			(end 3.45 0)
			(stroke
				(width 0.05)
				(type solid)
			)
			(fill none)
			(layer "F.CrtYd")
			(uuid "6c15490b-e1f5-49ff-b06f-e65f60bf281c")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
			(uuid "93681e7c-0033-4956-afb8-150b668596cc")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(pad "" np_thru_hole circle
			(at 0 0)
			(size 3.2 3.2)
			(drill 3.2)
			(layers "F&B.Cu" "*.Mask")
			(uuid "4c0eeb95-3737-4d79-becb-ceec04f71e1f")
		)
	)
	(footprint "Stripe-ch32:stripe"
		(layer "F.Cu")
		(uuid "9be699e6-8dfb-4df8-a18d-53ae051316d7")
		(at 24.329015 27.54033 90)
		(descr "Through hole straight socket strip, 1x06, 2.54mm pitch, single row (from Kicad 4.0.7), script generated")
		(tags "Through hole socket strip THT 1x06 2.54mm single row")
		(property "Reference" "J4"
			(at -9.12 0 0)
			(layer "F.SilkS")
			(uuid "585d551d-e711-4cf4-88ab-d116dfbac951")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "Conn_01x01_Pin"
			(at 0 2.794 90)
			(layer "F.Fab")
			(uuid "66d5f962-d5d1-4bf6-b59d-1d62b3cae9dc")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Footprint" "Stripe-ch32:stripe"
			(at -6.35 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "86a2eaae-400a-4e21-8fd0-736ee1bcf7b3")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" ""
			(at -6.35 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "b63cc06b-416b-42dd-9de8-76cf77899ba1")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "Generic connector, single row, 01x01, script generated"
			(at -6.35 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "51e98bd9-85e2-4ccf-b2f8-5e5b71b8d3b7")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "Connector*:*_1x??_*")
		(path "/d77be3ef-c716-4670-97eb-52e7c9c3b2a2")
		(sheetname "Root")
		(sheetfile "stripe_board.kicad_sch")
		(attr through_hole)
		(net_tie_pad_groups "stripe-net")
		(fp_line
			(start -5.85 0)
			(end 5.85 0)
			(stroke
				(width 0.5)
				(type default)
			)
			(layer "F.Cu")
			(uuid "3adc22e2-70f9-4f81-8274-65765421dc10")
		)
		(fp_line
			(start -7.62 -1.33)
			(end 7.68 -1.33)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "56565a84-dc5e-46a2-84c0-e7ab860cd4d3")
		)
		(fp_line
			(start 7.68 1.33)
			(end 7.68 -1.33)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "f4b7d2b5-cbf2-482a-97ab-02de47aaed41")
		)
		(fp_line
			(start -7.62 1.33)
			(end -7.62 -1.33)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "9f91ffaf-d9d6-453a-9efe-812443d17add")
		)
		(fp_line
			(start -7.62 1.33)
			(end 7.68 1.33)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "49c0b519-7465-4f17-ad7f-d7203f093408")
		)
		(fp_line
			(start 8.1 -1.75)
			(end 8.1 1.8)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "926b75af-70b7-4293-8f5a-e05b324afd48")
		)
		(fp_line
			(start -8.15 -1.75)
			(end 8.1 -1.75)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "5ebdc8e2-367b-4ada-baaa-a87df9d6cb75")
		)
		(fp_line
			(start 8.1 1.8)
			(end -8.15 1.8)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "ec3df767-8c45-4977-9793-3d5a08dd855f")
		)
		(fp_line
			(start -8.15 1.8)
			(end -8.15 -1.75)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "383e8126-7c4b-47e5-865c-ef4a5648ea3e")
		)
		(fp_line
			(start 7.62 -1.27)
			(end 7.62 1.27)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "a7ffb706-6345-4425-85a7-4649b14682e3")
		)
		(fp_line
			(start -6.985 -1.27)
			(end 7.62 -1.27)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "4c4a3a45-a5f2-41c9-b4bb-420c6816e88d")
		)
		(fp_line
			(start -7.62 -0.635)
			(end -6.985 -1.27)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "37a14c02-90b0-4afe-8aa3-a409da031033")
		)
		(fp_line
			(start 7.62 1.27)
			(end -7.62 1.27)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "758b3eb1-e406-42a6-bfa1-9f3612483419")
		)
		(fp_line
			(start -7.62 1.27)
			(end -7.62 -0.635)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "03580653-7be7-461a-9770-98124bdb682a")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
			(uuid "7425ebc9-b377-4a56-94da-b7c243cf2ea6")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(pad "1" thru_hole circle
			(at -6.35 0 180)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers yes)
			(keep_end_layers yes)
			(zone_layer_connections)
			(net 14 "/PD5")
			(pinfunction "Pin_1")
			(pintype "passive")
			(uuid "decbff48-cf85-4508-80e2-040fafe2b509")
		)
		(pad "1" thru_hole oval
			(at -3.81 0 180)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers yes)
			(keep_end_layers yes)
			(zone_layer_connections)
			(net 14 "/PD5")
			(pinfunction "Pin_1")
			(pintype "passive")
			(uuid "9f9c10b6-8723-4abf-bdfe-bf83952d7af9")
		)
		(pad "1" thru_hole oval
			(at -1.27 0 180)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers yes)
			(keep_end_layers yes)
			(zone_layer_connections)
			(net 14 "/PD5")
			(pinfunction "Pin_1")
			(pintype "passive")
			(uuid "15eb7680-5bf3-441b-bb39-ad436818e69b")
		)
		(pad "1" thru_hole oval
			(at 1.27 0 180)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers yes)
			(keep_end_layers yes)
			(zone_layer_connections)
			(net 14 "/PD5")
			(pinfunction "Pin_1")
			(pintype "passive")
			(uuid "063a6665-a611-4c55-975d-34f0da8b870f")
		)
		(pad "1" thru_hole oval
			(at 3.81 0 180)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers yes)
			(keep_end_layers yes)
			(zone_layer_connections)
			(net 14 "/PD5")
			(pinfunction "Pin_1")
			(pintype "passive")
			(uuid "4cf0fc26-d128-4c6b-9c6a-b647bb85b5c6")
		)
		(pad "1" thru_hole oval
			(at 6.35 0 180)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers yes)
			(keep_end_layers yes)
			(zone_layer_connections)
			(net 14 "/PD5")
			(pinfunction "Pin_1")
			(pintype "passive")
			(uuid "f735faee-f484-4aa6-9218-0fb19f77a0de")
		)
		(model "${KICAD8_3DMODEL_DIR}/Connector_PinSocket_2.54mm.3dshapes/PinSocket_1x06_P2.54mm_Vertical.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Stripe-ch32:Servo_pads"
		(layer "F.Cu")
		(uuid "ab28b729-813f-4016-a82a-baf04d5500df")
		(at 9.139015 42.80033 180)
		(descr "Through hole straight pin header, 1x03, 2.54mm pitch, single row")
		(tags "Through hole pin header THT 1x03 2.54mm single row")
		(property "Reference" "Srv6"
			(at 0 -2.33 0)
			(layer "F.SilkS")
			(hide yes)
			(uuid "27e384aa-9f7c-4e69-aa61-6d911618fab6")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "~"
			(at 0 7.41 0)
			(layer "F.Fab")
			(uuid "9bb757d0-5048-40bd-a212-80eff8c29dbf")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Footprint" "Stripe-ch32:Servo_pads"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "d75817f4-ef09-45f8-8677-060eb3d5b7ff")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "ebc1d251-6f4a-48ee-8463-03568271084c")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "529c98ab-0458-4c57-b404-c1eabac8f812")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(path "/2ae1d2d9-7c97-40df-9aab-31a73649f890")
		(sheetname "Root")
		(sheetfile "stripe_board.kicad_sch")
		(attr through_hole)
		(fp_line
			(start 1.33 6.41)
			(end 1.3208 -1.27)
			(stroke
				(width 0.1)
				(type default)
			)
			(layer "F.SilkS")
			(uuid "d218de87-59d1-4891-8fbe-c626e6baf300")
		)
		(fp_line
			(start -1.3208 -1.27)
			(end 1.3208 -1.27)
			(stroke
				(width 0.1)
				(type default)
			)
			(layer "F.SilkS")
			(uuid "c377bff3-b204-42c4-988a-da5cf58a4ba5")
		)
		(fp_line
			(start -1.33 6.41)
			(end 1.33 6.41)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "850e8892-6db3-42e2-b657-1275ed1da829")
		)
		(fp_line
			(start -1.33 6.41)
			(end -1.3208 -1.27)
			(stroke
				(width 0.1)
				(type default)
			)
			(layer "F.SilkS")
			(uuid "f2d05e85-0a4d-429d-8147-5d2a6d44d7ae")
		)
		(fp_line
			(start 1.8 6.85)
			(end 1.8 -1.8)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "eb0d2dc1-ac87-4cb4-8439-464c7742def6")
		)
		(fp_line
			(start 1.8 -1.8)
			(end -1.8 -1.8)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "045fb02a-85fd-41b2-b7dc-2279446ac4e5")
		)
		(fp_line
			(start -1.8 6.85)
			(end 1.8 6.85)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "04355293-d929-4531-b944-9e6444fd3d9e")
		)
		(fp_line
			(start -1.8 -1.8)
			(end -1.8 6.85)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "b28c8bde-7edb-473c-8a2d-42151c679af8")
		)
		(fp_line
			(start 1.27 6.35)
			(end -1.27 6.35)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "d9bc3a2f-e490-4aca-b544-88f3e5db0fea")
		)
		(fp_line
			(start 1.27 -1.27)
			(end 1.27 6.35)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "f7063be0-5360-4cb6-93ef-7e4dc5be02c5")
		)
		(fp_line
			(start -0.635 -1.27)
			(end 1.27 -1.27)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "6a88bd2b-c4e2-4cf7-87ea-526865ceb7e4")
		)
		(fp_line
			(start -1.27 6.35)
			(end -1.27 -0.635)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "03d9b49a-4872-4720-bd9d-30405e513754")
		)
		(fp_line
			(start -1.27 -0.635)
			(end -0.635 -1.27)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "d1c4dd99-0d1d-429d-8509-fbf5f27def58")
		)
		(fp_text user "5V"
			(at 1.3716 3.048 180)
			(unlocked yes)
			(layer "F.SilkS")
			(uuid "067236ab-1585-44b7-a559-c378068329eb")
			(effects
				(font
					(size 0.7 0.7)
					(thickness 0.1)
				)
				(justify left bottom)
			)
		)
		(fp_text user "GND"
			(at -1.3208 -1.27 180)
			(unlocked yes)
			(layer "F.SilkS")
			(uuid "6cccfb94-0b44-47fc-b3bf-5bef8228ba07")
			(effects
				(font
					(size 0.7 0.7)
					(thickness 0.1)
				)
				(justify left bottom)
			)
		)
		(fp_text user "${REFERENCE}"
			(at 0 2.54 90)
			(layer "F.Fab")
			(uuid "1e61e3a3-6516-40db-8aa9-9a9c07f97280")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(pad "1" thru_hole rect
			(at 0 0 180)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers yes)
			(keep_end_layers yes)
			(zone_layer_connections)
			(net 2 "GND")
			(pinfunction "GND")
			(pintype "passive")
			(uuid "acd5f0cb-d787-4a6b-87bd-24bafc609f58")
		)
		(pad "2" thru_hole oval
			(at 0 2.54 180)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers yes)
			(keep_end_layers yes)
			(zone_layer_connections)
			(net 1 "5V")
			(pinfunction "5v")
			(pintype "passive")
			(uuid "5a92f619-906a-4732-9be3-21ec33552815")
		)
		(pad "3" thru_hole oval
			(at 0 5.08 180)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers yes)
			(keep_end_layers yes)
			(zone_layer_connections)
			(net 8 "/PC5")
			(pinfunction "PWM")
			(pintype "passive")
			(uuid "b134c4f3-4ccf-49f5-a69a-783eb7a2fc50")
		)
		(model "${KICAD8_3DMODEL_DIR}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x03_P2.54mm_Vertical.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Stripe-ch32:stripe"
		(layer "F.Cu")
		(uuid "b34b9fbf-caf4-4e84-aeea-01e63f6f889b")
		(at 28.399015 27.54033 90)
		(descr "Through hole straight socket strip, 1x06, 2.54mm pitch, single row (from Kicad 4.0.7), script generated")
		(tags "Through hole socket strip THT 1x06 2.54mm single row")
		(property "Reference" "J5"
			(at -9.12 0 0)
			(layer "F.SilkS")
			(uuid "034d1fc9-a305-4232-ae5a-e2ec8119e5f6")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "Conn_01x01_Pin"
			(at 0 2.794 90)
			(layer "F.Fab")
			(uuid "a7639670-3012-4d53-b386-72e0d50f7fe0")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Footprint" "Stripe-ch32:stripe"
			(at -6.35 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "627211c3-7429-480e-b95a-c56732cc157b")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" ""
			(at -6.35 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "d3077404-84fd-4cd7-a2eb-0f1e9d7fa4b7")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "Generic connector, single row, 01x01, script generated"
			(at -6.35 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "da3ec8fd-c925-41f0-a91c-b7642afe671d")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "Connector*:*_1x??_*")
		(path "/3e29a168-596c-404d-a007-028051b9e6e6")
		(sheetname "Root")
		(sheetfile "stripe_board.kicad_sch")
		(attr through_hole)
		(net_tie_pad_groups "stripe-net")
		(fp_line
			(start -5.85 0)
			(end 5.85 0)
			(stroke
				(width 0.5)
				(type default)
			)
			(layer "F.Cu")
			(uuid "e38ba06d-d404-4c19-8663-8781244faf0f")
		)
		(fp_line
			(start -7.62 -1.33)
			(end 7.68 -1.33)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "a45062a5-de10-4a8e-a13a-5b20ec852836")
		)
		(fp_line
			(start 7.68 1.33)
			(end 7.68 -1.33)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "2eadc856-6aa6-43cb-9224-8ff9891e1cfd")
		)
		(fp_line
			(start -7.62 1.33)
			(end -7.62 -1.33)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "d2a816c5-d7f0-45e5-b410-9ed749d60303")
		)
		(fp_line
			(start -7.62 1.33)
			(end 7.68 1.33)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "58b1a1fa-ddd4-468b-ac28-7b7b8b52158e")
		)
		(fp_line
			(start 8.1 -1.75)
			(end 8.1 1.8)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "40b9062a-140e-4af2-8029-20d32e651890")
		)
		(fp_line
			(start -8.15 -1.75)
			(end 8.1 -1.75)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "002aa4af-adf8-4042-b37d-0038f65d8cc6")
		)
		(fp_line
			(start 8.1 1.8)
			(end -8.15 1.8)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "77efcce9-7fef-42f8-bc64-72b3ee8df969")
		)
		(fp_line
			(start -8.15 1.8)
			(end -8.15 -1.75)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "492756d8-d4c6-4613-886c-8a3808b9a387")
		)
		(fp_line
			(start 7.62 -1.27)
			(end 7.62 1.27)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "003fd8a0-12cf-4861-9f40-6480d871a36d")
		)
		(fp_line
			(start -6.985 -1.27)
			(end 7.62 -1.27)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "4c0eb1c4-abe9-49b9-b8df-bdbfbbb55f50")
		)
		(fp_line
			(start -7.62 -0.635)
			(end -6.985 -1.27)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "9cb36905-c327-4ac5-97a2-cfd4d4ad2a6b")
		)
		(fp_line
			(start 7.62 1.27)
			(end -7.62 1.27)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "eb711575-81a8-425c-bc9a-46bbb4e58427")
		)
		(fp_line
			(start -7.62 1.27)
			(end -7.62 -0.635)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "c5e50231-e7da-44fb-8181-259678ee13ba")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
			(uuid "83fede3e-ff99-4607-83b4-d1b4703440d8")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(pad "1" thru_hole circle
			(at -6.35 0 180)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers yes)
			(keep_end_layers yes)
			(zone_layer_connections)
			(net 12 "/PD6")
			(pinfunction "Pin_1")
			(pintype "passive")
			(uuid "0cf56d6e-f087-4d12-b5db-c1b9c954e165")
		)
		(pad "1" thru_hole oval
			(at -3.81 0 180)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers yes)
			(keep_end_layers yes)
			(zone_layer_connections)
			(net 12 "/PD6")
			(pinfunction "Pin_1")
			(pintype "passive")
			(uuid "df254a52-91d6-4ca5-9ea3-9a57899bd4f2")
		)
		(pad "1" thru_hole oval
			(at -1.27 0 180)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers yes)
			(keep_end_layers yes)
			(zone_layer_connections)
			(net 12 "/PD6")
			(pinfunction "Pin_1")
			(pintype "passive")
			(uuid "f8ffbbaa-4f9f-4b7a-9bfd-5b4cae085f41")
		)
		(pad "1" thru_hole oval
			(at 1.27 0 180)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers yes)
			(keep_end_layers yes)
			(zone_layer_connections)
			(net 12 "/PD6")
			(pinfunction "Pin_1")
			(pintype "passive")
			(uuid "58f75245-0eae-4b02-8cc9-b62db831d7eb")
		)
		(pad "1" thru_hole oval
			(at 3.81 0 180)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers yes)
			(keep_end_layers yes)
			(zone_layer_connections)
			(net 12 "/PD6")
			(pinfunction "Pin_1")
			(pintype "passive")
			(uuid "f55bd0ec-75a8-4d73-9669-2ea30f643581")
		)
		(pad "1" thru_hole oval
			(at 6.35 0 180)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers yes)
			(keep_end_layers yes)
			(zone_layer_connections)
			(net 12 "/PD6")
			(pinfunction "Pin_1")
			(pintype "passive")
			(uuid "e2417717-af0b-40a1-b745-ccfd5ce541ca")
		)
		(model "${KICAD8_3DMODEL_DIR}/Connector_PinSocket_2.54mm.3dshapes/PinSocket_1x06_P2.54mm_Vertical.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Stripe-ch32:stripe"
		(layer "F.Cu")
		(uuid "b6e92ffb-e53f-44dd-9a1a-11c6b6dafb5e")
		(at 1.017034 27.36044 90)
		(descr "Through hole straight socket strip, 1x06, 2.54mm pitch, single row (from Kicad 4.0.7), script generated")
		(tags "Through hole socket strip THT 1x06 2.54mm single row")
		(property "Reference" "J12"
			(at -9.12 0 0)
			(layer "F.SilkS")
			(uuid "46f2643a-bf88-4fe6-8ad3-9f243fa71703")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "Conn_01x01_Pin"
			(at 0 2.794 90)
			(layer "F.Fab")
			(uuid "609098f6-7bdc-4f77-b9c6-72b36afbe840")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Footprint" "Stripe-ch32:stripe"
			(at -6.35 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "61458af8-3422-42f9-b8e3-768f98e0da92")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" ""
			(at -6.35 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "d3292534-6bc1-444e-bd6d-b93dc11c9bee")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "Generic connector, single row, 01x01, script generated"
			(at -6.35 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "28e6b9df-b404-44eb-8687-142cef4e199a")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "Connector*:*_1x??_*")
		(path "/f50ec0dc-901c-4d3a-859d-22c97acb3b96")
		(sheetname "Root")
		(sheetfile "stripe_board.kicad_sch")
		(attr through_hole)
		(net_tie_pad_groups "stripe-net")
		(fp_line
			(start -5.85 0)
			(end 5.85 0)
			(stroke
				(width 0.5)
				(type default)
			)
			(layer "F.Cu")
			(uuid "227c75ab-741f-4655-b6bf-e16d939886ba")
		)
		(fp_line
			(start -7.62 -1.33)
			(end 7.68 -1.33)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "a6dc3baf-eaaf-4d04-9f20-a4722543ccfe")
		)
		(fp_line
			(start 7.68 1.33)
			(end 7.68 -1.33)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "6444a8d5-f57c-4aa7-96b5-2bd17c3416af")
		)
		(fp_line
			(start -7.62 1.33)
			(end -7.62 -1.33)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "f59c1383-cd91-47cf-8774-a3c8676fb193")
		)
		(fp_line
			(start -7.62 1.33)
			(end 7.68 1.33)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "3436744e-f34e-4eee-9bd2-31a199317b6c")
		)
		(fp_line
			(start 8.1 -1.75)
			(end 8.1 1.8)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "7b567269-247e-4ef9-b729-be0908c5a91d")
		)
		(fp_line
			(start -8.15 -1.75)
			(end 8.1 -1.75)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "841fc0f1-3cc5-463c-b3a1-37b61ba539be")
		)
		(fp_line
			(start 8.1 1.8)
			(end -8.15 1.8)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "d6cf0185-9383-41f3-aeb1-d152e6a93b73")
		)
		(fp_line
			(start -8.15 1.8)
			(end -8.15 -1.75)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "f3e4d503-b943-4b62-86c1-5e9c1199635b")
		)
		(fp_line
			(start 7.62 -1.27)
			(end 7.62 1.27)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "f9f7c6e6-1d24-4f11-8c8d-9f3227300ab8")
		)
		(fp_line
			(start -6.985 -1.27)
			(end 7.62 -1.27)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "b82d4085-66c1-4fcd-a9a0-e8bf27b5ad92")
		)
		(fp_line
			(start -7.62 -0.635)
			(end -6.985 -1.27)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "ea1f6df2-826c-48cf-bfaa-224c34502bc5")
		)
		(fp_line
			(start 7.62 1.27)
			(end -7.62 1.27)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "e2bf7020-88d5-47ca-98f7-7a5f663cf1c1")
		)
		(fp_line
			(start -7.62 1.27)
			(end -7.62 -0.635)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "123ebc02-5fec-4173-8c51-fc3101c4c5b9")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
			(uuid "7007bb55-243e-4e99-b788-12e8226c09d9")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(pad "1" thru_hole circle
			(at -6.35 0 180)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers yes)
			(keep_end_layers yes)
			(zone_layer_connections)
			(net 10 "PWM1")
			(pinfunction "Pin_1")
			(pintype "passive")
			(uuid "9bfed125-881e-4106-a915-0b44152cee0e")
		)
		(pad "1" thru_hole oval
			(at -3.81 0 180)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers yes)
			(keep_end_layers yes)
			(zone_layer_connections)
			(net 10 "PWM1")
			(pinfunction "Pin_1")
			(pintype "passive")
			(uuid "9eed2247-660e-4529-a688-7a89f38489d8")
		)
		(pad "1" thru_hole oval
			(at -1.27 0 180)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers yes)
			(keep_end_layers yes)
			(zone_layer_connections)
			(net 10 "PWM1")
			(pinfunction "Pin_1")
			(pintype "passive")
			(uuid "2f28d4e6-6301-4a2a-b136-941d32e33bd9")
		)
		(pad "1" thru_hole oval
			(at 1.27 0 180)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers yes)
			(keep_end_layers yes)
			(zone_layer_connections)
			(net 10 "PWM1")
			(pinfunction "Pin_1")
			(pintype "passive")
			(uuid "a42cf0e4-063f-412f-995f-31359eabcad2")
		)
		(pad "1" thru_hole oval
			(at 3.81 0 180)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers yes)
			(keep_end_layers yes)
			(zone_layer_connections)
			(net 10 "PWM1")
			(pinfunction "Pin_1")
			(pintype "passive")
			(uuid "c45a7854-6b34-458d-9f50-0585d80f314d")
		)
		(pad "1" thru_hole oval
			(at 6.35 0 180)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers yes)
			(keep_end_layers yes)
			(zone_layer_connections)
			(net 10 "PWM1")
			(pinfunction "Pin_1")
			(pintype "passive")
			(uuid "550d8b3d-2fb6-4e58-ad86-2247e53002e5")
		)
		(model "${KICAD8_3DMODEL_DIR}/Connector_PinSocket_2.54mm.3dshapes/PinSocket_1x06_P2.54mm_Vertical.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Stripe-ch32:Servo_pads"
		(layer "F.Cu")
		(uuid "b75f86b6-5f9d-4119-9c83-3ff9969c870d")
		(at 39.829015 42.78033 180)
		(descr "Through hole straight pin header, 1x03, 2.54mm pitch, single row")
		(tags "Through hole pin header THT 1x03 2.54mm single row")
		(property "Reference" "Srv8"
			(at 0 -2.33 0)
			(layer "F.SilkS")
			(hide yes)
			(uuid "eabbdd3b-4fa8-4193-b388-ffc488c79cb2")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "~"
			(at 0 7.41 0)
			(layer "F.Fab")
			(uuid "e3ee62b5-3d66-482e-99ea-c9dfc64b2142")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Footprint" "Stripe-ch32:Servo_pads"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "9c923f09-e351-4061-b5a1-fb982d8dd5f9")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "0d2b106c-f7a8-43bd-bf70-0e717a5b03da")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "2ee99ac0-c109-41d0-9daa-d1d09418729b")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(path "/c25cf8f4-4c97-4978-9245-4fc4f4f4ba9e")
		(sheetname "Root")
		(sheetfile "stripe_board.kicad_sch")
		(attr through_hole)
		(fp_line
			(start 1.33 6.41)
			(end 1.3208 -1.27)
			(stroke
				(width 0.1)
				(type default)
			)
			(layer "F.SilkS")
			(uuid "80675396-d165-4950-92f5-2d6a2c1a62ca")
		)
		(fp_line
			(start -1.3208 -1.27)
			(end 1.3208 -1.27)
			(stroke
				(width 0.1)
				(type default)
			)
			(layer "F.SilkS")
			(uuid "bc34c110-4c5c-4951-a1a2-d7787da3df24")
		)
		(fp_line
			(start -1.33 6.41)
			(end 1.33 6.41)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "e2750e02-32bd-485a-8ab8-53548fc4a67a")
		)
		(fp_line
			(start -1.33 6.41)
			(end -1.3208 -1.27)
			(stroke
				(width 0.1)
				(type default)
			)
			(layer "F.SilkS")
			(uuid "e6e1ff9d-ee33-41e3-bf2e-2e40a4a1e0cc")
		)
		(fp_line
			(start 1.8 6.85)
			(end 1.8 -1.8)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "b18fb2e6-39e8-42dd-9779-fe5daab21d56")
		)
		(fp_line
			(start 1.8 -1.8)
			(end -1.8 -1.8)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "9cbe8b18-33a2-46ad-a30e-6bad835fc565")
		)
		(fp_line
			(start -1.8 6.85)
			(end 1.8 6.85)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "e8748192-16ac-48a7-8696-b16e9600d387")
		)
		(fp_line
			(start -1.8 -1.8)
			(end -1.8 6.85)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "85363415-b328-4c76-8649-2bcc6c1dba5a")
		)
		(fp_line
			(start 1.27 6.35)
			(end -1.27 6.35)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "d6599894-aaa9-4070-990d-39f034176652")
		)
		(fp_line
			(start 1.27 -1.27)
			(end 1.27 6.35)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "f529c21c-0f08-4afd-a1f0-10fe9cc680f0")
		)
		(fp_line
			(start -0.635 -1.27)
			(end 1.27 -1.27)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "2f4100d8-c8f1-4a71-b57f-764a37ee6fa0")
		)
		(fp_line
			(start -1.27 6.35)
			(end -1.27 -0.635)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "3e84ae3f-7813-4821-81cc-3570c019e405")
		)
		(fp_line
			(start -1.27 -0.635)
			(end -0.635 -1.27)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "3d657de2-8d20-4dbb-8abf-af2b5257ea3d")
		)
		(fp_text user "5V"
			(at 1.3716 3.048 180)
			(unlocked yes)
			(layer "F.SilkS")
			(uuid "97b5b444-2e10-41b7-94f8-40c3ef45f014")
			(effects
				(font
					(size 0.7 0.7)
					(thickness 0.1)
				)
				(justify left bottom)
			)
		)
		(fp_text user "GND"
			(at -1.3208 -1.27 180)
			(unlocked yes)
			(layer "F.SilkS")
			(uuid "d64053dd-423e-497d-a287-1a702f4188b6")
			(effects
				(font
					(size 0.7 0.7)
					(thickness 0.1)
				)
				(justify left bottom)
			)
		)
		(fp_text user "${REFERENCE}"
			(at 0 2.54 90)
			(layer "F.Fab")
			(uuid "346542bc-7862-41ee-8b25-5b5ff43c23f9")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(pad "1" thru_hole rect
			(at 0 0 180)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers yes)
			(keep_end_layers yes)
			(zone_layer_connections)
			(net 2 "GND")
			(pinfunction "GND")
			(pintype "passive")
			(uuid "98f4e92d-36b2-4ae8-ba58-b4fd438a3287")
		)
		(pad "2" thru_hole oval
			(at 0 2.54 180)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers yes)
			(keep_end_layers yes)
			(zone_layer_connections)
			(net 1 "5V")
			(pinfunction "5v")
			(pintype "passive")
			(uuid "8b428d56-d141-4219-ab9c-1704bad4cd8f")
		)
		(pad "3" thru_hole oval
			(at 0 5.08 180)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers yes)
			(keep_end_layers yes)
			(zone_layer_connections)
			(net 15 "/PA2")
			(pinfunction "PWM")
			(pintype "passive")
			(uuid "8d4d5d1a-79b2-4f9c-b5fa-553ea61a0f13")
		)
		(model "${KICAD8_3DMODEL_DIR}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x03_P2.54mm_Vertical.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Stripe-ch32:Servo_pads"
		(layer "F.Cu")
		(uuid "c1d45e67-3b0f-45e3-b3e2-98b93c1eb92a")
		(at 16.759015 42.80033 180)
		(descr "Through hole straight pin header, 1x03, 2.54mm pitch, single row")
		(tags "Through hole pin header THT 1x03 2.54mm single row")
		(property "Reference" "Srv4"
			(at 0 -2.33 0)
			(layer "F.SilkS")
			(hide yes)
			(uuid "254b18f4-778d-4764-a0ef-11187142e823")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "~"
			(at 0 7.41 0)
			(layer "F.Fab")
			(uuid "6dba6d1f-5064-4374-bf04-eb550e603b28")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Footprint" "Stripe-ch32:Servo_pads"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "bd5ea053-7bc0-4614-8962-92bda1718722")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "ed65bdec-56e7-4ce8-a654-a3acfa02aa53")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "549629cc-a76b-4903-9556-f18b67b50e59")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(path "/392a8b9d-4245-4da4-9fe0-6a224565e482")
		(sheetname "Root")
		(sheetfile "stripe_board.kicad_sch")
		(attr through_hole)
		(fp_line
			(start 1.33 6.41)
			(end 1.3208 -1.27)
			(stroke
				(width 0.1)
				(type default)
			)
			(layer "F.SilkS")
			(uuid "4c2ecf51-6223-4dd0-835c-ea951b1de655")
		)
		(fp_line
			(start -1.3208 -1.27)
			(end 1.3208 -1.27)
			(stroke
				(width 0.1)
				(type default)
			)
			(layer "F.SilkS")
			(uuid "560350eb-2f8f-4609-b1ff-c4f85f8b4091")
		)
		(fp_line
			(start -1.33 6.41)
			(end 1.33 6.41)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "c692de39-0a83-4217-83b9-c282beab41b0")
		)
		(fp_line
			(start -1.33 6.41)
			(end -1.3208 -1.27)
			(stroke
				(width 0.1)
				(type default)
			)
			(layer "F.SilkS")
			(uuid "735369eb-0221-46e9-804c-5757c8239556")
		)
		(fp_line
			(start 1.8 6.85)
			(end 1.8 -1.8)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "6926df41-1ff0-4772-afd5-5cc3cb1b142a")
		)
		(fp_line
			(start 1.8 -1.8)
			(end -1.8 -1.8)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "5c7ae6d1-17c2-4c9f-982e-26078df859e6")
		)
		(fp_line
			(start -1.8 6.85)
			(end 1.8 6.85)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "b68e0cce-105b-482e-97d7-8721c0e84b98")
		)
		(fp_line
			(start -1.8 -1.8)
			(end -1.8 6.85)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "283a2dcb-f259-4e5b-aab8-327113925ee8")
		)
		(fp_line
			(start 1.27 6.35)
			(end -1.27 6.35)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "bfca6723-ae23-4ae7-b450-f13acb72d630")
		)
		(fp_line
			(start 1.27 -1.27)
			(end 1.27 6.35)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "fd8a491a-3260-40ce-842e-c69ae9d678ba")
		)
		(fp_line
			(start -0.635 -1.27)
			(end 1.27 -1.27)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "7b7c0937-f3b4-4630-9c7a-86f3ec0bd11d")
		)
		(fp_line
			(start -1.27 6.35)
			(end -1.27 -0.635)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "5ce4afb9-613e-4db6-8a9c-847b4319cfe6")
		)
		(fp_line
			(start -1.27 -0.635)
			(end -0.635 -1.27)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "d5423981-1701-4efa-8ecb-d65dc73452bc")
		)
		(fp_text user "GND"
			(at -1.3208 -1.27 180)
			(unlocked yes)
			(layer "F.SilkS")
			(uuid "10381eb4-3625-49b0-b7cf-3dd6478c34fd")
			(effects
				(font
					(size 0.7 0.7)
					(thickness 0.1)
				)
				(justify left bottom)
			)
		)
		(fp_text user "5V"
			(at 1.3716 3.048 180)
			(unlocked yes)
			(layer "F.SilkS")
			(uuid "43cca8e5-b75a-4670-9f4d-a3e9c90c58bd")
			(effects
				(font
					(size 0.7 0.7)
					(thickness 0.1)
				)
				(justify left bottom)
			)
		)
		(fp_text user "${REFERENCE}"
			(at 0 2.54 90)
			(layer "F.Fab")
			(uuid "39ebfedf-783a-44fb-a403-6680cb6f5cfe")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(pad "1" thru_hole rect
			(at 0 0 180)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers yes)
			(keep_end_layers yes)
			(zone_layer_connections)
			(net 2 "GND")
			(pinfunction "GND")
			(pintype "passive")
			(uuid "f31de549-ce71-4b19-82ef-ed9ad3f6632e")
		)
		(pad "2" thru_hole oval
			(at 0 2.54 180)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers yes)
			(keep_end_layers yes)
			(zone_layer_connections)
			(net 1 "5V")
			(pinfunction "5v")
			(pintype "passive")
			(uuid "48f48536-1a0a-40a3-8f9d-dd0dcdc2fb81")
		)
		(pad "3" thru_hole oval
			(at 0 5.08 180)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers yes)
			(keep_end_layers yes)
			(zone_layer_connections)
			(net 16 "/PD4")
			(pinfunction "PWM")
			(pintype "passive")
			(uuid "5845924b-94bd-416b-b22a-5ca7f587e447")
		)
		(model "${KICAD8_3DMODEL_DIR}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x03_P2.54mm_Vertical.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Stripe-ch32:stripe"
		(layer "F.Cu")
		(uuid "c5e96caf-455e-41be-b029-ef7dabf4b271")
		(at 20.61951 27.640605 -90)
		(descr "Through hole straight socket strip, 1x06, 2.54mm pitch, single row (from Kicad 4.0.7), script generated")
		(tags "Through hole socket strip THT 1x06 2.54mm single row")
		(property "Reference" "J18"
			(at -9.12 0 0)
			(layer "F.SilkS")
			(uuid "3d4d6dbd-d617-447b-ab90-a56c9ef251bb")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "Conn_01x01_Pin"
			(at 0 2.794 90)
			(layer "F.Fab")
			(uuid "7b7ff188-2ed9-4b6a-921f-3625812b0062")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Footprint" "Stripe-ch32:stripe"
			(at -6.35 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "def2f6d7-e6f5-4048-b047-f8a91ce06541")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" ""
			(at -6.35 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "bbf6f8e6-b22b-4fe1-9920-a1853b96f652")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "Generic connector, single row, 01x01, script generated"
			(at -6.35 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "6a7d061d-f928-47b6-9dfe-20d4cb1a0884")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "Connector*:*_1x??_*")
		(path "/7f33ddc7-f00a-42be-a554-8c0050f23611")
		(sheetname "Root")
		(sheetfile "stripe_board.kicad_sch")
		(attr through_hole)
		(net_tie_pad_groups "stripe-net")
		(fp_line
			(start -5.85 0)
			(end 5.85 0)
			(stroke
				(width 0.5)
				(type default)
			)
			(layer "F.Cu")
			(uuid "85eb0d78-1b0c-4cbb-9945-8db33a8acdad")
		)
		(fp_line
			(start -7.62 1.33)
			(end 7.68 1.33)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "c05aa12f-392d-4dfe-94ce-ca049f8a1b14")
		)
		(fp_line
			(start -7.62 1.33)
			(end -7.62 -1.33)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "b3270407-770c-4d3d-9ef9-ed8ac9b12bee")
		)
		(fp_line
			(start 7.68 1.33)
			(end 7.68 -1.33)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "7653d6cc-bac8-4fb8-bfad-05cadcad1c19")
		)
		(fp_line
			(start -7.62 -1.33)
			(end 7.68 -1.33)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "51232ff3-e46d-4870-ad5e-7b1e8ae315ca")
		)
		(fp_line
			(start -8.15 1.8)
			(end -8.15 -1.75)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "970995d9-b423-47ed-9f1b-ce4262c4b8d1")
		)
		(fp_line
			(start 8.1 1.8)
			(end -8.15 1.8)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "d1b44f28-fab7-4761-a472-3b77d20c7b38")
		)
		(fp_line
			(start -8.15 -1.75)
			(end 8.1 -1.75)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "151bc82e-f957-4807-95c2-a928ba989c1f")
		)
		(fp_line
			(start 8.1 -1.75)
			(end 8.1 1.8)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "c4f759ee-156d-4bf5-ae4b-dc8d84769efd")
		)
		(fp_line
			(start -7.62 1.27)
			(end -7.62 -0.635)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "d9c28b9b-877d-456c-aec9-e90c11761b30")
		)
		(fp_line
			(start 7.62 1.27)
			(end -7.62 1.27)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "997d7b42-258f-42b1-8d60-af322dc6b365")
		)
		(fp_line
			(start -7.62 -0.635)
			(end -6.985 -1.27)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "42f2e1f1-07f1-48f9-bc3b-d4fb5d5188a7")
		)
		(fp_line
			(start -6.985 -1.27)
			(end 7.62 -1.27)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "81af26a2-098a-447c-88a3-437b338492e7")
		)
		(fp_line
			(start 7.62 -1.27)
			(end 7.62 1.27)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "0c1c2375-e0a8-4fec-afab-24cb802ba828")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
			(uuid "af836215-093b-422c-b71d-fe7f903f5ff7")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(pad "1" thru_hole circle
			(at -6.35 0)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers yes)
			(keep_end_layers yes)
			(zone_layer_connections)
			(net 1 "5V")
			(pinfunction "Pin_1")
			(pintype "passive")
			(uuid "3e93f359-f03b-4e98-b597-3f03bc2db414")
		)
		(pad "1" thru_hole oval
			(at -3.81 0)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers yes)
			(keep_end_layers yes)
			(zone_layer_connections)
			(net 1 "5V")
			(pinfunction "Pin_1")
			(pintype "passive")
			(uuid "8d22d7e6-d289-47a7-8f19-d179387681f5")
		)
		(pad "1" thru_hole oval
			(at -1.27 0)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers yes)
			(keep_end_layers yes)
			(zone_layer_connections)
			(net 1 "5V")
			(pinfunction "Pin_1")
			(pintype "passive")
			(uuid "43ad8572-77b4-40f9-9e5d-facdfcd47bf0")
		)
		(pad "1" thru_hole oval
			(at 1.27 0)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers yes)
			(keep_end_layers yes)
			(zone_layer_connections)
			(net 1 "5V")
			(pinfunction "Pin_1")
			(pintype "passive")
			(uuid "32f9c7ab-f057-4327-987a-803e6eb5f9b0")
		)
		(pad "1" thru_hole oval
			(at 3.81 0)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers yes)
			(keep_end_layers yes)
			(zone_layer_connections)
			(net 1 "5V")
			(pinfunction "Pin_1")
			(pintype "passive")
			(uuid "b163a85d-7577-4b6a-8823-875d2aa2be51")
		)
		(pad "1" thru_hole oval
			(at 6.35 0)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers yes)
			(keep_end_layers yes)
			(zone_layer_connections)
			(net 1 "5V")
			(pinfunction "Pin_1")
			(pintype "passive")
			(uuid "89e21ac7-53c3-4b9b-81ca-0ddc3d973716")
		)
		(model "${KICAD8_3DMODEL_DIR}/Connector_PinSocket_2.54mm.3dshapes/PinSocket_1x06_P2.54mm_Vertical.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Stripe-ch32:Servo_pads"
		(layer "F.Cu")
		(uuid "d585fd8b-6377-4964-b748-926c46fcc486")
		(at 28.399015 42.78033 180)
		(descr "Through hole straight pin header, 1x03, 2.54mm pitch, single row")
		(tags "Through hole pin header THT 1x03 2.54mm single row")
		(property "Reference" "Srv2"
			(at 0 -2.33 0)
			(layer "F.SilkS")
			(hide yes)
			(uuid "333db687-2534-4d6d-a1a4-45e4ec1d43a4")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "~"
			(at 0 7.41 0)
			(layer "F.Fab")
			(uuid "57d35dda-0a39-43e6-8735-d4b102c074a0")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Footprint" "Stripe-ch32:Servo_pads"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "866b366e-04fc-4321-bb8e-ee35b02493c2")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "8a96c90b-5bb8-4528-b5d2-45bde1601f4d")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "8b9ecb60-26bc-44ab-904e-2ce08af71b19")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(path "/887058ad-a76f-4826-b969-a298fbfc2a3a")
		(sheetname "Root")
		(sheetfile "stripe_board.kicad_sch")
		(attr through_hole)
		(fp_line
			(start 1.33 6.41)
			(end 1.3208 -1.27)
			(stroke
				(width 0.1)
				(type default)
			)
			(layer "F.SilkS")
			(uuid "abec4955-865a-4803-9862-67235ad602f6")
		)
		(fp_line
			(start -1.3208 -1.27)
			(end 1.3208 -1.27)
			(stroke
				(width 0.1)
				(type default)
			)
			(layer "F.SilkS")
			(uuid "85327ef3-1aab-49a5-a6c5-cebfdacce579")
		)
		(fp_line
			(start -1.33 6.41)
			(end 1.33 6.41)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "49d70ec2-03c4-41d9-82ba-48f820085386")
		)
		(fp_line
			(start -1.33 6.41)
			(end -1.3208 -1.27)
			(stroke
				(width 0.1)
				(type default)
			)
			(layer "F.SilkS")
			(uuid "1dc0b3df-11c1-4d06-9277-9c9d436e722b")
		)
		(fp_line
			(start 1.8 6.85)
			(end 1.8 -1.8)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "a6d23623-2565-4ce1-994e-ce965dd34b52")
		)
		(fp_line
			(start 1.8 -1.8)
			(end -1.8 -1.8)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "53793a5d-ec35-4cde-9afd-a4fcd4a1900a")
		)
		(fp_line
			(start -1.8 6.85)
			(end 1.8 6.85)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "a844c05d-043d-49e1-aa1c-30e39d956c96")
		)
		(fp_line
			(start -1.8 -1.8)
			(end -1.8 6.85)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "2f0b3fdf-571c-4aa2-a917-6d8bc10a8b3e")
		)
		(fp_line
			(start 1.27 6.35)
			(end -1.27 6.35)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "ae443320-d0a1-4a49-8939-d758ffc9eaa9")
		)
		(fp_line
			(start 1.27 -1.27)
			(end 1.27 6.35)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "c96ccf20-5d41-40ce-8b35-a7705642bffe")
		)
		(fp_line
			(start -0.635 -1.27)
			(end 1.27 -1.27)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "a9d86867-012b-4bfb-889c-e092763a4205")
		)
		(fp_line
			(start -1.27 6.35)
			(end -1.27 -0.635)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "d9ad9a7c-baab-41ce-82e7-b409a79445ff")
		)
		(fp_line
			(start -1.27 -0.635)
			(end -0.635 -1.27)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "c649f5fd-7464-4d97-836a-334866ff1fb4")
		)
		(fp_text user "5V"
			(at 1.3716 3.048 180)
			(unlocked yes)
			(layer "F.SilkS")
			(uuid "add9d2eb-f559-498c-87e6-2cf10048c1c1")
			(effects
				(font
					(size 0.7 0.7)
					(thickness 0.1)
				)
				(justify left bottom)
			)
		)
		(fp_text user "GND"
			(at -1.3208 -1.27 180)
			(unlocked yes)
			(layer "F.SilkS")
			(uuid "afa4e96d-ed65-433f-b453-4df59eacef3b")
			(effects
				(font
					(size 0.7 0.7)
					(thickness 0.1)
				)
				(justify left bottom)
			)
		)
		(fp_text user "${REFERENCE}"
			(at 0 2.54 90)
			(layer "F.Fab")
			(uuid "cdc7006c-706b-4f2d-a8a6-f833f256f5c4")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(pad "1" thru_hole rect
			(at 0 0 180)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers yes)
			(keep_end_layers yes)
			(zone_layer_connections)
			(net 2 "GND")
			(pinfunction "GND")
			(pintype "passive")
			(uuid "a5efbc36-2b7c-4b32-8d0f-dd9a354c0378")
		)
		(pad "2" thru_hole oval
			(at 0 2.54 180)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers yes)
			(keep_end_layers yes)
			(zone_layer_connections)
			(net 1 "5V")
			(pinfunction "5v")
			(pintype "passive")
			(uuid "d071a12d-b8ae-44a3-a2bf-662a47559695")
		)
		(pad "3" thru_hole oval
			(at 0 5.08 180)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers yes)
			(keep_end_layers yes)
			(zone_layer_connections)
			(net 12 "/PD6")
			(pinfunction "PWM")
			(pintype "passive")
			(uuid "b72d8a15-454e-49a4-81a2-4514fbc954f4")
		)
		(model "${KICAD8_3DMODEL_DIR}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x03_P2.54mm_Vertical.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Stripe-ch32:stripe"
		(layer "F.Cu")
		(uuid "d8188901-6fc3-4a22-a6a2-7701a037b45c")
		(at 43.626733 27.541247 90)
		(descr "Through hole straight socket strip, 1x06, 2.54mm pitch, single row (from Kicad 4.0.7), script generated")
		(tags "Through hole socket strip THT 1x06 2.54mm single row")
		(property "Reference" "J19"
			(at -9.12 0 0)
			(layer "F.SilkS")
			(uuid "16e20efd-29d8-4023-a579-259d8ac0d6b7")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "Conn_01x01_Pin"
			(at 0 2.794 90)
			(layer "F.Fab")
			(uuid "a2193089-3740-4e44-a56f-33d437dd6b06")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Footprint" "Stripe-ch32:stripe"
			(at -6.35 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "43c17085-c91f-4da5-9bf1-87558ff65efc")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" ""
			(at -6.35 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "e9afeeb2-1b25-4f5a-9a8a-b5994607428d")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "Generic connector, single row, 01x01, script generated"
			(at -6.35 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "53efb793-3361-47dd-9d88-6c29d3932863")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "Connector*:*_1x??_*")
		(path "/ab27e0c4-688d-40ba-9378-d4675d0030eb")
		(sheetname "Root")
		(sheetfile "stripe_board.kicad_sch")
		(attr through_hole)
		(net_tie_pad_groups "stripe-net")
		(fp_line
			(start -5.85 0)
			(end 5.85 0)
			(stroke
				(width 0.5)
				(type default)
			)
			(layer "F.Cu")
			(uuid "fd0349c1-cf76-4b24-b0b1-44efad4db290")
		)
		(fp_line
			(start -7.62 -1.33)
			(end 7.68 -1.33)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "a37708d6-8742-424e-ac23-5050cb8d2c8f")
		)
		(fp_line
			(start 7.68 1.33)
			(end 7.68 -1.33)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "dd358db7-e009-453e-a836-8f318135fcdd")
		)
		(fp_line
			(start -7.62 1.33)
			(end -7.62 -1.33)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "e229a196-84bc-4ef9-9d88-8283f3d30c62")
		)
		(fp_line
			(start -7.62 1.33)
			(end 7.68 1.33)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "73c19145-cdd6-426d-a2cd-1f07f1bcd5dd")
		)
		(fp_line
			(start 8.1 -1.75)
			(end 8.1 1.8)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "37e53bb2-7ee3-42d5-8b6e-64e5575286a5")
		)
		(fp_line
			(start -8.15 -1.75)
			(end 8.1 -1.75)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "bb3053b9-e068-4c86-b217-ce8ec489550a")
		)
		(fp_line
			(start 8.1 1.8)
			(end -8.15 1.8)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "fe42b5ac-fe9d-4fb2-ab91-76b006619343")
		)
		(fp_line
			(start -8.15 1.8)
			(end -8.15 -1.75)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "22dcf034-4509-449b-847b-5bdd589aba73")
		)
		(fp_line
			(start 7.62 -1.27)
			(end 7.62 1.27)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "26e45d90-21ee-44f2-b3cb-113d63f67cd4")
		)
		(fp_line
			(start -6.985 -1.27)
			(end 7.62 -1.27)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "c2985e59-9129-498d-ae30-ee9d56fc3212")
		)
		(fp_line
			(start -7.62 -0.635)
			(end -6.985 -1.27)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "092674e9-0e94-429c-bb68-05ea9dede85a")
		)
		(fp_line
			(start 7.62 1.27)
			(end -7.62 1.27)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "00327684-6735-4b75-a8e8-2a7417a0901c")
		)
		(fp_line
			(start -7.62 1.27)
			(end -7.62 -0.635)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "be95bf63-a208-426d-a3e8-8e44f758dd34")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
			(uuid "1ba0f125-61f8-4d56-a987-bf972d34ef52")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(pad "1" thru_hole circle
			(at -6.35 0 180)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers yes)
			(keep_end_layers yes)
			(zone_layer_connections)
			(net 2 "GND")
			(pinfunction "Pin_1")
			(pintype "passive")
			(uuid "81ef2472-aa07-4005-b159-9b40cf15067b")
		)
		(pad "1" thru_hole oval
			(at -3.81 0 180)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers yes)
			(keep_end_layers yes)
			(zone_layer_connections)
			(net 2 "GND")
			(pinfunction "Pin_1")
			(pintype "passive")
			(uuid "dd36ab10-db9b-43a8-834d-855d21b98b41")
		)
		(pad "1" thru_hole oval
			(at -1.27 0 180)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers yes)
			(keep_end_layers yes)
			(zone_layer_connections)
			(net 2 "GND")
			(pinfunction "Pin_1")
			(pintype "passive")
			(uuid "feba565d-2f1a-418a-bd98-b4d2d196c7bb")
		)
		(pad "1" thru_hole oval
			(at 1.27 0 180)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers yes)
			(keep_end_layers yes)
			(zone_layer_connections)
			(net 2 "GND")
			(pinfunction "Pin_1")
			(pintype "passive")
			(uuid "4daee4c3-f19d-4690-a93b-88571732465c")
		)
		(pad "1" thru_hole oval
			(at 3.81 0 180)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers yes)
			(keep_end_layers yes)
			(zone_layer_connections)
			(net 2 "GND")
			(pinfunction "Pin_1")
			(pintype "passive")
			(uuid "a81272cd-a5c5-4a1b-8f9f-c196d2ea2c9e")
		)
		(pad "1" thru_hole oval
			(at 6.35 0 180)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers yes)
			(keep_end_layers yes)
			(zone_layer_connections)
			(net 2 "GND")
			(pinfunction "Pin_1")
			(pintype "passive")
			(uuid "ce612e12-fe45-44f8-8c55-06737a50cc19")
		)
		(model "${KICAD8_3DMODEL_DIR}/Connector_PinSocket_2.54mm.3dshapes/PinSocket_1x06_P2.54mm_Vertical.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Stripe-ch32:stripe"
		(layer "F.Cu")
		(uuid "dd0ec517-96a4-45b3-a299-f4407b226f82")
		(at 5.329015 27.56033 90)
		(descr "Through hole straight socket strip, 1x06, 2.54mm pitch, single row (from Kicad 4.0.7), script generated")
		(tags "Through hole socket strip THT 1x06 2.54mm single row")
		(property "Reference" "J11"
			(at -9.12 0 0)
			(layer "F.SilkS")
			(uuid "c03dcf37-5e7c-40ca-a653-cc65558e4cb8")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "Conn_01x01_Pin"
			(at 0 2.794 90)
			(layer "F.Fab")
			(uuid "d5f46f3f-b8f9-41b0-93d7-c6898945f5e7")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Footprint" "Stripe-ch32:stripe"
			(at -6.35 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "7a205465-40e3-4c4b-ace4-ae2d50fe9e5e")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" ""
			(at -6.35 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "90d0906e-c765-403f-b8b5-472f2235ae90")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "Generic connector, single row, 01x01, script generated"
			(at -6.35 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "fda724f1-d701-409d-9647-024dc1190ac9")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "Connector*:*_1x??_*")
		(path "/dc73eb1e-fcd5-405c-8e41-3b0aa11673e9")
		(sheetname "Root")
		(sheetfile "stripe_board.kicad_sch")
		(attr through_hole)
		(net_tie_pad_groups "stripe-net")
		(fp_line
			(start -5.85 0)
			(end 5.85 0)
			(stroke
				(width 0.5)
				(type default)
			)
			(layer "F.Cu")
			(uuid "88b7b9de-4065-4fb0-baad-693c178c29d7")
		)
		(fp_line
			(start -7.62 -1.33)
			(end 7.68 -1.33)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "a1622fd3-ab45-4ec6-a7c9-c98e22060303")
		)
		(fp_line
			(start 7.68 1.33)
			(end 7.68 -1.33)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "71af9805-8795-47ab-b17b-3b2a715cc0e4")
		)
		(fp_line
			(start -7.62 1.33)
			(end -7.62 -1.33)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "2c75b086-d26f-4911-b7b6-2d3fe9cda087")
		)
		(fp_line
			(start -7.62 1.33)
			(end 7.68 1.33)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "6a1cdbf0-4ff2-423a-af94-7bfa94ad9eca")
		)
		(fp_line
			(start 8.1 -1.75)
			(end 8.1 1.8)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "5723dd9a-cd5f-4392-9deb-04c2d853742c")
		)
		(fp_line
			(start -8.15 -1.75)
			(end 8.1 -1.75)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "639003d5-68ed-450f-a553-4e13aecd94f2")
		)
		(fp_line
			(start 8.1 1.8)
			(end -8.15 1.8)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "f5fcd46e-30a7-437f-8499-411c20d375b4")
		)
		(fp_line
			(start -8.15 1.8)
			(end -8.15 -1.75)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "5b15c803-fe0a-4e48-aff9-ba741984852a")
		)
		(fp_line
			(start 7.62 -1.27)
			(end 7.62 1.27)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "b660f724-7a09-41ae-8b3a-a45d5b46cf0a")
		)
		(fp_line
			(start -6.985 -1.27)
			(end 7.62 -1.27)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "5b99d64a-2ad1-4760-9754-cd6894e9a76c")
		)
		(fp_line
			(start -7.62 -0.635)
			(end -6.985 -1.27)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "d0054a14-3428-4b5c-ae9c-609cc26b3660")
		)
		(fp_line
			(start 7.62 1.27)
			(end -7.62 1.27)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "c257e005-0d93-49dc-9fe1-fed3f7f6d39b")
		)
		(fp_line
			(start -7.62 1.27)
			(end -7.62 -0.635)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "63ca9294-ebcb-4c6b-87e2-e3d5b6aaf402")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
			(uuid "f98a9c88-0d1f-4b74-9313-78d8e281caea")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(pad "1" thru_hole circle
			(at -6.35 0 180)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers yes)
			(keep_end_layers yes)
			(zone_layer_connections)
			(net 6 "PWM2")
			(pinfunction "Pin_1")
			(pintype "passive")
			(uuid "7addfa42-e344-4172-84b4-98f49cf5a6e5")
		)
		(pad "1" thru_hole oval
			(at -3.81 0 180)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers yes)
			(keep_end_layers yes)
			(zone_layer_connections)
			(net 6 "PWM2")
			(pinfunction "Pin_1")
			(pintype "passive")
			(uuid "dd8484c6-23ee-4493-882c-056ab5bad07a")
		)
		(pad "1" thru_hole oval
			(at -1.27 0 180)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers yes)
			(keep_end_layers yes)
			(zone_layer_connections)
			(net 6 "PWM2")
			(pinfunction "Pin_1")
			(pintype "passive")
			(uuid "06a6f855-d6e5-4042-9b7b-af8ed638ccff")
		)
		(pad "1" thru_hole oval
			(at 1.27 0 180)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers yes)
			(keep_end_layers yes)
			(zone_layer_connections)
			(net 6 "PWM2")
			(pinfunction "Pin_1")
			(pintype "passive")
			(uuid "cb2b1b4c-de24-4ad9-977a-40940cecb8ba")
		)
		(pad "1" thru_hole oval
			(at 3.81 0 180)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers yes)
			(keep_end_layers yes)
			(zone_layer_connections)
			(net 6 "PWM2")
			(pinfunction "Pin_1")
			(pintype "passive")
			(uuid "fd6c5547-c10c-416a-9348-7e52dbc10977")
		)
		(pad "1" thru_hole oval
			(at 6.35 0 180)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers yes)
			(keep_end_layers yes)
			(zone_layer_connections)
			(net 6 "PWM2")
			(pinfunction "Pin_1")
			(pintype "passive")
			(uuid "f00a331a-c13a-4144-b78c-f815435315d7")
		)
		(model "${KICAD8_3DMODEL_DIR}/Connector_PinSocket_2.54mm.3dshapes/PinSocket_1x06_P2.54mm_Vertical.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Connector_JST:JST_XH_B3B-XH-A_1x03_P2.50mm_Vertical"
		(layer "F.Cu")
		(uuid "e43eba4c-0f3c-4985-ae5f-63f063aaf82e")
		(at 40.649015 11.70033 90)
		(descr "JST XH series connector, B3B-XH-A (http://www.jst-mfg.com/product/pdf/eng/eXH.pdf), generated with kicad-footprint-generator")
		(tags "connector JST XH vertical")
		(property "Reference" "J13"
			(at 2.5 -3.55 90)
			(layer "F.SilkS")
			(uuid "6129ea8d-a769-4a88-ac0a-00f04173dd71")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "RC_IN"
			(at 2.5 4.6 90)
			(layer "F.Fab")
			(uuid "0f835fef-08d0-4d29-85d7-48bb65216892")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Footprint" "Connector_JST:JST_XH_B3B-XH-A_1x03_P2.50mm_Vertical"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "50a526f3-b6e7-47d6-b620-ac9926d56b03")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "c082b6c8-4697-4be6-beb2-f743c668d5f4")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "Generic connector, single row, 01x03, script generated"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "8fd365c8-5cde-439e-8180-fe83180df2eb")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "Connector*:*_1x??_*")
		(path "/3dc8ace7-f636-4a01-94b2-ec950676dc3f")
		(sheetname "Root")
		(sheetfile "stripe_board.kicad_sch")
		(attr through_hole)
		(fp_line
			(start -1.6 -2.75)
			(end -2.85 -2.75)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "a1b13335-44f5-4808-beae-a56d81f316f8")
		)
		(fp_line
			(start -2.85 -2.75)
			(end -2.85 -1.5)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "72252985-b3cc-4665-910f-34005424ba6b")
		)
		(fp_line
			(start 7.56 -2.46)
			(end -2.56 -2.46)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "9b4b4ce8-51d1-40a9-877c-0392b4ae87ee")
		)
		(fp_line
			(start -2.56 -2.46)
			(end -2.56 3.51)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "a54514dc-93f0-4429-82a4-05b01abcea59")
		)
		(fp_line
			(start 7.55 -2.45)
			(end 5.75 -2.45)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "88b15c1a-be3d-408e-9792-3de6b0cbcd81")
		)
		(fp_line
			(start 5.75 -2.45)
			(end 5.75 -1.7)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "a8d11562-7830-4e19-9f62-c53e01183cb3")
		)
		(fp_line
			(start 4.25 -2.45)
			(end 0.75 -2.45)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "f290ef67-a946-4bf9-b3dd-80f3c6f73a33")
		)
		(fp_line
			(start 0.75 -2.45)
			(end 0.75 -1.7)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "d0d699be-b8cd-4d7a-b4d5-59826ef281b2")
		)
		(fp_line
			(start -0.75 -2.45)
			(end -2.55 -2.45)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "0ec2d848-7513-4654-b9fa-05134375dcd8")
		)
		(fp_line
			(start -2.55 -2.45)
			(end -2.55 -1.7)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "9166508d-867e-4695-9422-3685afb7b03c")
		)
		(fp_line
			(start 7.55 -1.7)
			(end 7.55 -2.45)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "88ca99c3-3cf5-4f1e-9bfb-b0e4cf61a300")
		)
		(fp_line
			(start 5.75 -1.7)
			(end 7.55 -1.7)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "9e0db691-b9c6-430a-918d-278c25b9fafd")
		)
		(fp_line
			(start 4.25 -1.7)
			(end 4.25 -2.45)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "ffcf7e4d-82e8-4b49-b970-9dc56b5ff600")
		)
		(fp_line
			(start 0.75 -1.7)
			(end 4.25 -1.7)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "3f40a604-f2a2-4537-9f15-f19466e30b4d")
		)
		(fp_line
			(start -0.75 -1.7)
			(end -0.75 -2.45)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "7bf4226d-53ba-4b06-a691-b1e42dbd104a")
		)
		(fp_line
			(start -2.55 -1.7)
			(end -0.75 -1.7)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "3de61bb8-dc6c-471a-903e-0f6c9773617f")
		)
		(fp_line
			(start 7.55 -0.2)
			(end 6.8 -0.2)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "10c1de8a-438f-4bdd-a325-864f37a52499")
		)
		(fp_line
			(start 6.8 -0.2)
			(end 6.8 2.75)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "c1598798-f714-46bf-990d-0343aebdd85b")
		)
		(fp_line
			(start -1.8 -0.2)
			(end -1.8 2.75)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "eae8728f-43cd-44d7-bf82-3dffb04e3955")
		)
		(fp_line
			(start -2.55 -0.2)
			(end -1.8 -0.2)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "b47766d9-4305-4938-8fac-857e5246cbdb")
		)
		(fp_line
			(start 6.8 2.75)
			(end 2.5 2.75)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "0bb394f4-b079-4dc1-bbab-737cf28b3aed")
		)
		(fp_line
			(start -1.8 2.75)
			(end 2.5 2.75)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "926d8df8-b601-4556-9080-32d1a94989ea")
		)
		(fp_line
			(start 7.56 3.51)
			(end 7.56 -2.46)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "90bb8756-d98c-4a59-8415-971502deae06")
		)
		(fp_line
			(start -2.56 3.51)
			(end 7.56 3.51)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "1e482a16-1100-498c-93d8-7f9fd18571fa")
		)
		(fp_line
			(start 7.95 -2.85)
			(end -2.95 -2.85)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "ab4cee1d-002c-4457-8501-11ccee58bab0")
		)
		(fp_line
			(start -2.95 -2.85)
			(end -2.95 3.9)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "6ed23ac8-fd42-43d3-932e-a743a156aaf7")
		)
		(fp_line
			(start 7.95 3.9)
			(end 7.95 -2.85)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "5b9e3e87-b137-43ca-a466-6570bc26734e")
		)
		(fp_line
			(start -2.95 3.9)
			(end 7.95 3.9)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "4bcbecd5-691b-4e46-b985-512a3843fb00")
		)
		(fp_line
			(start 7.45 -2.35)
			(end -2.45 -2.35)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "e3ce7ab3-81da-44de-a221-2ec4ad93d4dc")
		)
		(fp_line
			(start -0.625 -2.35)
			(end 0 -1.35)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "9410a275-300a-4a80-942e-4b7ca3ec6868")
		)
		(fp_line
			(start -2.45 -2.35)
			(end -2.45 3.4)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "f051594c-692a-4963-ae8e-b46961d756d4")
		)
		(fp_line
			(start 0 -1.35)
			(end 0.625 -2.35)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "f290f5e6-1990-4119-85c7-1b89b5793b04")
		)
		(fp_line
			(start 7.45 3.4)
			(end 7.45 -2.35)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "ef542115-c177-41ee-b870-e62ba3290e28")
		)
		(fp_line
			(start -2.45 3.4)
			(end 7.45 3.4)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "01819326-edee-4aee-b715-67229c75fab5")
		)
		(fp_text user "${REFERENCE}"
			(at 2.5 2.7 90)
			(layer "F.Fab")
			(uuid "4f48fd5f-7052-4b73-a42f-7aa86bebce88")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(pad "1" thru_hole roundrect
			(at 0 0 90)
			(size 1.7 1.95)
			(drill 0.95)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(roundrect_rratio 0.147059)
			(net 2 "GND")
			(pinfunction "Pin_1")
			(pintype "passive")
			(uuid "fa8b0265-c5a4-4aa2-a3d3-9f2e8a7fb7ed")
		)
		(pad "2" thru_hole oval
			(at 2.5 0 90)
			(size 1.7 1.95)
			(drill 0.95)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "5V")
			(pinfunction "Pin_2")
			(pintype "passive")
			(uuid "af59dd10-09e2-44e8-810e-8ddc6bcb13ea")
		)
		(pad "3" thru_hole oval
			(at 5 0 90)
			(size 1.7 1.95)
			(drill 0.95)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 9 "RC_IN")
			(pinfunction "Pin_3")
			(pintype "passive")
			(uuid "8f89ddc6-7efc-44c4-b796-234942f90df8")
		)
		(model "${KICAD8_3DMODEL_DIR}/Connector_JST.3dshapes/JST_XH_B3B-XH-A_1x03_P2.50mm_Vertical.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Stripe-ch32:Servo_pads"
		(layer "F.Cu")
		(uuid "f80ce8aa-93f1-4685-a7fb-5ea1215b06f5")
		(at 12.949015 42.80033 180)
		(descr "Through hole straight pin header, 1x03, 2.54mm pitch, single row")
		(tags "Through hole pin header THT 1x03 2.54mm single row")
		(property "Reference" "Srv5"
			(at 0 -2.33 0)
			(layer "F.SilkS")
			(hide yes)
			(uuid "a5ab477e-caae-48ca-8965-49cd288bd0c6")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "~"
			(at 0 7.41 0)
			(layer "F.Fab")
			(uuid "fc3df8f4-a896-4446-922e-97957d0c4f19")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Footprint" "Stripe-ch32:Servo_pads"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "c5c0cfb3-a573-4475-9002-623cbd5f0e81")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "0158d5ad-8c77-4ba5-893a-b8d7f49c6413")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "28b733c8-66ad-4602-8f2c-52fa4ae6b66d")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(path "/c92a661b-8f67-4823-bc8d-504f7b17a9ff")
		(sheetname "Root")
		(sheetfile "stripe_board.kicad_sch")
		(attr through_hole)
		(fp_line
			(start 1.33 6.41)
			(end 1.3208 -1.27)
			(stroke
				(width 0.1)
				(type default)
			)
			(layer "F.SilkS")
			(uuid "004f8e5a-9591-4326-9b68-da61b2bdceaa")
		)
		(fp_line
			(start -1.3208 -1.27)
			(end 1.3208 -1.27)
			(stroke
				(width 0.1)
				(type default)
			)
			(layer "F.SilkS")
			(uuid "647be3ad-cd0d-403b-8e04-99831cfe4b70")
		)
		(fp_line
			(start -1.33 6.41)
			(end 1.33 6.41)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "8b5c44cf-98ad-4486-a890-402a7641f65b")
		)
		(fp_line
			(start -1.33 6.41)
			(end -1.3208 -1.27)
			(stroke
				(width 0.1)
				(type default)
			)
			(layer "F.SilkS")
			(uuid "47870d52-1e56-41a7-a4fa-b12b9053c6ea")
		)
		(fp_line
			(start 1.8 6.85)
			(end 1.8 -1.8)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "2748ec53-5643-4e4d-8cf0-d6cf95630092")
		)
		(fp_line
			(start 1.8 -1.8)
			(end -1.8 -1.8)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "2f7d47cc-8911-4440-9e1b-a807f3355dba")
		)
		(fp_line
			(start -1.8 6.85)
			(end 1.8 6.85)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "ac1f429a-3911-47dd-ba2f-a5d1727fec1e")
		)
		(fp_line
			(start -1.8 -1.8)
			(end -1.8 6.85)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "7120e254-6df8-4b91-b4e3-9236e22941d0")
		)
		(fp_line
			(start 1.27 6.35)
			(end -1.27 6.35)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "b327a9ec-9335-4671-a53b-70a3daef756e")
		)
		(fp_line
			(start 1.27 -1.27)
			(end 1.27 6.35)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "ae48e791-02f3-4163-a3cd-62827a0e9add")
		)
		(fp_line
			(start -0.635 -1.27)
			(end 1.27 -1.27)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "767adee0-b4d2-43ab-ba4e-27e747fe7f7d")
		)
		(fp_line
			(start -1.27 6.35)
			(end -1.27 -0.635)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "10bbbe3e-31ef-4293-b76e-f1681f7dedf2")
		)
		(fp_line
			(start -1.27 -0.635)
			(end -0.635 -1.27)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "4c403802-fce0-4dbe-aac5-ddd6986a144c")
		)
		(fp_text user "GND"
			(at -1.3208 -1.27 180)
			(unlocked yes)
			(layer "F.SilkS")
			(uuid "3fe1df35-b6e3-4659-bc22-bfb466110006")
			(effects
				(font
					(size 0.7 0.7)
					(thickness 0.1)
				)
				(justify left bottom)
			)
		)
		(fp_text user "5V"
			(at 1.3716 3.048 180)
			(unlocked yes)
			(layer "F.SilkS")
			(uuid "971114ef-af65-4383-92b4-e022cdf1b947")
			(effects
				(font
					(size 0.7 0.7)
					(thickness 0.1)
				)
				(justify left bottom)
			)
		)
		(fp_text user "${REFERENCE}"
			(at 0 2.54 90)
			(layer "F.Fab")
			(uuid "8903d4b4-e3fe-41a5-b26c-81baac0cbe6e")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(pad "1" thru_hole rect
			(at 0 0 180)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers yes)
			(keep_end_layers yes)
			(zone_layer_connections)
			(net 2 "GND")
			(pinfunction "GND")
			(pintype "passive")
			(uuid "1896bd6f-4465-4608-afaa-1d4980cf6c98")
		)
		(pad "2" thru_hole oval
			(at 0 2.54 180)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers yes)
			(keep_end_layers yes)
			(zone_layer_connections)
			(net 1 "5V")
			(pinfunction "5v")
			(pintype "passive")
			(uuid "ab373599-9624-41dd-92ca-eb87a6062bef")
		)
		(pad "3" thru_hole oval
			(at 0 5.08 180)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers yes)
			(keep_end_layers yes)
			(zone_layer_connections)
			(net 7 "/PC7")
			(pinfunction "PWM")
			(pintype "passive")
			(uuid "20322697-16ba-410e-871a-bccbafedb726")
		)
		(model "${KICAD8_3DMODEL_DIR}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x03_P2.54mm_Vertical.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Stripe-ch32:Servo_pads"
		(layer "F.Cu")
		(uuid "f928b439-78a2-4908-9ec3-7bf55d3302d7")
		(at 24.329015 42.78033 180)
		(descr "Through hole straight pin header, 1x03, 2.54mm pitch, single row")
		(tags "Through hole pin header THT 1x03 2.54mm single row")
		(property "Reference" "Srv3"
			(at 0 -2.33 0)
			(layer "F.SilkS")
			(hide yes)
			(uuid "e62b01c3-3586-4408-9176-aa77242a8993")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "~"
			(at 0 7.41 0)
			(layer "F.Fab")
			(uuid "5d31508c-e97a-46d8-b781-01007891df49")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Footprint" "Stripe-ch32:Servo_pads"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "82eb5ef7-facb-4121-b320-72f49d35c6c6")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "15870d7c-049c-4ea6-addc-64a8717d414c")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "ac2415f2-ee66-49d9-a3f9-5d543a2ae603")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(path "/45c1200b-bffe-4a23-bea0-c1ea3896aa4f")
		(sheetname "Root")
		(sheetfile "stripe_board.kicad_sch")
		(attr through_hole)
		(fp_line
			(start 1.33 6.41)
			(end 1.3208 -1.27)
			(stroke
				(width 0.1)
				(type default)
			)
			(layer "F.SilkS")
			(uuid "b8c20109-ee7b-4bf5-a4b5-98868314b921")
		)
		(fp_line
			(start -1.3208 -1.27)
			(end 1.3208 -1.27)
			(stroke
				(width 0.1)
				(type default)
			)
			(layer "F.SilkS")
			(uuid "1b8595af-c26f-440e-87f2-a74d23c0c9ab")
		)
		(fp_line
			(start -1.33 6.41)
			(end 1.33 6.41)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "5d8bcff2-14b4-41d1-89e7-720977fe4859")
		)
		(fp_line
			(start -1.33 6.41)
			(end -1.3208 -1.27)
			(stroke
				(width 0.1)
				(type default)
			)
			(layer "F.SilkS")
			(uuid "d820f368-5622-4722-8cdb-09339ecc2fc0")
		)
		(fp_line
			(start 1.8 6.85)
			(end 1.8 -1.8)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "ec4e545f-621b-4b66-b1da-7d26f9e90c83")
		)
		(fp_line
			(start 1.8 -1.8)
			(end -1.8 -1.8)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "378c3699-4bb6-4cce-ab78-28fca9d9941f")
		)
		(fp_line
			(start -1.8 6.85)
			(end 1.8 6.85)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "c2bd393e-9e89-4db3-914c-c0b46c59b599")
		)
		(fp_line
			(start -1.8 -1.8)
			(end -1.8 6.85)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "e7418e44-fb53-438a-b8c5-09b6f93a77af")
		)
		(fp_line
			(start 1.27 6.35)
			(end -1.27 6.35)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "903054b6-7942-4ea0-bcd6-0bcbdb14766e")
		)
		(fp_line
			(start 1.27 -1.27)
			(end 1.27 6.35)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "63dbf3f1-fa74-42d0-b4da-e0c15ef1bec0")
		)
		(fp_line
			(start -0.635 -1.27)
			(end 1.27 -1.27)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "807488b9-b8f0-430c-9ccf-eb8a169f62ab")
		)
		(fp_line
			(start -1.27 6.35)
			(end -1.27 -0.635)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "caa80d16-5f10-4cef-b8b7-6ab89f5aa366")
		)
		(fp_line
			(start -1.27 -0.635)
			(end -0.635 -1.27)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "cf3317a8-b175-4208-beb3-f3fb74fe593f")
		)
		(fp_text user "5V"
			(at 1.3716 3.048 180)
			(unlocked yes)
			(layer "F.SilkS")
			(uuid "8da2bd85-b931-4203-97d1-acabce890101")
			(effects
				(font
					(size 0.7 0.7)
					(thickness 0.1)
				)
				(justify left bottom)
			)
		)
		(fp_text user "GND"
			(at -1.3208 -1.27 180)
			(unlocked yes)
			(layer "F.SilkS")
			(uuid "b16f5527-06ff-419c-bfc8-2cb3b9f9d53a")
			(effects
				(font
					(size 0.7 0.7)
					(thickness 0.1)
				)
				(justify left bottom)
			)
		)
		(fp_text user "${REFERENCE}"
			(at 0 2.54 90)
			(layer "F.Fab")
			(uuid "65358234-e06a-4dbb-8a47-9afee847a5e6")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(pad "1" thru_hole rect
			(at 0 0 180)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers yes)
			(keep_end_layers yes)
			(zone_layer_connections)
			(net 2 "GND")
			(pinfunction "GND")
			(pintype "passive")
			(uuid "66b1800d-394e-4584-9362-95fbca5bf4a4")
		)
		(pad "2" thru_hole oval
			(at 0 2.54 180)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers yes)
			(keep_end_layers yes)
			(zone_layer_connections)
			(net 1 "5V")
			(pinfunction "5v")
			(pintype "passive")
			(uuid "029b631d-1a0a-454a-a9f2-e21fc4bf30c1")
		)
		(pad "3" thru_hole oval
			(at 0 5.08 180)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers yes)
			(keep_end_layers yes)
			(zone_layer_connections)
			(net 14 "/PD5")
			(pinfunction "PWM")
			(pintype "passive")
			(uuid "995e2dc6-a84e-41cf-b5f2-062d4b5945d0")
		)
		(model "${KICAD8_3DMODEL_DIR}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x03_P2.54mm_Vertical.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(gr_rect
		(start -5 -5)
		(end 45.399015 45.20033)
		(stroke
			(width 0.05)
			(type default)
		)
		(fill none)
		(layer "Edge.Cuts")
		(uuid "303295d6-c977-49c9-ba67-63731e697983")
	)
	(segment
		(start 28.279015 15.678984)
		(end 28.399015 15.798984)
		(width 0.65)
		(layer "F.Cu")
		(net 1)
		(uuid "041e657a-e643-45d8-a9e5-f629f740cea7")
	)
	(segment
		(start 28.279015 7.90033)
		(end 30.304015 7.90033)
		(width 0.65)
		(layer "F.Cu")
		(net 1)
		(uuid "0f8665a5-1a46-475d-9c5a-0811867425ab")
	)
	(segment
		(start 24.329015 40.24033)
		(end 20.899015 40.24033)
		(width 0.65)
		(layer "F.Cu")
		(net 1)
		(uuid "1d3a402f-9208-4c14-825a-7d88f9569966")
	)
	(segment
		(start 28.399015 15.798984)
		(end 27.097669 17.10033)
		(width 0.65)
		(layer "F.Cu")
		(net 1)
		(uuid "2a86fc34-939e-4293-9b10-b9a18d80fe08")
	)
	(segment
		(start 26.359015 0.39033)
		(end 25.494015 -0.47467)
		(width 0.65)
		(layer "F.Cu")
		(net 1)
		(uuid "2c50cc78-cf5c-45f0-a907-e6acbfc0b138")
	)
	(segment
		(start 5.984015 6.25033)
		(end 4.254015 6.25033)
		(width 0.65)
		(layer "F.Cu")
		(net 1)
		(uuid "2e7b12b8-4c79-4bc5-8654-3f84b3cfa306")
	)
	(segment
		(start 36.019015 40.24033)
		(end 39.829015 40.24033)
		(width 0.65)
		(layer "F.Cu")
		(net 1)
		(uuid "314ad16c-62bf-4198-95d9-28dc2fbb40b7")
	)
	(segment
		(start 29.191001 7.90033)
		(end 28.279015 6.988344)
		(width 0.65)
		(layer "F.Cu")
		(net 1)
		(uuid "3bb38ea5-f2f4-40cd-9e06-dda044bb2d9d")
	)
	(segment
		(start 26.359015 1.20033)
		(end 26.359015 -0.001751)
		(width 0.65)
		(layer "F.Cu")
		(net 1)
		(uuid "3ea93ddf-16f2-43f3-9dd0-f3e75a120d27")
	)
	(segment
		(start 16.779015 40.24033)
		(end 16.759015 40.26033)
		(width 0.65)
		(layer "F.Cu")
		(net 1)
		(uuid "3efe13e0-0cbe-457b-8844-a999eb5047e0")
	)
	(segment
		(start 32.209015 40.24033)
		(end 36.019015 40.24033)
		(width 0.65)
		(layer "F.Cu")
		(net 1)
		(uuid "44ab8787-c54a-428a-87c0-e2daf4f19ee2")
	)
	(segment
		(start 20.399015 40.24033)
		(end 16.779015 40.24033)
		(width 0.65)
		(layer "F.Cu")
		(net 1)
		(uuid "543617b3-c6b0-4b87-a30e-1ae04ef4fbea")
	)
	(segment
		(start 20.899015 34.565605)
		(end 20.61951 34.565605)
		(width 0.65)
		(layer "F.Cu")
		(net 1)
		(uuid "5bd6351d-2edb-4051-9bfb-d11c023e9e64")
	)
	(segment
		(start 12.949015 40.26033)
		(end 9.139015 40.26033)
		(width 0.65)
		(layer "F.Cu")
		(net 1)
		(uuid "66d30e67-8a84-4029-8100-bd5afa234be7")
	)
	(segment
		(start 28.279015 7.90033)
		(end 28.279015 15.678984)
		(width 0.65)
		(layer "F.Cu")
		(net 1)
		(uuid "68ecd35b-f169-4e64-83d6-af7ab20a52c8")
	)
	(segment
		(start 28.399015 40.24033)
		(end 32.209015 40.24033)
		(width 0.65)
		(layer "F.Cu")
		(net 1)
		(uuid "6cd11ca5-8259-48ef-8418-f71adfad61d3")
	)
	(segment
		(start 9.139015 40.26033)
		(end 6.399015 40.26033)
		(width 0.65)
		(layer "F.Cu")
		(net 1)
		(uuid "74478b07-aeea-4720-b771-87a9e66b4606")
	)
	(segment
		(start 3.654015 38.58533)
		(end 5.329015 40.26033)
		(width 0.65)
		(layer "F.Cu")
		(net 1)
		(uuid "7499daef-dd5e-4ffc-9ab6-8af0120b3748")
	)
	(segment
		(start 16.759015 40.26033)
		(end 12.949015 40.26033)
		(width 0.65)
		(layer "F.Cu")
		(net 1)
		(uuid "766414ce-bb9a-47de-a788-7983baff8302")
	)
	(segment
		(start 30.304015 7.90033)
		(end 29.191001 7.90033)
		(width 0.65)
		(layer "F.Cu")
		(net 1)
		(uuid "76971362-a7b4-4bb0-8138-a07d937bbaaa")
	)
	(segment
		(start 27.097669 17.10033)
		(end 22.999015 17.10033)
		(width 0.65)
		(layer "F.Cu")
		(net 1)
		(uuid "82ffb2cd-fe97-4a19-8299-f38134e56d9a")
	)
	(segment
		(start 26.359015 -0.001751)
		(end 25.311096 -1.04967)
		(width 0.65)
		(layer "F.Cu")
		(net 1)
		(uuid "87150b1a-3e84-430a-b816-802673f47a6f")
	)
	(segment
		(start 7.659015 10.46533)
		(end 7.659015 7.92533)
		(width 0.65)
		(layer "F.Cu")
		(net 1)
		(uuid "8926d46a-7c60-4e08-983d-c298633b7372")
	)
	(segment
		(start 7.659015 10.46533)
		(end 3.654015 14.47033)
		(width 0.65)
		(layer "F.Cu")
		(net 1)
		(uuid "8981fba5-aaba-452b-8701-7f6aa1041bb1")
	)
	(segment
		(start 20.61951 19.479835)
		(end 20.61951 20.715605)
		(width 0.65)
		(layer "F.Cu")
		(net 1)
		(uuid "8cfd17dc-3c27-469f-96ff-dbf8e344e0f0")
	)
	(segment
		(start 31.467029 7.95033)
		(end 31.417029 7.90033)
		(width 0.65)
		(layer "F.Cu")
		(net 1)
		(uuid "91d0ee2b-9d4b-4013-bf9b-0af9eba280d8")
	)
	(segment
		(start 20.899015 40.24033)
		(end 20.899015 34.565605)
		(width 0.65)
		(layer "F.Cu")
		(net 1)
		(uuid "a2bd5612-a1f5-48cd-88b4-747b8b668d88")
	)
	(segment
		(start 6.399015 40.26033)
		(end 5.329015 40.26033)
		(width 0.65)
		(layer "F.Cu")
		(net 1)
		(uuid "a3c4c716-a50f-4343-9a08-3cc5379cfa2b")
	)
	(segment
		(start 28.399015 8.692316)
		(end 28.399015 15.798984)
		(width 0.65)
		(layer "F.Cu")
		(net 1)
		(uuid "ae57f149-dfc7-405c-b7d0-edc8d087fea6")
	)
	(segment
		(start 7.659015 7.92533)
		(end 5.984015 6.25033)
		(width 0.65)
		(layer "F.Cu")
		(net 1)
		(uuid "b4e203b9-6a78-4052-8a6e-5bce4f5919f7")
	)
	(segment
		(start 4.254015 6.25033)
		(end 2.579015 7.92533)
		(width 0.65)
		(layer "F.Cu")
		(net 1)
		(uuid "c0becd58-619d-4b65-8f0f-758a4b6946a4")
	)
	(segment
		(start 22.999015 17.10033)
		(end 20.61951 19.479835)
		(width 0.65)
		(layer "F.Cu")
		(net 1)
		(uuid "c5032eda-4f34-4454-8147-1e6a9104df8c")
	)
	(segment
		(start 37.849015 7.90033)
		(end 30.304015 7.90033)
		(width 0.65)
		(layer "F.Cu")
		(net 1)
		(uuid "c5c4250d-0050-4e14-bc2f-e41446a9ba00")
	)
	(segment
		(start 26.359015 1.20033)
		(end 26.359015 0.39033)
		(width 0.65)
		(layer "F.Cu")
		(net 1)
		(uuid "c8b0901f-b53e-4ecb-987c-37d09b4423e9")
	)
	(segment
		(start 20.899015 40.24033)
		(end 20.399015 40.24033)
		(width 0.65)
		(layer "F.Cu")
		(net 1)
		(uuid "d4b9dc20-1dc9-434c-81b5-40aa1c282550")
	)
	(segment
		(start 28.279015 6.988344)
		(end 28.279015 3.12033)
		(width 0.65)
		(layer "F.Cu")
		(net 1)
		(uuid "d958c6bd-9c7a-47ad-b00c-524d9a6dadc3")
	)
	(segment
		(start 25.311096 -1.04967)
		(end 15.899015 -1.04967)
		(width 0.65)
		(layer "F.Cu")
		(net 1)
		(uuid "e0ce43f5-ed05-4ad8-a5be-6ff7346f32dc")
	)
	(segment
		(start 28.279015 3.12033)
		(end 26.359015 1.20033)
		(width 0.65)
		(layer "F.Cu")
		(net 1)
		(uuid "e2ba4eda-e7ff-4c1e-92e3-818a2bd213d4")
	)
	(segment
		(start 29.191001 7.90033)
		(end 28.399015 8.692316)
		(width 0.65)
		(layer "F.Cu")
		(net 1)
		(uuid "ec47e8e2-af48-45b4-8973-49717d1fcbe8")
	)
	(segment
		(start 39.149015 9.20033)
		(end 37.849015 7.90033)
		(width 0.65)
		(layer "F.Cu")
		(net 1)
		(uuid "ec73f468-db39-462f-baba-8a1b4e394a5b")
	)
	(segment
		(start 24.329015 40.24033)
		(end 28.399015 40.24033)
		(width 0.65)
		(layer "F.Cu")
		(net 1)
		(uuid "ed8473c7-24bd-4d0e-9c46-84fbfb45456d")
	)
	(segment
		(start 40.649015 9.20033)
		(end 39.149015 9.20033)
		(width 0.65)
		(layer "F.Cu")
		(net 1)
		(uuid "ef9c7b14-69fa-41e9-9f14-88bc39c335e7")
	)
	(segment
		(start 3.654015 14.47033)
		(end 3.654015 38.58533)
		(width 0.65)
		(layer "F.Cu")
		(net 1)
		(uuid "f3a82ede-5889-4068-827e-96ba0196c4fc")
	)
	(segment
		(start 28.279015 6.988344)
		(end 28.279015 7.90033)
		(width 0.65)
		(layer "F.Cu")
		(net 1)
		(uuid "fc1c390f-5fc9-4dba-b642-5a2564e96e3d")
	)
	(segment
		(start 30.304015 7.90033)
		(end 31.417029 7.90033)
		(width 0.65)
		(layer "F.Cu")
		(net 1)
		(uuid "fdb2aa67-cee1-4663-b638-056df70d4426")
	)
	(segment
		(start 26.417029 14.25033)
		(end 27.129015 13.538344)
		(width 0.65)
		(layer "F.Cu")
		(net 3)
		(uuid "2d9c91b8-841c-46a6-818d-a79c218c4b50")
	)
	(segment
		(start 27.129015 4.51033)
		(end 23.819015 1.20033)
		(width 0.65)
		(layer "F.Cu")
		(net 3)
		(uuid "478127b9-8a5c-429c-a982-051051d97a72")
	)
	(segment
		(start 27.129015 13.538344)
		(end 27.129015 4.51033)
		(width 0.65)
		(layer "F.Cu")
		(net 3)
		(uuid "b1f31179-185d-4817-a51c-be5f8243b5a2")
	)
	(segment
		(start 25.304015 14.25033)
		(end 26.417029 14.25033)
		(width 0.65)
		(layer "F.Cu")
		(net 3)
		(uuid "fe1b2c35-280a-434c-8b84-6dd768ede66a")
	)
	(segment
		(start 25.304015 7.90033)
		(end 13.524015 7.90033)
		(width 0.65)
		(layer "F.Cu")
		(net 4)
		(uuid "703c4b16-7e02-4d6a-9fcb-97c1c2e5c97b")
	)
	(segment
		(start 13.524015 7.90033)
		(end 10.899015 5.27533)
		(width 0.65)
		(layer "F.Cu")
		(net 4)
		(uuid "78ef2e54-2ebf-474a-8df6-24c3f44299d2")
	)
	(segment
		(start 10.899015 5.27533)
		(end 10.899015 -1.04967)
		(width 0.65)
		(layer "F.Cu")
		(net 4)
		(uuid "fa0fa5b6-3418-4b98-82b6-95489323ceb7")
	)
	(segment
		(start 15.829015 6.63033)
		(end 13.399015 4.20033)
		(width 0.65)
		(layer "F.Cu")
		(net 5)
		(uuid "501b2f94-34a2-49f6-b48d-f9088fbee736")
	)
	(segment
		(start 13.399015 4.20033)
		(end 13.399015 -1.04967)
		(width 0.65)
		(layer "F.Cu")
		(net 5)
		(uuid "6a453286-923c-4edc-8606-effa6d53831d")
	)
	(segment
		(start 15.829015 6.63033)
		(end 25.304015 6.63033)
		(width 0.65)
		(layer "F.Cu")
		(net 5)
		(uuid "b11d5a8a-6b66-4550-852c-96ce925a21f5")
	)
	(segment
		(start 25.304015 10.44033)
		(end 10.224015 10.44033)
		(width 0.65)
		(layer "F.Cu")
		(net 6)
		(uuid "4d226d92-ac70-4d15-b339-59d0e205d028")
	)
	(segment
		(start 5.329015 37.72033)
		(end 5.329015 34.11033)
		(width 0.5)
		(layer "F.Cu")
		(net 6)
		(uuid "506246c1-70a4-4e69-8b4a-99d5c9f12597")
	)
	(segment
		(start 10.224015 10.44033)
		(end 10.199015 10.46533)
		(width 0.65)
		(layer "F.Cu")
		(net 6)
		(uuid "7ebc4135-d66c-4597-9970-d078f1398b37")
	)
	(segment
		(start 10.199015 10.46533)
		(end 10.199015 15.76533)
		(width 0.65)
		(layer "F.Cu")
		(net 6)
		(uuid "c3637807-779b-43fb-bb7c-2c15d3f63f38")
	)
	(segment
		(start 10.199015 15.76533)
		(end 5.329015 20.63533)
		(width 0.65)
		(layer "F.Cu")
		(net 6)
		(uuid "d668c0bd-b932-4730-a54d-e6063b7f2a28")
	)
	(segment
		(start 20.158735 12.98033)
		(end 12.949015 20.19005)
		(width 0.65)
		(layer "F.Cu")
		(net 7)
		(uuid "296cc149-7030-4ff9-8c88-13889d7e0bd4")
	)
	(segment
		(start 25.304015 12.98033)
		(end 20.158735 12.98033)
		(width 0.65)
		(layer "F.Cu")
		(net 7)
		(uuid "6161b5bd-d27f-4569-9f23-eb377de8a1a6")
	)
	(segment
		(start 12.949015 20.19005)
		(end 12.949015 20.63533)
		(width 0.65)
		(layer "F.Cu")
		(net 7)
		(uuid "a5efdd36-e7ea-4d06-a7b5-ec1e3ebbc7cb")
	)
	(segment
		(start 12.949015 37.72033)
		(end 12.949015 34.11033)
		(width 0.5)
		(layer "F.Cu")
		(net 7)
		(uuid "ca93fb35-f5e9-4e69-81ee-88d29c916d71")
	)
	(segment
		(start 25.304015 11.71033)
		(end 18.064015 11.71033)
		(width 0.65)
		(layer "F.Cu")
		(net 8)
		(uuid "13d52d75-63b2-4949-9652-13e2c76ef179")
	)
	(segment
		(start 18.064015 11.71033)
		(end 9.139015 20.63533)
		(width 0.65)
		(layer "F.Cu")
		(net 8)
		(uuid "b373506f-8cd5-456b-88b6-9c13cb809301")
	)
	(segment
		(start 9.139015 37.72033)
		(end 9.139015 34.11033)
		(width 0.5)
		(layer "F.Cu")
		(net 8)
		(uuid "d07dcee8-ac60-4fc1-ac03-dd4fae7606ec")
	)
	(segment
		(start 30.374015 6.70033)
		(end 30.304015 6.63033)
		(width 0.65)
		(layer "F.Cu")
		(net 9)
		(uuid "7fd9d0f1-4b5e-42fb-91d6-22a6959d0225")
	)
	(segment
		(start 40.649015 6.70033)
		(end 30.374015 6.70033)
		(width 0.65)
		(layer "F.Cu")
		(net 9)
		(uuid "8508f17e-ebf2-446b-b2d8-ad01e07ddd48")
	)
	(segment
		(start 10.199015 7.92533)
		(end 7.374015 5.10033)
		(width 0.65)
		(layer "F.Cu")
		(net 10)
		(uuid "048ae486-337c-4beb-bc7d-a767bed3fc7b")
	)
	(segment
		(start 0.904015 17.20033)
		(end 0.904015 20.02033)
		(width 0.65)
		(layer "F.Cu")
		(net 10)
		(uuid "3f95e34f-4abc-4565-aea5-ca5bbffc54ee")
	)
	(segment
		(start 0.904015 20.46561)
		(end 1.073735 20.63533)
		(width 0.65)
		(layer "F.Cu")
		(net 10)
		(uuid "4c17021e-a4dc-4456-9e8c-1460cbacda74")
	)
	(segment
		(start 7.374015 5.10033)
		(end 2.999015 5.10033)
		(width 0.65)
		(layer "F.Cu")
		(net 10)
		(uuid "56789796-17f1-4fbd-995b-ff959956113e")
	)
	(segment
		(start 1.017034 37.52044)
		(end 1.017034 33.91044)
		(width 0.5)
		(layer "F.Cu")
		(net 10)
		(uuid "7e22c080-8222-4931-87a3-bca3d971c1ab")
	)
	(segment
		(start 0.904015 17.20033)
		(end 0.904015 20.46561)
		(width 0.65)
		(layer "F.Cu")
		(net 10)
		(uuid "96668812-2e84-4ab0-b89c-797f21eab5ec")
	)
	(segment
		(start 2.999015 5.10033)
		(end 0.904015 7.19533)
		(width 0.65)
		(layer "F.Cu")
		(net 10)
		(uuid "b27aee2d-dc5f-405b-b35a-0a4bda09277e")
	)
	(segment
		(start 1.073735 20.63533)
		(end 1.519015 20.63533)
		(width 0.65)
		(layer "F.Cu")
		(net 10)
		(uuid "cb0fba34-7fbe-4c50-a126-f1d92bd58541")
	)
	(segment
		(start 11.444015 9.17033)
		(end 10.199015 7.92533)
		(width 0.65)
		(layer "F.Cu")
		(net 10)
		(uuid "dc9c3b96-1b68-44c4-ace4-1f2626db3de7")
	)
	(segment
		(start 25.304015 9.17033)
		(end 11.444015 9.17033)
		(width 0.65)
		(layer "F.Cu")
		(net 10)
		(uuid "ddc03c30-817b-494f-a644-cd705e83fc1c")
	)
	(segment
		(start 0.904015 7.19533)
		(end 0.904015 17.20033)
		(width 0.65)
		(layer "F.Cu")
		(net 10)
		(uuid "fa11d006-a4f6-4b10-af73-5a35b2cb5696")
	)
	(segment
		(start 31.773375 12.98033)
		(end 33.399015 14.60597)
		(width 0.65)
		(layer "F.Cu")
		(net 11)
		(uuid "264fed00-4bb1-4540-b5bd-dd3a08b42bcb")
	)
	(segment
		(start 33.399015 19.42533)
		(end 32.209015 20.61533)
		(width 0.65)
		(layer "F.Cu")
		(net 11)
		(uuid "3a513385-338c-4afe-8ae4-39be740e1cf6")
	)
	(segment
		(start 30.304015 12.98033)
		(end 31.773375 12.98033)
		(width 0.65)
		(layer "F.Cu")
		(net 11)
		(uuid "cb07ab4d-60c0-4263-95f3-779ce41bd1c2")
	)
	(segment
		(start 32.209015 37.70033)
		(end 32.209015 34.09033)
		(width 0.5)
		(layer "F.Cu")
		(net 11)
		(uuid "cdf6cf24-f431-42fb-b50f-c972762e6833")
	)
	(segment
		(start 33.399015 14.60597)
		(end 33.399015 19.42533)
		(width 0.65)
		(layer "F.Cu")
		(net 11)
		(uuid "e5dd2a92-3eca-436d-aa29-8fcbf3b31ee3")
	)
	(segment
		(start 32.129015 17.33061)
		(end 28.844295 20.61533)
		(width 0.65)
		(layer "F.Cu")
		(net 12)
		(uuid "0bf773af-c18b-46db-a03f-c442cc56ffa3")
	)
	(segment
		(start 32.129015 14.962316)
		(end 32.129015 17.33061)
		(width 0.65)
		(layer "F.Cu")
		(net 12)
		(uuid "2acfe05e-1a1d-4364-8fc8-04f46e5628f1")
	)
	(segment
		(start 31.417029 14.25033)
		(end 32.129015 14.962316)
		(width 0.65)
		(layer "F.Cu")
		(net 12)
		(uuid "5fd46991-c0d6-4a5a-81b3-1bc5ea6acedd")
	)
	(segment
		(start 28.844295 20.61533)
		(end 28.399015 20.61533)
		(width 0.65)
		(layer "F.Cu")
		(net 12)
		(uuid "ad162cb2-c89e-49b4-9a23-cc89c47bf16f")
	)
	(segment
		(start 30.304015 14.25033)
		(end 31.417029 14.25033)
		(width 0.65)
		(layer "F.Cu")
		(net 12)
		(uuid "ae1d1daa-9bd5-4b5d-ad16-dac9f28494f3")
	)
	(segment
		(start 28.399015 37.70033)
		(end 28.399015 34.09033)
		(width 0.5)
		(layer "F.Cu")
		(net 12)
		(uuid "c341e5b7-0bca-4898-85b0-470ac94e28d9")
	)
	(segment
		(start 36.464295 16.044904)
		(end 36.464295 20.61533)
		(width 0.65)
		(layer "F.Cu")
		(net 13)
		(uuid "09eff772-bc7e-4802-9844-0e4ab31c56a3")
	)
	(segment
		(start 32.129721 11.71033)
		(end 36.464295 16.044904)
		(width 0.65)
		(layer "F.Cu")
		(net 13)
		(uuid "740c5cf2-65b6-4329-b2bd-62121b51d26e")
	)
	(segment
		(start 36.019015 37.70033)
		(end 36.019015 34.09033)
		(width 0.5)
		(layer "F.Cu")
		(net 13)
		(uuid "e1294f58-05e2-41a1-8caa-e81f8905e83d")
	)
	(segment
		(start 30.304015 11.71033)
		(end 32.129721 11.71033)
		(width 0.65)
		(layer "F.Cu")
		(net 13)
		(uuid "e1a0b2d9-f7c6-48dc-bae3-fc10ac3f5623")
	)
	(segment
		(start 36.464295 20.61533)
		(end 36.019015 20.61533)
		(width 0.65)
		(layer "F.Cu")
		(net 13)
		(uuid "fa236e4c-646c-4540-ac94-ea21e02be1b6")
	)
	(segment
		(start 25.209015 20.61533)
		(end 24.329015 20.61533)
		(width 0.65)
		(layer "F.Cu")
		(net 14)
		(uuid "5eaa345c-b681-4aba-8e2b-6c06b0330d56")
	)
	(segment
		(start 24.329015 37.70033)
		(end 24.329015 34.09033)
		(width 0.5)
		(layer "F.Cu")
		(net 14)
		(uuid "8ccd2c9f-e332-4421-9e6a-e0dff0a52daf")
	)
	(segment
		(start 30.304015 15.52033)
		(end 25.209015 20.61533)
		(width 0.65)
		(layer "F.Cu")
		(net 14)
		(uuid "bc3add70-0e71-4323-af49-eaef3cec5944")
	)
	(segment
		(start 32.486067 10.44033)
		(end 39.829015 17.783278)
		(width 0.65)
		(layer "F.Cu")
		(net 15)
		(uuid "12073305-fdbb-4e7c-b7a3-1170b8e590bf")
	)
	(segment
		(start 39.829015 37.70033)
		(end 39.829015 34.09033)
		(width 0.5)
		(layer "F.Cu")
		(net 15)
		(uuid "22aa7705-170a-4844-a0f1-32b1adc0905b")
	)
	(segment
		(start 39.829015 17.783278)
		(end 39.829015 20.61533)
		(width 0.65)
		(layer "F.Cu")
		(net 15)
		(uuid "cd0ba34e-54cc-4707-8927-70c00787ac29")
	)
	(segment
		(start 30.304015 10.44033)
		(end 32.486067 10.44033)
		(width 0.65)
		(layer "F.Cu")
		(net 15)
		(uuid "db86b6ab-dfb4-4051-a5d8-5e1eed751d2b")
	)
	(segment
		(start 16.759015 37.72033)
		(end 16.759015 34.11033)
		(width 0.5)
		(layer "F.Cu")
		(net 16)
		(uuid "58e0df1f-dbb3-4879-90ec-702a2ebc7f3c")
	)
	(segment
		(start 21.874015 15.52033)
		(end 16.759015 20.63533)
		(width 0.65)
		(layer "F.Cu")
		(net 16)
		(uuid "bacb6e5e-cd3a-4148-a402-159743a8ceda")
	)
	(segment
		(start 25.304015 15.52033)
		(end 21.874015 15.52033)
		(width 0.65)
		(layer "F.Cu")
		(net 16)
		(uuid "de8ef48f-36dd-4545-81f4-62a7ac4b5d64")
	)
	(segment
		(start 5.119015 7.92533)
		(end 5.119015 10.46533)
		(width 0.65)
		(layer "F.Cu")
		(net 17)
		(uuid "82930127-0fd4-4350-9a71-65e92cfeff2f")
	)
	(zone
		(net 0)
		(net_name "")
		(layer "F.Cu")
		(uuid "3799d836-cf83-4d04-87a2-2d00fca304c8")
		(hatch edge 0.5)
		(connect_pads
			(clearance 0.5)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 24.629015 4.09033) (xy 25.899015 4.09033) (xy 25.264015 5.36033)
			)
		)
	)
	(zone
		(net 2)
		(net_name "GND")
		(layer "F.Cu")
		(uuid "93e1f69c-06e4-4397-9eee-40a4a6a240eb")
		(name "gnd")
		(hatch edge 0.5)
		(priority 1)
		(connect_pads yes
			(clearance 0.5)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(fill
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 47.2 -8.2) (xy 47.2 48.35033) (xy -7.160985 48.35033) (xy -7.160985 -8.06967)
			)
		)
	)
	(group ""
		(uuid "00073c5e-c811-48b8-97d2-3dcf99eb35de")
		(members "0fa2c90e-46eb-4d6f-8477-4fc2d336d207" "7e22c080-8222-4931-87a3-bca3d971c1ab"
			"b6e92ffb-e53f-44dd-9a1a-11c6b6dafb5e"
		)
	)
	(group ""
		(uuid "1c0ad684-ed1d-4a3c-b73a-fe158cafaddc")
		(members "1fc05b22-4ed7-4937-8fb2-fe229ebba179" "99c7a693-6077-4c19-bf19-6de414b0314c"
			"cdf6cf24-f431-42fb-b50f-c972762e6833"
		)
	)
	(group ""
		(uuid "29c3effd-1c22-4d28-8d7f-0e8d06dff567")
		(members "4adba61e-ecd5-4d7e-a4f7-d711af8a4977" "506246c1-70a4-4e69-8b4a-99d5c9f12597"
			"dd0ec517-96a4-45b3-a299-f4407b226f82"
		)
	)
	(group ""
		(uuid "4ef8e3a5-6692-4e50-8ce6-78fe7f12347a")
		(members "3e38b468-ad46-4ad2-8e7f-58214fde18e7" "7ea60f4a-81b7-47a7-ae9f-e3986336433e"
			"e1294f58-05e2-41a1-8caa-e81f8905e83d"
		)
	)
	(group ""
		(uuid "53f27786-ec9b-4736-8e20-8aa9ad94db60")
		(members "58e0df1f-dbb3-4879-90ec-702a2ebc7f3c" "5968e0d7-93a4-44ae-a1bd-e7bdb1989d25"
			"c1d45e67-3b0f-45e3-b3e2-98b93c1eb92a"
		)
	)
	(group ""
		(uuid "91cfed61-194b-4b58-ad33-c8d7ecf25591")
		(members "22aa7705-170a-4844-a0f1-32b1adc0905b" "7f428ec5-eca3-4328-9b76-e3f3d91675de"
			"b75f86b6-5f9d-4119-9c83-3ff9969c870d"
		)
	)
	(group ""
		(uuid "92b26cc0-71ed-44ab-bd78-b2981578a780")
		(members "8ccd2c9f-e332-4421-9e6a-e0dff0a52daf" "9be699e6-8dfb-4df8-a18d-53ae051316d7"
			"f928b439-78a2-4908-9ec3-7bf55d3302d7"
		)
	)
	(group ""
		(uuid "96ce943f-c754-4273-8e98-a53efc19a4fb")
		(members "975d3b9b-55cf-42b0-a4e2-f8707991610d" "ca93fb35-f5e9-4e69-81ee-88d29c916d71"
			"f80ce8aa-93f1-4685-a7fb-5ea1215b06f5"
		)
	)
	(group ""
		(uuid "a901aba9-93ac-4dd2-b84c-bb263c8c023d")
		(members "8961659e-159b-492f-acaa-9f54416c1dec" "ab28b729-813f-4016-a82a-baf04d5500df"
			"d07dcee8-ac60-4fc1-ac03-dd4fae7606ec"
		)
	)
	(group ""
		(uuid "b37598bb-3bcd-4b2f-a3c1-f58332979fc9")
		(members "b34b9fbf-caf4-4e84-aeea-01e63f6f889b" "c341e5b7-0bca-4898-85b0-470ac94e28d9"
			"d585fd8b-6377-4964-b748-926c46fcc486"
		)
	)
	(group ""
		(uuid "deca0837-bd64-4dde-b398-e8d964bc48a4")
		(members "139e0f84-ec00-46b4-a285-6ec3ca936ac8" "3799d836-cf83-4d04-87a2-2d00fca304c8")
	)
)
