(footprint "Bridged-0.5sqmm_1x03_P4.6mm_D0.9mm_OD2.1mm"
	(version 20240108)
	(generator "pcbnew")
	(generator_version "8.0")
	(layer "F.Cu")
	(descr "Soldered wire connection, for 3 times 0.5 mm² wires, basic insulation, conductor diameter 0.9mm, outer diameter 2.1mm, size source Multi-Contact FLEXI-E 0.5 (https://ec.staubli.com/AcroFiles/Catalogues/TM_Cab-Main-11014119_(en)_hi.pdf), bend radius 3 times outer diameter, generated with kicad-footprint-generator")
	(tags "connector wire 0.5sqmm")
	(property "Reference" "REF**"
		(at -1.905 0 90)
		(layer "F.SilkS")
		(hide yes)
		(uuid "7e0cfbc4-65f4-4eb3-b4c0-c2d0058af638")
		(effects
			(font
				(size 0.8 0.8)
				(thickness 0.15)
			)
		)
	)
	(property "Value" "Bridged-0.5sqmm_1x03_P4.6mm_D0.9mm_OD2.1mm"
		(at 4.6 2.25 0)
		(layer "F.Fab")
		(uuid "29dc9771-8f13-4b81-a702-afbd5fd2072c")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "Footprint" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
		(uuid "5402c37b-5971-4f43-9799-d006fcc1219e")
		(effects
			(font
				(size 1.27 1.27)
				(thickness 0.15)
			)
		)
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
		(uuid "cc2214a8-cc7d-48ca-9e12-8e614787bcab")
		(effects
			(font
				(size 1.27 1.27)
				(thickness 0.15)
			)
		)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
		(uuid "a6beaf35-cdf9-4cdb-b5eb-d29e48062bd2")
		(effects
			(font
				(size 1.27 1.27)
				(thickness 0.15)
			)
		)
	)
	(attr exclude_from_pos_files exclude_from_bom)
	(fp_text user "${REFERENCE}"
		(at 4.6 0 90)
		(layer "F.Fab")
		(uuid "4dc56ff3-d495-4aa5-99d0-9b0e3fb10a95")
		(effects
			(font
				(size 0.52 0.52)
				(thickness 0.08)
			)
		)
	)
	(model "${KICAD8_3DMODEL_DIR}/Connector_Wire.3dshapes/SolderWire-0.5sqmm_1x03_P4.6mm_D0.9mm_OD2.1mm.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
