(footprint "Servo_pads"
	(version 20240108)
	(generator "pcbnew")
	(generator_version "8.0")
	(layer "F.Cu")
	(descr "Through hole straight pin header, 1x03, 2.54mm pitch, single row")
	(tags "Through hole pin header THT 1x03 2.54mm single row")
	(property "Reference" "REF**"
		(at 0 -2.33 0)
		(layer "F.SilkS")
		(hide yes)
		(uuid "4a42150c-e2cb-48c8-8496-6e7fedd454bb")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "Value" "PinHeader_1x03_P2.54mm_Vertical"
		(at 0 7.41 0)
		(layer "F.Fab")
		(uuid "db29ad0b-b335-4faf-88c7-319c7ace35e3")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "Footprint" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
		(uuid "840b1083-fa5a-4072-9eb0-7342e96d093b")
		(effects
			(font
				(size 1.27 1.27)
				(thickness 0.15)
			)
		)
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
		(uuid "60f94ef9-eb50-4806-9b58-af3e1017387f")
		(effects
			(font
				(size 1.27 1.27)
				(thickness 0.15)
			)
		)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
		(uuid "f90835a1-dd76-43e2-9d6a-67a16fd76063")
		(effects
			(font
				(size 1.27 1.27)
				(thickness 0.15)
			)
		)
	)
	(attr through_hole)
	(fp_line
		(start -1.33 6.41)
		(end -1.3208 -1.27)
		(stroke
			(width 0.1)
			(type default)
		)
		(layer "F.SilkS")
		(uuid "6ddd8f5a-008f-4b59-9b9e-ec026d2bd3a5")
	)
	(fp_line
		(start -1.33 6.41)
		(end 1.33 6.41)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "1b8d7228-c97e-4f3b-bb80-5394d1336ea8")
	)
	(fp_line
		(start -1.3208 -1.27)
		(end 1.3208 -1.27)
		(stroke
			(width 0.1)
			(type default)
		)
		(layer "F.SilkS")
		(uuid "0dcd5700-e496-43ed-a0f5-72391eb2c492")
	)
	(fp_line
		(start 1.33 6.41)
		(end 1.3208 -1.27)
		(stroke
			(width 0.1)
			(type default)
		)
		(layer "F.SilkS")
		(uuid "79eb21bf-86a9-4c95-bd6e-a9bc2a5b17cf")
	)
	(fp_line
		(start -1.8 -1.8)
		(end -1.8 6.85)
		(stroke
			(width 0.05)
			(type solid)
		)
		(layer "F.CrtYd")
		(uuid "76c67b9f-3f15-4145-bbbc-8312e5795846")
	)
	(fp_line
		(start -1.8 6.85)
		(end 1.8 6.85)
		(stroke
			(width 0.05)
			(type solid)
		)
		(layer "F.CrtYd")
		(uuid "56a0eaa8-1f42-4824-9fc4-0cbfa375ec08")
	)
	(fp_line
		(start 1.8 -1.8)
		(end -1.8 -1.8)
		(stroke
			(width 0.05)
			(type solid)
		)
		(layer "F.CrtYd")
		(uuid "757b6603-0fa3-41f4-942f-2ab155c45604")
	)
	(fp_line
		(start 1.8 6.85)
		(end 1.8 -1.8)
		(stroke
			(width 0.05)
			(type solid)
		)
		(layer "F.CrtYd")
		(uuid "0624b2c1-b80d-48b5-9bf7-4536c6317e1c")
	)
	(fp_line
		(start -1.27 -0.635)
		(end -0.635 -1.27)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "890db0d5-b901-40c2-b3ae-477fdabfa366")
	)
	(fp_line
		(start -1.27 6.35)
		(end -1.27 -0.635)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "f4fb5e79-dd44-4947-9d51-22633c17ad61")
	)
	(fp_line
		(start -0.635 -1.27)
		(end 1.27 -1.27)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "5eacb716-3494-462e-bcdc-e6b518f66765")
	)
	(fp_line
		(start 1.27 -1.27)
		(end 1.27 6.35)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "8e173d00-babf-4201-8f82-f5030a24fbf9")
	)
	(fp_line
		(start 1.27 6.35)
		(end -1.27 6.35)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "5a8bc881-5fff-4bac-96c1-41af6ae648ff")
	)
	(fp_text user "5V"
		(at 1.3716 3.048 0)
		(unlocked yes)
		(layer "F.SilkS")
		(uuid "205deb0e-736b-489d-90e1-05959f0aa717")
		(effects
			(font
				(size 0.7 0.7)
				(thickness 0.1)
			)
			(justify left bottom)
		)
	)
	(fp_text user "GND"
		(at -1.3208 -1.27 0)
		(unlocked yes)
		(layer "F.SilkS")
		(uuid "e758dd9d-6b3a-4ce8-a7ca-2c7c563bc7b4")
		(effects
			(font
				(size 0.7 0.7)
				(thickness 0.1)
			)
			(justify left bottom)
		)
	)
	(fp_text user "${REFERENCE}"
		(at 0 2.54 90)
		(layer "F.Fab")
		(uuid "788c9283-32be-4c0b-b74e-17c5f67f5b7f")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(pad "1" thru_hole rect
		(at 0 0)
		(size 1.7 1.7)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "c7351bc0-95e7-4de9-93f8-e2fc166956da")
	)
	(pad "2" thru_hole oval
		(at 0 2.54)
		(size 1.7 1.7)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "2e14092c-1e97-4b3c-b1f4-9b887ef28570")
	)
	(pad "3" thru_hole oval
		(at 0 5.08)
		(size 1.7 1.7)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "7072b420-9990-4d8f-a6b8-3c72e84d3433")
	)
	(model "${KICAD8_3DMODEL_DIR}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x03_P2.54mm_Vertical.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
