(footprint "PWR_pads"
	(version 20240108)
	(generator "pcbnew")
	(generator_version "8.0")
	(layer "F.Cu")
	(descr "Soldered wire connection, for 4 times 0.5 mm² wires, reinforced insulation, conductor diameter 0.9mm, outer diameter 2.3mm, size source Multi-Contact FLEXI-xV 0.5 (https://ec.staubli.com/AcroFiles/Catalogues/TM_Cab-Main-11014119_(en)_hi.pdf), bend radius 3 times outer diameter, generated with kicad-footprint-generator")
	(tags "connector wire 0.5sqmm")
	(property "Reference" "REF**"
		(at 7.1628 -5.08 0)
		(layer "F.SilkS")
		(hide yes)
		(uuid "71181a33-7603-424d-be94-90498585d728")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "Value" "SolderWire-0.5sqmm_1x04_P4.8mm_D0.9mm_OD2.3mm"
		(at 7.2 2.35 0)
		(layer "F.Fab")
		(uuid "97b7f273-3f67-434b-901f-59b0e3e329a4")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "Footprint" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
		(uuid "bb5d0ac7-31dd-47e2-96ec-6966e38aa322")
		(effects
			(font
				(size 1.27 1.27)
				(thickness 0.15)
			)
		)
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
		(uuid "81703cc9-3901-4151-94c9-94579c554cd8")
		(effects
			(font
				(size 1.27 1.27)
				(thickness 0.15)
			)
		)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
		(uuid "4a93c3bd-01a7-4354-9a2f-2975337de766")
		(effects
			(font
				(size 1.27 1.27)
				(thickness 0.15)
			)
		)
	)
	(attr exclude_from_pos_files exclude_from_bom)
	(fp_line
		(start -1.9 -1.65)
		(end -1.9 1.65)
		(stroke
			(width 0.05)
			(type solid)
		)
		(layer "F.CrtYd")
		(uuid "d9e9a302-ed7e-4694-bb80-eefe78d87e61")
	)
	(fp_line
		(start -1.9 1.65)
		(end 1.9 1.65)
		(stroke
			(width 0.05)
			(type solid)
		)
		(layer "F.CrtYd")
		(uuid "3914a3de-cffc-4c7d-a4ab-89575c6fc999")
	)
	(fp_line
		(start 1.9 -1.65)
		(end -1.9 -1.65)
		(stroke
			(width 0.05)
			(type solid)
		)
		(layer "F.CrtYd")
		(uuid "7b0d72ac-7c8e-4ea9-badc-63925093d3c4")
	)
	(fp_line
		(start 1.9 1.65)
		(end 1.9 -1.65)
		(stroke
			(width 0.05)
			(type solid)
		)
		(layer "F.CrtYd")
		(uuid "1a8493da-c69f-4d69-afe3-c6a35a7b9926")
	)
	(fp_line
		(start 2.9 -1.65)
		(end 2.9 1.65)
		(stroke
			(width 0.05)
			(type solid)
		)
		(layer "F.CrtYd")
		(uuid "a7bf0d6d-aaf0-463a-ad2b-cc3a1cfd0231")
	)
	(fp_line
		(start 2.9 1.65)
		(end 6.7 1.65)
		(stroke
			(width 0.05)
			(type solid)
		)
		(layer "F.CrtYd")
		(uuid "97de451f-5af1-4423-bed2-636d0a1811a8")
	)
	(fp_line
		(start 6.7 -1.65)
		(end 2.9 -1.65)
		(stroke
			(width 0.05)
			(type solid)
		)
		(layer "F.CrtYd")
		(uuid "aba52c9f-3d84-4ca6-bb2e-de37767ea5a4")
	)
	(fp_line
		(start 6.7 1.65)
		(end 6.7 -1.65)
		(stroke
			(width 0.05)
			(type solid)
		)
		(layer "F.CrtYd")
		(uuid "ef700fd7-5d3b-4cfe-86ee-d06eb7e67d22")
	)
	(fp_line
		(start 7.7 -1.65)
		(end 7.7 1.65)
		(stroke
			(width 0.05)
			(type solid)
		)
		(layer "F.CrtYd")
		(uuid "4c44ea4f-b537-4b1b-bbed-96b71947307a")
	)
	(fp_line
		(start 7.7 1.65)
		(end 11.5 1.65)
		(stroke
			(width 0.05)
			(type solid)
		)
		(layer "F.CrtYd")
		(uuid "8ab9d4d8-e7ce-4fa9-8e7d-e5603c3ee104")
	)
	(fp_line
		(start 11.5 -1.65)
		(end 7.7 -1.65)
		(stroke
			(width 0.05)
			(type solid)
		)
		(layer "F.CrtYd")
		(uuid "a589c73b-5f2c-4300-a438-01245c296d69")
	)
	(fp_line
		(start 11.5 1.65)
		(end 11.5 -1.65)
		(stroke
			(width 0.05)
			(type solid)
		)
		(layer "F.CrtYd")
		(uuid "2d490de9-50ae-4247-9e57-7a3095895130")
	)
	(fp_line
		(start 12.5 -1.65)
		(end 12.5 1.65)
		(stroke
			(width 0.05)
			(type solid)
		)
		(layer "F.CrtYd")
		(uuid "461cd0c8-3c7f-43ce-adf1-93c37679735e")
	)
	(fp_line
		(start 12.5 1.65)
		(end 16.3 1.65)
		(stroke
			(width 0.05)
			(type solid)
		)
		(layer "F.CrtYd")
		(uuid "2102829e-190b-4efb-84df-9945f9e890c1")
	)
	(fp_line
		(start 16.3 -1.65)
		(end 12.5 -1.65)
		(stroke
			(width 0.05)
			(type solid)
		)
		(layer "F.CrtYd")
		(uuid "5ca9ec20-1517-4b87-b955-9208cbd6cfde")
	)
	(fp_line
		(start 16.3 1.65)
		(end 16.3 -1.65)
		(stroke
			(width 0.05)
			(type solid)
		)
		(layer "F.CrtYd")
		(uuid "8a264120-0460-415e-8421-c44f2ebcd131")
	)
	(fp_circle
		(center 0 0)
		(end 1.15 0)
		(stroke
			(width 0.1)
			(type solid)
		)
		(fill none)
		(layer "F.Fab")
		(uuid "d009f5c9-6dcc-4b65-b248-6f9ea76799c0")
	)
	(fp_circle
		(center 4.8 0)
		(end 5.95 0)
		(stroke
			(width 0.1)
			(type solid)
		)
		(fill none)
		(layer "F.Fab")
		(uuid "ba08360b-9314-4745-9ddb-758e6498d99e")
	)
	(fp_circle
		(center 9.6 0)
		(end 10.75 0)
		(stroke
			(width 0.1)
			(type solid)
		)
		(fill none)
		(layer "F.Fab")
		(uuid "c609c737-7dde-416f-b3c3-1febd18af5c6")
	)
	(fp_circle
		(center 14.4 0)
		(end 15.55 0)
		(stroke
			(width 0.1)
			(type solid)
		)
		(fill none)
		(layer "F.Fab")
		(uuid "f4e92e5f-e6ef-4c7e-814f-97cf019c95f3")
	)
	(fp_text user "5V"
		(at 13.462 2.6416 0)
		(unlocked yes)
		(layer "F.SilkS")
		(uuid "457f6fe4-7c76-4763-9861-9d55b9c9932d")
		(effects
			(font
				(size 1 1)
				(thickness 0.1)
			)
			(justify left bottom)
		)
	)
	(fp_text user "GND"
		(at 3.302 2.7432 0)
		(unlocked yes)
		(layer "F.SilkS")
		(uuid "63722f28-f1bc-4ab6-8104-9ac0a2379034")
		(effects
			(font
				(size 1 1)
				(thickness 0.1)
			)
			(justify left bottom)
		)
	)
	(fp_text user "GND"
		(at 8.2296 2.794 0)
		(unlocked yes)
		(layer "F.SilkS")
		(uuid "a44f0ed5-ab04-4978-b0ff-26f077a67db8")
		(effects
			(font
				(size 1 1)
				(thickness 0.1)
			)
			(justify left bottom)
		)
	)
	(fp_text user "12V"
		(at -1.4732 2.7432 0)
		(unlocked yes)
		(layer "F.SilkS")
		(uuid "b7f07db1-d127-43da-b2ad-3b4c2da90cd7")
		(effects
			(font
				(size 1 1)
				(thickness 0.1)
			)
			(justify left bottom)
		)
	)
	(fp_text user "${REFERENCE}"
		(at 7.2 0 90)
		(layer "F.Fab")
		(uuid "523c41bb-4b53-485c-934d-247c1ca071df")
		(effects
			(font
				(size 0.82 0.82)
				(thickness 0.12)
			)
		)
	)
	(pad "1" thru_hole circle
		(at 0 0)
		(size 2.3 2.3)
		(drill 1.1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "7d0aaa4f-a7f1-43ba-b3f6-e9a1a90d3e31")
	)
	(pad "2" thru_hole roundrect
		(at 4.8 0)
		(size 2.3 2.3)
		(drill 1.1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(roundrect_rratio 0.1086956522)
		(uuid "a285960d-c398-4df8-b1a7-8b4e947afc81")
	)
	(pad "3" thru_hole roundrect
		(at 9.6 0)
		(size 2.3 2.3)
		(drill 1.1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(roundrect_rratio 0.1086956522)
		(uuid "4a89183c-fb9b-4b62-a81b-dc353c9cf8c2")
	)
	(pad "4" thru_hole circle
		(at 14.4 0)
		(size 2.3 2.3)
		(drill 1.1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "6bb107a5-cebb-47f2-9245-47d2aecd321f")
	)
	(model "${KICAD8_3DMODEL_DIR}/Connector_Wire.3dshapes/SolderWire-0.5sqmm_1x04_P4.8mm_D0.9mm_OD2.3mm.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
